Automatically Generated Test Frames from a Q Specification of ICAO Flight Plan Form Instructions

Michael R. Donat donat@cs.ubc.ca http://www.cs.ubc.ca/spider/donat http://www.cs.ubc.ca/formalWARE

April 30, 1998

Abstract

A partially automated process for generating tests has been experimentally applied to a portion of a real world system-level requirements specification. This paper discusses the problems addressed by this process along with how and why this automation was achieved. The requirements were formalized using a notation designed to be readable by a large proportion of requirements stakeholders. This report also addresses traceability of requirements to tests and introduces the requirements specification language Q.

Technical Report TR-98-05 Department of Computer Science University of British Columbia Vancouver, B.C.

CANADA

Contents

1 Introduction 4

2 Test Frame Generation: Process Overview 5

3 Test Steps from Test Frames 7

4 Coverage Criteria 8

5 Test Frame Styles 9

6 Traceability 12

7 Processing Times 12

8 Summary 12

A Q Specification of ICAO Flight Plan Instructions 15

B Mathematical Definition of Term Coverage 26

C The Q Requirements Specification Language 27 C.1 Overview . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 27 C.2 Expressions . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 30 C.3 Predicate Definitions . . . . . . . . . . . . . . . . . . . . . . . . . 31 C.4 Conjunctive and Disjunctive Lists . . . . . . . . . . . . . . . . . . 31 C.5 Argument Based Conjunctions and Disjunctions . . . . . . . . . 31 C.6 Expression Aliasing . . . . . . . . . . . . . . . . . . . . . . . . . . 32 C.7 Argument Permutation . . . . . . . . . . . . . . . . . . . . . . . . 32 C.8 Quantification . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 33

D Test Frames for Flight Plan Creation 34 D.1 Introduction . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 34 D.2 Base Test Frames . . . . . . . . . . . . . . . . . . . . . . . . . . . 34

E Test Frames for Flight Plan Validation 60 E.1 Introduction . . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 60 E.2 Base Test Frames . . . . . . . . . . . . . . . . . . . . . . . . . . 61 E.3 Differentiated Test Frames . . . . . . . . . . . . . . . . . . . . . 87 E.3.1 Aircraft Identification . . . . . . . . . . . . . . . . . . . . 88 E.3.2 FlightRules and Type of Flight . . . . . . . . . . . . . . . 96 E.3.3 Number and Type of Aircraft and Wake Turbulence Category . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 107 E.3.4 Equipment . . . . . . . . . . . . . . . . . . . . . . . . . . 122 E.3.5 Departure Aerodrome and Time . . . . . . . . . . . . . . 184 E.3.6 Route . . . . . . . . . . . . . . . . . . . . . . . . . . . . . 199 E.3.7 Destination Aerodrome and Total Estimated Elapsed Time297

E.3.8 Other Information . . . . . . . . . . . . . . . . . . . . . . 304 E.3.9 Supplementary Information . . . . . . . . . . . . . . . . . 324

1 INTRODUCTION 4

1 Introduction

This document reports on the semi-automatic generation of a set of 252 test frames from a portion of the ICAO instructions for filling out a flight plan as specified in Appendix 2, Subsection 2 of ICAO’s Rules of the Air and Air Traffic Services [6]. Appendices D and E contain a list of 252 test frames which were automatically generated by a software tool from a parseable representation of testable requirements. Figure 1 provides a sample of one of these automatically generated test frames. The test frames for Appendices D and E are generated through different uses of the same requirements specification. Each set of test frames provides complete coverage of all the testable requirements relative to the context in which they are used. The 122 test frames contained in Appendix D are schemas for testing a system that automatically fills out a flight plan. The remaining 130 test frames in Appendix E are schemas for testing a system that validates a given flight plan.

ROIDs: I19ES4
Stimuli Response

  1. Dinghies are carried 1. insert {Item 19 D} - {number
                               of dinghies carried}

                             2. insert {Item 19 D} - {total
                               capacity in persons of all
                               dinghies carried}

                             3. insert {Item 19 D} - {colour
                               of dinghies}

Figure 1: A test frame from Appendix D.

Each test frame specifies a specific combination of conditions corresponding to a single step in a test procedure.^1 The contents of the “Stimuli” field of each test frame are used to determine the contents of the “Stimuli” field of a test step. A test engineer would refine a test frame into a test step by entering appropriate data values into the “Stimuli” and “Responses” fields of the test step that satisfy the “Stimuli” of the test frame. In addition to specifying the contents of the “Stimuli” field, each test frame includes traceability information which may be used by the test engineer to specify Requirement Object IDentifiers (ROIDs) in the “Verified Requirements” field of the test step.

The test frames in this report are provided as an example of a semi-automated process employing a formal yet readable-by-non-specialists requirements specification. It is expected that these 252 test frames could be used directly by test engineers in the development of test procedures for software that produces

1A test procedure is a sequence of test steps. Each test step contributes to the demonstration that a specified requirement has indeed been implemented.

a filled out flight plan (Appendix D) and for software validating filled out flight plans (Appendix E). The generation of these 252 test frames was performed by means of an algorithm based on a specific, precisely defined coverage criterion. The ten pages of testable requirements were manually translated into a parseable representation of similar size. This representation was then parsed by the software tool and systematically transformed into test frames. Each step in this derivation is a logical inference. These inferences can be grouped into meta-steps which parallel the steps that would be taken by a test engineer in a manual process.

An overview of the process used to generate the test frames is briefly described in Section 2. Appendix A contains the Q translation of the ICAO flight plan instructions. Appendix C describes the Q specification language. Section 3 of this report outlines a process for the refinement of test frames from Appendix D or E into test steps within a test outline. The coverage criterion determines the number of test frames generated as well as serving as the basis of any claim about the completeness of a test procedure. Section 4 provides a description of the coverage criterion used to generate the 252 test frames in Appendices D and E. Appendix B details the mathemtical definition of the coverage criterion. For each of the test frames, all of the conditions specified in the “Stimuli” field of the test frame are both necessary and sufficient. Section 5 of this report describes an alternate approach which supplements the necessary and sufficient conditions with additional conditions that fully differentiate the test frame from other test frames as a means of helping the test engineer ensure that the expected response has a unique cause. Traceability of requirements to tests is addressed in Section 6. The time required to generate these test frames is described in Section 7. A brief summary of this report is provided in Section 8.

2 Test Frame Generation: Process Overview

This overview provides a brief introduction to the test frame generation process. Details of this process are not essential to the use of the test frames in Appendices D and E. The process used to generate test frames uses a parseable representation of the specification and a test frame generation tool, QTCG. The purpose of this process is to enhance the current manual process through automation while leaving enough flexibility for engineering judgment to be applied. Figure 2 illustrates this process.

Once a set of system-level requirements has been selected, the process of generating test frames involves three steps:

1. Translate the system-level requirements into a parseable representation that can be processed mechanically.

2. Add domain knowledge to document dependencies between conditions.

This information is used to eliminate infeasible tests.

Figure 2: Automatic Generation of Test Frames

3 TEST STEPS FROM TEST FRAMES 7

3. Use the QTCG tool to generate test frames from the parseable representation. The conversion to a parseable representation is a relatively simple translation task.

To produce the formal specification in Appendix A, text was translated directly from the ICAO flight plan instructions into the parseable representation. The parseable representation is written in a formal language. An important characteristic of the parseable representation is that it is also readable by those unfamiliar with the formal language. The Q fragment below is taken directly from the specification in Appendix A.

I19ES4.
if {not {Dinghies are carried}} then {
  cross out {Item 19 D} - {each of {D, C}}}
else {all of {
  insert {Item 19 D} - {number of dinghies carried},

  insert {Item 19 D} -
    {total capacity in persons of all dinghies carried},

  if {not {Dinghies are covered}} then {
    cross out {Item 19 D} - {C}},

  insert {Item 19 D} - {colour of dinghies}
  }}

This fragment explicitly expresses the logical relationships between conditions but does not assign any meaning to these conditions. The logical relationships are required for algorithmic test frame generation. The language of this parseable representation is described in more detail in Appendix C.

The parseable representation makes the logical structure containing testable requirements and the alternatives within the requirements explicit. The QTCG tool exploits this structure in the parseable representation to generate test frames. Furthermore, the parseable representation allows requirements to be tagged with identifiers. The QTCG tool preserves these identifiers while generating test frames. The requirement identifiers associated with a test frame indicate which requirements were relevant to its construction. A traceability mapping from test frames to requirements would normally be constructed manually by test engineers as they construct test frames. The QTCG tool provides this mapping automatically.

3 Test Steps from Test Frames

A softcopy of the test frames can be developed into test steps by following the steps below:

1. Sequence the test frames into outlines of test procedures.

4 COVERAGE CRITERIA 8

2. For each test frame in the outline, select appropriate values that satisfy the stimuli specified by the test frame in a manner compatible with the response in the previous test step.

If it is not possible to select values in step 2, either the outline is infeasible or previously selected values must be adjusted to construct a feasible test procedure.

4 Coverage Criteria

The completeness of a test set is determined by a coverage criterion. The test frames in Appendices D and E were generated using a condition coverage criterion. A simple description of this criterion is that there is at least one test frame for each condition in the Q specification of the requirements. This coverage criterion is based on a mathematical foundation [2]. The precise mathematical definition of this coverage criterion is given in Appendix B. This coverage criterion is intended to be a precise interpretation of the guidance provided in paragraph 6.4.4.1(a)^2 of DO178B [11] that “test cases exist for each software requirement.”

This coverage criterion is illustrated by the following example:

The condition R exists if all of the following conditions are satisfied:

1. condition A is true or condition B is true, and 2. condition C is true or condition D is true.

In this example, the letters A, B, C, D, and R are used to symbolically represent a set of conditions. For instance, the letter A may actually be a phrase such as “the total number of persons is known.” Given that each of the four conditions A, B, C, and D can be true or false, there are sixteen possible logical combinations of these values. But, of course, it is not practical to generate test steps for each of the possible logical combinations since, in general, the number of test cases would grow exponentially with the number of conditions.

The coverage criterion defined mathematically in Appendix B, requires each requirement to be verified once in the sense that every condition must appear in at least one test procedure step. The coverage criterion also requires the conditions to be both necessary and sufficient. For the above example, these constraints can be satisfied by just two test procedures steps. A step in which condition A and condition C are both true together with step in which condition B and condition D are true would satisfy this coverage criterion. An equally valid combination is a step in which condition A and condition D are both true together with a step in which condition B and condition C are true.

26.4.4.1(b) refers to data selection.

5 Test Frame Styles

The QTCG tool is capable of listing conditions for test frames in one of two styles. The “base style” lists only those conditions that are necessary and sufficient to cause the response. However, this list may not be sufficient to differentiate this cause of the response from that of an overlapping test frame. For this purpose test frame conditions can be listed using the “differentiated style.” The style is selected by the test engineer.

The difference between “base style” and “differentiated style” is illustrated in the following example.

Produce response R if any of the following conditions are true:

1. the value of field X is less than 5, 2. the value of field Y is less than 3, or 3. the value of field Z is less than 7.

The test frames for this fragment using a base style are:

–Test Frame 1:

Stimuli Response

1. X < 5 1. R

–Test Frame 2:

Stimuli Response

1. Y < 3 1. R

–Test Frame 3:

Stimuli Response

1. Z < 7 1. R

This style allows for the maximum amount of choice exercised by test engineers in constructing test steps. However, while specifying the test step corresponding to test frame 1, it may be necessary to specify values for Y and Z. The test step corresponding to:

Stimulus Response

1. X = 4

2. Y = 2

3. Z = 8

1. R

does not differentiate between test frames 1 and 2. The differentiated style can assist test engineers by adding constraints to the list of conditions that differentiate the test frames. In this example the set of differentiated test frames is (the extra constraints, or differentiating conditions, are marked with a “•”):

–Test Frame 1:

Stimuli Response

1. Y < 3

2. • ¬ (X < 5)

3. • ¬ (Z < 7)

1. R

–Test Frame 2:

Stimuli Response

1. Z < 7

2. • ¬ (X < 5)

3. • ¬ (Y < 3)

1. R

–Test Frame 3:

Stimuli Response

1. X < 5

2. • ¬ (Y < 3)

3. • ¬ (Z < 7)

1. R

Differentiated frames can be useful in ensuring that test engineers construct test steps that are differentiated. However, in some cases, test frame differentiation takes significant processing time and there may be several alternatives to choose from in order to achieve differentiation. In the QTCG prototype, the choice between alternatives is arbitrary and might not always be appropriate according to best engineering judgment.

As a second example, a base test frame from Section E.2 is:

--Test Frame 1.14:
 ROIDs: I19P
 Stimuli Response
   1. Number of persons is required by the
      ATS authority
   2. The total number of persons is known
   3. NOT (insert {Item 19 P} - {the total
      number of persons [passengers and
      crew] on board} )

                                                1. report error

while its differentiated form (Section E.3) is:

--Test Frame 1.10:
 ROIDs: I19P
 Stimuli Response
   1. Number of persons is required by the ATS
      authority
   2. The total number of persons is known
   3. NOT (insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • Equipment is correct
   8. • Departure Aerodrome and time are correct
   9. • Route is correct
  10. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  11. • Other Information is correct
  12. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and mi nutes}
  13. • cross out {Item 19 R} - {U}
  14. • cross out {Item 19 R} - {V}
  15. • Emergency location beacon is available
  16. • Polar equipment is carried
  17. • Desert equipment is carried
  18. • Maritime equipment is carried
  19. • Jungle equipment is carried
  20. • cross out {Item 19 J} - {V}
  21. • cross out {Item 19 J} - {U}
  22. • cross out {Item 19 J} - {F }
  23. • cross out {Item 19 J} - {L}
  24. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

The advantage of the differentiated test frame is that the additional conditions ensure there is no overlap with another test frame. The disadvantage is that there may be several different ways to differentiate the test frame, but the current prototype test frame generator takes this flexibility away from the engineer by making an arbitrary choice. It is important to note that test frame style is independent of coverage criteria.

6 TRACEABILITY 12

6 Traceability

Traceability is necessary for providing an audit trail to support process monitoring. The QTCG tool supports traceability by keeping track of requirement identifiers inserted into the Q specification by requirements authors. These requirement identifiers are propagated through the logical inferences during the derivation of test frames. This automates the construction of a traceability mapping between requirements and test frames that is currently done manually by test engineers.

7 Processing Times

Computing the base test frames for Appendix D required a total of one minute and 42 seconds^3 on an Ultra-Sparc 60. The base test frames for Appendix E required a total of two minutes and 39 seconds. Computing the differentiated test frames for Appendix E had to be done in pieces and required fifty minutes and seven seconds. Constructing the set of scripts for generating test frames took approximately half an hour.

From the author’s exposure to industry practice, a conservative estimate of the time required to construct, review, and produce a traceability map for a single test frame, on average, is one hour.^4 By this estimate, the base test frames in Appendix E that were automatically generated in under three minutes would require approximately three person-weeks to prepare manually. This comparison does not include the translation time due to the expectation that requirements authors would produce original specifications in Q.

8 Summary

This document has reported the production of 252 test frames using a semiautomated process. Test frames can be used during test development to construct test steps. The automatic production of test frames from a parseable interpretation of system-level requirements has the potential to reduce the labour required to produce test steps for logically complex conditions. In addition, the test frames are produced according to a precise definition of coverage which ensures that the coverage provided by the test frames is consistent and homogenous. Conditions for test frames can be listed in one of two styles: 1) necessary and sufficient, or 2) necessary and sufficient along with additional conditions to ensure that no test step can satisfy more than one test frame. Requirement identifier information is automatically propagated to the test frames during their production. This report includes a description of the Q requirements specification language. Further details of this research can be found in [5, 3, 4, 13].

3The times given are the elapsed time reported by the unix time utility. 4In some cases the estimate is one day.

Acknowledgments

Phil Gray of MacDonald Dettwiler proposed using the ICAO flight plan instructions as the subject of this case study. Some of the ideas for Q are due to Jeffrey Joyce of Raytheon Systems Canada Ltd., and Kendra Cooper, a fellow UBC Ph.D. student. Comments by Jeffrey Joyce have contributed to the presentation of this report.

This work is supported by formalWARE, a university-industry collaborative research project sponsored jointly by the BC Advanced Systems Institute, Raytheon Systems Canada Ltd., MacDonald Dettwiler, The University of British Columbia and The University of Victoria.

http://www.cs.ubc.ca/formalWARE

References

[1] Kendra Cooper. Flex-fix predicates. conversation, June 1997.

[2] Michael R. Donat. Automating formal specification-based testing. In Michel Bidoit and Max Dauchet, editors, TAPSOFT ’97:Theory and Practice of Software Development, 7th International Joint Conference CAAP/FASE, volume 1214 of Lecture Notes in Computer Science, pages 833–847. Springer-Verlag, April 1997.

[3] Michael R. Donat. Automatically generated test frames from an S specification of separation minima for the North Atlantic region. Technical Report TR-98-04, Department of Computer Science, University of British Columbia, Vancouver, B.C., Canada, April 1998.

[4] Michael R. Donat. A Discipline of Specification-Based Test Generation. PhD thesis, Department of Computer Science, University of British Columbia, Vancouver, B.C., Canada, 1998. In preparation.

[5] Michael R. Donat and Jeffrey J. Joyce. Applying an automated test description tool to testing based on system level requirements. In 8th Annual Symposium of the International Council on Systems Engineering, Vancouver, July 1998. International Council on Systems Engineering. http://www.incose.org.

[6] International Civil Aviation Organization, Montréal, Canada. Rules of the Air and Air Traffic Services (PANS-RAC Doc 4444), November 1994. http://www.icao.int.

[7] C. B. Jones. Systematic Software Development Using VDM (2nd edition).

Prentice Hall, 1990.

[8] Jeffrey J. Joyce. TCEL. Proprietary document, April 1997.

[9] Jeffrey J. Joyce, Nancy Day, and Michael R. Donat. S: A machine readable specification notation based on higher order logic. In Thomas F. Melham and Juanito Camilleri, editors, Higher Order Logic Theorem Proving and Its Applications, 7th International Workshop, volume 859 of Lecture Notes in Computer Science, pages 285–299. Springer-Verlag, 1994.

[10] Lawrence C. Paulson. ML for the Working Programmer. Cambridge University Press, second, paperback edition, 1992.

[11] RTCA, Inc. and EUROCAE. DO-178B, Software Considerations in Airbourne Systems and Equipment Certification, 12B edition, December 1992.

[12] J. Michael Spivey. Understanding Z: A Specification language and its formal semantics. Cambridge University Press, 1988.

[13] Kalman Toth, Michael R. Donat, and Jeffrey J. Joyce. Generating test cases from formal specifications. In 6th Annual Symposium of the International Council on Systems Engineering, Boston, July 1996. International Council on Systems Engineering. http://www.incose.org.

A Q Specification of ICAO Flight Plan Instructions

%include startup.s

%include icaofpdefs.s

BEGIN_Q

{Aircraft Identification is correct} is true iff
{all of {

  I7A.
  if {{The radiotelephony call sign to be used by the aircraft will
  consist of {
    any of {
      the registration marking of the aircraft,

      the registration marking of the aircraft preceeded by the ICAO
      telephony designator for the aircraft operating agency}}}
    or {not {The aircraft is equipped with radio}}} then
  {insert {Item 7} - {the registration marking of the aircraft}},

  I7B.
  {id} is {the ICAO telephony designator for the operating agency followed by
  the flight identification} in {
  if {The radiotelephony call sign to be used by the aircraft will consist of
  {id}} then {insert {Item 7} - {id}}}
}}.

{FlightRules and Type of Flight is correct} is true iff
{all of {

  I8FR.
  all of {
  if {IFR rules} then {insert {Item 8 Flight Rules} - {I}},
  if {VFR rules} then {insert {Item 8 Flight Rules} - {V}},
  if {IFR first} then {insert {Item 8 Flight Rules} - {Y}},
  if {VFR first} then {insert {Item 8 Flight Rules} - {Z}}},

  I8FT.
  if {Scheduled Air Service} then {insert {Item 8 Type of Flight} - {S}}
  else {if {Non-scheduled Air Transport Operation} then {insert {Item 8 Type of Flight} - {N}}
  else {if {General Aviation} then {insert {Item 8 Type of Flight} - {G}}
  else {if {Military} then {insert {Item 8 Type of Flight} - {M}}
  else {insert {Item 8 Type of Flight} - {X}}}}}
}}.

{Number and Type of Aircraft and Wake Turbulence Category is correct}
is true iff
{all of{

  I9N.
  if {There is more than one aircraft} then
  {insert {Item 9 Number of Aircraft} - {the number of aircraft}},

  I9T.
  if {{not {There is an appropriate ICAO type designator}}
    or {This is a formation flight with more than one type}}
  then {{insert {Item 9 Type of Aircraft} - {ZZZZ}} and {insert {Item 18} - {TYP/
    Types of aircraft preceded by numbers of aircraft}}}
  else {insert {Item 9 Type of Aircraft} - {the appropriate ICAO type
    designator}},

  I9W.
  all of {
  if {The maximum certified take-off mass is {136000} kg or more} then
  {insert {Item 9 Wake Turnulence} - {/H}},
  if {The maximum certified take-off mass is less than {136000} kg but more
  than {7000} kg} then {insert {Item 9 Wake Turnulence} - {/M}},
  if {The maximum certified take-off mass is {7000} kg or less} then
  {insert {Item 9 Wake Turnulence} - {/L}}
  }
}}.

{Equipment [Part E] is correct} is true iff
{all of{

  I10SE.
  all of {
  if {not {SSR equipment is present}} then {insert {Item 10 SE} - {N}},
  if {SSR transponder mode A} then {insert {Item 10 SE} - {A}},
  if {SSR transponder mode A and mode C} then {insert {Item 10 SE} - {C}},
  if {SSR transponder mode S only} then {insert {Item 10 SE} - {X}},
  if {SSR transponder mode S including pressure-altitude trasmission} then
    {insert {Item 10 SE} - {P}},
  if {SSR transponder mode S including aircraft identification trasmission} then
    {insert {Item 10 SE} - {I}},
  if {SSR transponder mode S including pressure-altitude and aicraft identification trasmission} then
    {insert {Item 10 SE} - {S}},

  if {ADS capability} then {insert {Item 10 SE} - {D}}}
}}.

{Equipment [Part 1] is correct} is true iff
{all of {

    if {COM/NAV/approach aid equipment is {LORAN C}} then
    {insert {Item 10 CNA} - {C}},

    if {COM/NAV/approach aid equipment is {DME}} then
    {insert {Item 10 CNA} - {D}},

    if {COM/NAV/approach aid equipment is {ADF}} then
    {insert {Item 10 CNA} - {F_}},

    if {COM/NAV/approach aid equipment is {GNSS}} then
    {insert {Item 10 CNA} - {G}},

    if {COM/NAV/approach aid equipment is {HF RTF}} then
    {insert {Item 10 CNA} - {H}},

    if {COM/NAV/approach aid equipment is {Inertial Navigation}} then
    {insert {Item 10 CNA} - {I}},

    if {COM/NAV/approach aid equipment is {Data Link}} then
    {{insert {Item 10 CNA} - {J}} and {insert {Item 18} - {DAT/}}},

    if {COM/NAV/approach aid equipment is {MLS}} then
    {insert {Item 10 CNA} - {K}},

    if {COM/NAV/approach aid equipment is {ILS}} then
    {insert {Item 10 CNA} - {L}}
}}.

{Equipment [Part 2] is correct} is true iff
{all of {

    if {COM/NAV/approach aid equipment is {Omega}} then
    {insert {Item 10 CNA} - {M}},

    if {COM/NAV/approach aid equipment is {VOR}} then
    {insert {Item 10 CNA} - {O}},

    if {COM/NAV/approach aid equipment is {RNP type certification}} then
    {insert {Item 10 CNA} - {R}},

    if {COM/NAV/approach aid equipment is {TACAN}} then
    {insert {Item 10 CNA} - {T_}},

    if {COM/NAV/approach aid equipment is {UHF RTF}} then
    {insert {Item 10 CNA} - {U}},

    if {COM/NAV/approach aid equipment is {VHF RTF}} then
    {insert {Item 10 CNA} - {V}},

    if {COM/NAV/approach aid equipment is {other}} then
    {{insert {Item 10 CNA} - {Z}} and {insert {Item 18} - {COM/ or NAV/}}},

    {letter} is {each of {W, X, Y}} in
    {if {{letter} is prescribed by ATS} then {insert {Item 10 CNA} - {letter}}}
}}.

{Equipment is correct} is true iff
{all of {

  I10.
  if {Standard COM/NAV/approach aid equipment for the route to be flown is
  carried and is serviceable} then
  {all of {

    insert {Item 10 CNA} - {S},

    Equipment [Part 1] is correct,

    Equipment [Part 2] is correct}},

  Equipment [Part E] is correct
}}.

{Departure Aerodrome and time are correct} is true iff
{I13.all of{

  if {The flight plan is received from an aircraft in flight} then {
    {insert {Item 13 A} - {AFIL}} and {insert {Item 18} - {DEP/ the four-letter
    location indicator of the location of the ATS unit from which supplementary
    flight data can be obtained}}}
  else {if {not {Location indicator has been assigned}} then
    {{insert {Item 13 A} - {ZZZZZ}} and {insert {Item 13} - {DEP/ aerodrome name}}}
  else
    {insert {Item 13 A} - {the ICAO four-letter location indicator of the
    departure aerodrome}}},

  if {The flight plan was submitted before departure} then
    {insert {Item 13 B} - {the estimated off-block time}}
  else
    {insert {Item 13 B} - {{any of {the actual time, the estimated time}} over
    the first point of the route to which the flight plan applies}}
}}.

{Route is correct} is true iff
{all of {

  I15A.

if {Mach number is prescribed by the appropriate ATS authority} then
  {insert {Item 15 A} - {the true airspeed for the first or the whole cruising
  portion of the flight expressed as {M followed by 3 digits of Mach
  hundredths}}}
else {insert {Item 15 A} - {the true airspeed for the first or the whole
  cruising portion of the flight expressed as {any of {
    K followed by 4 digits of kilometres per hour,
    N followed by 4 digits of knots
  }}}},

I15B.
if {Flight is uncontrolled VFR} then {insert {Item 15 B} - {VFR}}
else {insert {Item 15 B} - {the planned cruising level for the first or the
  whole portion of the route to be flown as {any of {
    F followed by 3 digits of Flight level,
    S followed by 4 digits of Standard Metric Level in tens of metres,
    A followed by 3 digits of Altitude in tens of metres
  }}}},

I15C.
if {The flight is along a designated ATS route} then
  {all of {

  if {The departure aerodrome is {any of {located on, connected to}} the
    ATS route} then
    {insert {Item 15 C} - {the designator of the first ATS route}}
  else {insert {Item 15 C} - {the letters DCT followed by the point of
    joining the first ATS route followed by the designator of the ATS route}},

  for any {point} {
  if {A change of {any of {speed, level, ATS route other than same
      direction lower/upper, flight rules}} is planned at {point}} then
    {if {{The flight to the {next {point}} will be outside a designated route}
      and {not {{each of {point, next {point}}} is
      defined by geological co-ordinates}}} then
      {insert {Item 15 C} - {{point} followed by DCT}}
    else {insert {Item 15 C} - {{point} followed by the designator of the
      next ATS route segment}}}}}}

else {all of {

  if {ATS flight track points are required by the appropriate ATS authority}
  then
    {all of {
    Use ATS style track points,
    for any {point A} {
    for any {point B} {
      if {{point A} and {point B} are successive points} then
        {{point def} is {each of {
          goegraphical co-ordinates,

        bearing and distance}} in
      {if {{each of {point A, point B}} is defined by {point def}} then
        {insert {Item 15 C} - {DCT between {point A} and {point B}}}
      else
        {insert {Item 15 C} - {{point A} followed by {point B}}}}}}}
  }}
else
  {for any {point} {
  {insert {Item 15 C} - {{point} details}} if and only if
    {{not {{point} and {next {point}} are normally more than
    {each of {30 minutes flying time, 370km}} apart}} and
    {A change of {any of {speed, level, track, flight rules}}
    is planned at {point}}}}},

for any {point} {if {{point} is listed in Item 15 C} then
{all of {

I15C1.
the code designator assigned to {any of {route, route segment}} including
  where appropriate the coded designator assigned to the standard
  {any of {departure, arrival}} route is associated with {point},

I15C2.
if {not{A significant point code designator has been assigned to {point}}} then
  {any of {

  2 figures describing latitude in degrees followed
  by {any of {N, S}} followed by 3 figures describing longitude in degrees
  followed by {any of {E, W}} is associated with {point},

  4 figures describing latitude in degrees and
  tens of units of minutes followed by {any of {N, S}} followed by 5
  figures describing longitude in degrees and tens of units of minutes
  followed by {any of {E, W}} is associated with {point},

  the 2 or 3 character identification of the
  navigation aid followed by the 3 figure bearing from the aid in degrees
  magnetic followed by the distance from the aid in 3 figures expressing
  nautical miles is associated with {point}
  }}
else
  {the 2 to 5 characters of the assigned coded
  designator is associated with {point}},

I15C3.
{change} is
{each of {speed - 5pc TAS or more, speed - 0.01 Mach or more, level}} in {
if {A change of {change} is planned at {point}} then {

  an oblique stroke and both the cruising speed

      and the cruising level is associated with {point}}},

    I15C4.
    if {A change of {flight rules} is planned at {point}} then {
      if {IFR to VFR} then
        {the letters VFR are associated with {point}}
      else {if {VFR to IFR} then
        {the letters IFR are associated with {point}}}},

    I15C5.
    if {A change of {level - climb} is planned at {point}} then {
      an oblique stroke followed by the speed to be maintained during
      cruise climb followed by {any of {
        the two levels defining the layer to be occupied during cruide climb,
        the level above which cruise climb is planned followed by PLUS}} is
        associated with {point}}
    }}
    }}}
}}.

END_Q

/* NOTE - Item 15 C, outside ATS routes:

The scope of the instructions 1 - 5 is not clear, i.e., are these
        conventions applied:

1. to each point in Item 15 C,
2. only when outside ATS routes, or
3. only when required by an ATS authority.

(2) is assumed in the above spec.
*/

Subsm ["insert * - * " "Item 10 CNA" V; "insert * - * " "Item 10 CNA" S];
Subsm ["insert * - * " "Item 10 CNA" "F_"; "insert * - * " "Item 10 CNA" S];
Subsm ["insert * - * " "Item 10 CNA" O; "insert * - * " "Item 10 CNA" S];
Subsm ["insert * - * " "Item 10 CNA" L; "insert * - * " "Item 10 CNA" S];

BEGIN_Q

{Destination Aerodrome and Total Estimated Elapsed Time is correct} is true iff
{all of {

  I16-1.
  if {not {Location indicator has been assigned}} then

    {{insert {Item 16 Dest} - {ZZZZ followed by the total estimated elapsed time}}
    and {insert {Item 18} - {DEST/ the name of the aerodrome}}}
  else
    {insert {Item 16 Dest} - {the ICAO four letter location indicator of the
    destination aerodrome followed by the total estimated elapsed time}},

  I16-2.
  if {not {Location indicator has been assigned to the alternate aerodrome}} then
    {{insert {Item 16 Alt} - {ZZZZ}}
    and {insert {Item 18} - {ALTN/ the name of the alternate aerodrome}}}
}}.

{Other Information is correct} is true iff
{all of {

  I18-1.
  for any {point} {
  if {{point} is a {any of {significant point, FIR boundary}} prescribed
    {any of {
      on the basis of regional air navigation agreements,
      by the approapriate ATS authority}}} then {
    insert {Item 18} - {EET/ {point}}}},

  I18-2.
  if {The route is revised} then {
    insert {Item 18} - {RIF/route details to the revised destination
    aerodrome followed by the ICAO four letter location indicator of the
    aerodrome}},

  I18-3.
  if {The registration markings of the aircraft are different from the
    aircraft identification in Item 7} then {
    insert {Item 18} - {REG/registration markings of the aircraft}},

  I18-4.
  if {A SELCAL Code is prescribed by the appropriate ATS authority} then {
    insert {Item 18} - {SEL/SELCAL Code}},

  I18-5.
  if {not {The name of the operator is obvious from the aircraft identification
    in Item 7}} then {
    insert {Item 18} - {OPR/operator name}},

  I18-6.
  if {There is a reason for special handling} then {
    insert {Item 18} - {STS/reason for special handling}},

  I18-7.
  if {Aircraft performance data is prescribed by the appropriate ATS

    authority} then {
    insert {Item 18} - {PER/Aircraft performance data}},

  I18-8.
  for any {aerodrome} {
  if {{aerodrome} is an en-route alternate aerodrome} then {
    insert {Item 18} - {RALT/ {aerodrome}}}},

  I18-9.
  if {Any other plain lanugage remarks are necessary} then {
    insert {Item 18} - {RMK/any other remarks}}
}}.

{Supplementary Information [Part 1] is correct} is true iff
{all of {

  I19E.
  insert {Item 19 E} - {the four digit fuel endurance in hours and minutes},

  I19P.
  if {Number of persons is required by the ATS authority} then {
      if {not {The total number of persons is known}} then {
        insert {Item 19 P} - {TBN}}
      else {
        insert {Item 19 P} - {the total number of persons [passengers and crew]
            on board}}},

  I19ES1.
  all of {
    if {not {UHF on frequency 243.0 MHz is available}} then {
      cross out {Item 19 R} - {U}},

    if {not {VHF on frequency 121.5 MHz is available}} then {
      cross out {Item 19 R} - {V}},

    if {not {Emergency location beacon is available}} then {
      cross out {Item 19 R} - {E}}
    },

  I19ES2.
  all of {
    if {not {Polar equipment is carried}} then {
      cross out {Item 19 S} - {P}},

    if {not {Desert equipment is carried}} then {
      cross out {Item 19 S} - {D}},

    if {not {Maritime equipment is carried}} then {
      cross out {Item 19 S} - {M}},

    if {not {Jungle equipment is carried}} then {
      cross out {Item 19 S} - {J}}
    },

  I19ES3.
  if {not {Life jackets are carried}} then {
    cross out {Item 19 J} - {each of {L, F_, U, V}}}
  else {all of {
    if {not {Life jackets are equipped with lights}} then {
      cross out {Item 19 J} - {L}},

    if {not {Life jackets are equipped with fluorescein}} then {
      cross out {Item 19 J} - {F_}},

    {cross out {Item 19 J} - {U}} exactly when {cross out {Item 19 R} - {U}},

    {cross out {Item 19 J} - {V}} exactly when {cross out {Item 19 R} - {V}}
    }}
}}.

{Supplementary Information [Part 2] is correct} is true iff
{all of {

  I19ES4.
  if {not {Dinghies are carried}} then {
    cross out {Item 19 D} - {each of {D, C}}}
  else {all of {
    insert {Item 19 D} - {number of dinghies carried},

    insert {Item 19 D} - {total capacity in persons of all dinghies carried},

    if {not {Dinghies are covered}} then {
      cross out {Item 19 D} - {C}},

    insert {Item 19 D} - {colour of dinghies}
    }},

  I19ES5.
  insert {Item 19 A} - {colour of aircraft and significant markings},

  I19ES6.
  if {not{There are remarks}} then {
    cross out {Item 19 N} - {N}}
  else {
    indicate {Item 19 N} - {any other survival equipment carried and any other
        remarks regarding survival equipment}},

  I19ES7.
  insert {Item 19 C} - {name of pilot in command}

}}.

{Supplementary Information is correct} is true iff
{all of {
  Supplementary Information [Part 1] is correct,
  Supplementary Information [Part 2] is correct
}}.

{Correct Form} is true iff
{all of {
  Aircraft Identification is correct,
  FlightRules and Type of Flight is correct,
  Number and Type of Aircraft and Wake Turbulence Category is correct,
  Equipment is correct,
  Departure Aerodrome and time are correct,
  Route is correct,
  Destination Aerodrome and Total Estimated Elapsed Time is correct,
  Other Information is correct,
  Supplementary Information is correct
}}.

{Flag Errors} is true iff
{if {not {Correct Form}} then {report error}}.

END_Q

B MATHEMATICAL DEFINITION OF TERM COVERAGE 26

B Mathematical Definition of Term Coverage

The definition of Term Coverage is based on definitions of test classes, test frames, frame stimuli, and test class normal form [2]. The definition of Term Coverage expresses a relationship between frame stimuli within test frames and the frame stimuli of a test class normal form of the specification. The mathematical definition of Term Coverage follows.

The following definitions are assumed:

• Let C_i , 1 6 i 6 n, represent the n test classes of specification Q, i.e., Q = C1 ∧ ... ∧ C_n .

• Let c_i represent the test class antecedent of C_i .

• Let Conj(E ) represent the set of conjuncts in an expression E .

Now, let S (E ) represent the set of frame stimuli in the test class normal form of an expression, E , i.e.,

S = {s | ∃ i.C_i ∈ Conj(TC (E )) ∧ s ∈ FS (c_i )},

where TC is the test class algorithm and FS (c) represents the set of frame stimuli obtained from the test class antecedent, c, as determined by the test frame generation algorithms [2].

Let f_{ik} represent the antecedent of the kth test frame F_{ik} derived from C_i , i.e., ∀ ik.(f_{ik} ⇒ c_i ) ∧ ∀ e.(e ⇒ c_i ) ⇒ Conj(e) ⊄ Conj(f_{ik} ). (1)

Equation (1) states that F_{ik} is a valid test frame of test class C_i and f_{ik} is a prime implicant. The F_{ik} test frames satisfy Term Coverage of a specification, E , when:

∀ s ∈ S (E ). ∃ ik.s ∈ Conj(f_{ik} ). (2)

An alternative variation of Term Coverage is where the coverage of the F_{ik} test frames is measured relative to each individual test class rather than the specification as a whole:

∀ i.C_i ∈ Conj(TC (E )) ⇒ ∀ s ∈ S (C_i ). ∃ k.s ∈ Conj(f_{ik} ). (3)

C The Q Requirements Specification Language

This report introduces a specification making use of certain requirements specification language features. These features are combined to form Q, a requirements specification language. This section describes the motivation for Q and defines the Q specification language.

C.1 Overview

To be practical, the syntax of the specification language should impose as few restrictions on specification authors as possible. It may be necessary to produce test frames for a specification which is an arbitrary relation between any number of stimuli, pre- and post-conditions, and responses. This approach is different from techniques based on specification styles such as Z [12] or VDM [7] which require specifications to be broken down into pieces to be modeled in terms of schemata or operations.

The objective of Q is to provide a means of formalizing requirements phrases while maintaining readability and conciseness as much as possible. The formal aspect of the language is required by the test frame generator. A formal specification that is also readable relieves the need for maintaining two specifications; one formal for input to the test frame generator and another readable by non-specialists. Thus, a key design issue is that Q must be readable by non-specialists.

The specification language provides a concise syntax for denoting the logical relationships and alternatives within the requirements while also providing a natural language style. For example, the requirement fragment,

Either the leading aircraft or the trailing aircraft is supersonic

is specified as

{any of {the leading aircraft, the trailing aircraft}} is supersonic.

The braces impose a parseable structure on the requirements. The semantics of the language constructs, such as ‘‘any of,’’ allows the test frame generator to calculate the logically equivalent expression, which in this case is:

{{the leading aircraft} is supersonic} or {{the trailing aircraft}

is supersonic}.

Q is implemented as an extension of the S specification language [9] and is used to formalize natural language stimulus-response style specifications for the purpose of requirements-based testing. Q can be used to define predicates within a requirements specification but relies on S syntax for defining constants, type, and functions. Q statements are contained within the keywords BEGIN Q and END Q.

The light-weight simplicity of the Q language helps to preserve the readability and conciseness of the specification. The mathematical semantics of Q ensure that each statement has an unambiguous meaning. With these qualities, Q provides the mathematical link between a requirements specification and the test frame generation tool introduced in the previous chapter.

Three features of Q substantially contribute to preserving readability and conciseness. The first is the use of braces, {}, which delimit phrases and parameters within the specification. Injecting these braces into the specification effectively transforms the phrases of natural language into formal functions and arguments. This technique was first used by Joyce in his Test Case Element Language (TCEL) [8].

When formalizing the natural language phrase

the leading aircraft is supersonic or the following aircraft is supersonic

for the purpose of system-level requirements-based testing, only the choices need to be made explicit. Thus, the appropriate formalization for testing is to choose

‘‘or’’ as the predicate and the two adjoining phrases are conditions. The

resulting Q version of the above phrase is:

{the leading aircraft is supersonic} or {the following aircraft

is supersonic}.

In this Q expression, ‘‘ * or * ’’ is the function and ‘‘the leading aircraft

is supersonic’’ and ‘‘the following aircraft is supersonic’’ are its

arguments. The lambda calculus equivalent is

‘‘ * or * ’’ ‘‘the leading aircraft is supersonic’’ ‘‘the following
aircraft is supersonic’’

where ‘‘ * or * ’’ has the type bool → bool → bool, as expected.

The ‘‘ * ’’ in the function name denotes positions in the text where arguments are placed. This type of notation is referred to as a flex-fix notation [1]. Flex-fix, the second Q feature, allows arguments to be distributed within a function name. This helps preserve readability. For example, the Q expression

‘‘{aircraft A} and {aircraft B} are separated by at least {1000
feet}’’

corresponds to the following lambda calculus representation:

‘‘ * and * are separated by at least * ’’ ‘‘aircraft A’’ ‘‘aircraft
B’’ ‘‘1000 feet.’’

The Q expression is more readable than, say, a Z or VDM-SL expression

ABS (Altitude(aircraft A) − Altitude(aircraft B)) ¿ feet(1000).

The third feature of Q, due to the author, is the use of keywords which define multiple arguments for a function’s parameter. These keywords are motivated by natural language phraseology such as “both aircraft are...,” “either A or B is a... .” For example, the requirement either the leading aircraft or the following aircraft is supersonic

can be formalized in Q as

{any of {the leading aircraft, the following aircraft}} is supersonic.

A predicate containing an “any of” argument is equivalent to a disjunction of that predicate evaluated at each of the values in the “any of” set. In this case, the equivalent expression is

{{the leading aircraft} is supersonic} or {{the following aircraft}

is supersonic}.

This example contains more formal detail than the first example in this section. Here, there are formal references to two aircraft. In the first example, there were only two conditions. The fact that these conditions were based on two aircraft was not made explicit in the first example. This latest example is referred to as a deeper specification because it contains more formal detail. Test engineers decide how deep a specification should be by determining the condition dependencies they wish to reveal to the test frame generator.

Another parameter mechanism is the “distinct choices” keyword. This keyword is used in encoding phrases such as:

all of the following are true:

1. aircraft A is dumping fuel, 2. aircraft B is using standard altimeter setting, 3. if one aircraft is supersonic and the other is not then ...

In this example, “one aircraft” and “the other” refer to either “aircraft A” or “aircraft B,” interchangeably. i.e., They represent distinct choices of the two aircraft. The Q version is:

{all of {

1. {aircraft A} is dumping fuel,

2. {aircraft B} is using standard altimeter setting,

3. if {{one aircraft, the other} are any distinct choices of {aircraft
   A, aircraft B} in

{{{one aircraft} is supersonic} and {it is not the case that {{the other} is supersonic}}}} then...

The loss of conciseness in this example is necessary in order to formally define the references “one aircraft” and “the other.” However, this construction is still more concise and more readable than the full expansion of the distinct choice which is:

{{{aircraft A} is supersonic} and

{it is not the case that {{aircraft B} is supersonic}}}

or

{{{aircraft B} is supersonic} and

{it is not the case that {{aircraft A} is supersonic}}}

This point is even more apparent when considering the case where a third aircraft is involved.

{one aircraft, another} are any distinct choices of {aircraft A,

aircraft B, aircraft C} in

{{{one aircraft} is supersonic} and {it is not the case that {{another}

is supersonic}}}

is equivalent to:

{{{aircraft A} is supersonic} and {it is not the case that {{aircraft

B} is supersonic}}} or

{{{{aircraft A} is supersonic} and {it is not the case that {{aircraft

C} is supersonic}}} or

{{{{aircraft B} is supersonic} and {it is not the case that {{aircraft

A} is supersonic}}} or

{{{{aircraft B} is supersonic} and {it is not the case that {{aircraft

C} is supersonic}}} or

{{{{aircraft C} is supersonic} and {it is not the case that {{aircraft

A} is supersonic}}} or

{{{{aircraft C} is supersonic} and {it is not the case that {{aircraft

B} is supersonic}}}}}}}}

This example also demonstrates that the use of the distinct choices keyword helps preserve the understandability of the specification. Comprehending the Q expression above requires more effort than text which makes use of the

‘‘distinct choices’’ keyword.

The formal semantics of ‘‘any of,’’ its counterpart, ‘‘each of,’’ and other parameter mechanisms are more precisely defined in later sections.

C.2 Expressions

A Q expression is a string of at least one word and any number of arguments separated by white-space characters. Arguments are expressions contained within a comma delimited list surrounded by braces. In this thesis Q expressions are usually enclosed in braces to delimit them from the rest of the text. To be concise, an ambiguous grammar is used to express the syntax of Q. In the following grammar, e* represents zero or more e’s concatenated, e.g., any of nil, e, ee, . . ., where nil is the empty string. The expression e+ is equivalent to ee*. Parentheses are used to group expressions together in order to then apply * or +, e.g., a (“;” b)* represents any of a, a;b, a;b;b, . . ..

expression := word+ “.” primitive expression | primitive expresion

primitive expression := (“{” expression (“,” expression)* “}”)+ primitive expression | primitive expression (“{” expression (“,” expression)* “}”)+ | word+

The optional prefix for each expression allows specification authors to tag expressions for traceability purposes. These tags have no semantic value with respect to the logical meaning of the specification.

C.3 Predicate Definitions

A Q specification is a collection of predicate definitions. Predicates are defined using the ‘‘ * is true iff * ’’ statement.

definition := “{” parm expression “}” is true iff “{” expression “}” “.”

parm expression := (“{” word+ (“,” word+)* “}”)+ parm expression | parm expression (“{” word+ (“,” word+)* “}”)+ | word+

C.4 Conjunctive and Disjunctive Lists

Requirements specifications often provide lists of conditions which represent logical conjunction, e.g., “all of the following,” or disjunction, e.g., “at least one of the following.” Such a list format is provided by the predicates ‘‘all of’’ and ‘‘any of.’’ The Q expression {all of {S}}, where S is a comma separated list of predicates, is semantically equivalent to V S, where V({x } ∪ A) = x ∧ (V A), and V{} = ⊤. Similarly, {any of {S}} is semantically equivalent to

W_{S, where} W_{({x } ∪ A) = x ∨ (}V_{A), and} W_{{} = ⊥.}

C.5 Argument Based Conjunctions and Disjunctions

The functions ‘‘each of * ’’ and ‘‘any of * ’’ are used to construct conjunctions and disjunctions, respectively, of a predicate over different arguments. These functions both have the type (t)list → t. The semantics of these functions is defined in terms of predicates (Boolean expressions that do not contain logical connectives). The equivalent logic expression is determining by evaluating the Boolean expression AE Ua P for ‘‘any of’’ or AE Ue P for

‘‘each of’’ using axioms [4]. These two functions map the application of a

predicate to a list of arguments into a disjunction or conjunction, respectively, of the predicate applied to each argument of the list, separately.

Although multiple uses of one of these keywords can be used within a predicate, mixtures of ‘‘any of’’ and ‘‘each of’’ within arguments to a single reference of a predicate are problematic. This is because it is unclear whether the expression containing argument keywords represents a conjunction of disjunctions or vice versa.

For example, the expression

{the {each of {apple, tomato}} is a {any of {vegetable, fruit}}}

may have been intended to mean either

{{{the {apple} is a {vegetable}} or {the {tomato} is a {vegetable}}}

and {{the {apple} is a {fruit}} or {the {tomato} is a {fruit}}}}

or, alternatively,

{{{the {apple} is a {vegetable}} and {the {tomato} is a {vegetable}}}

or {{the {apple} is a {fruit}} and {the {tomato} is a {fruit}}}}.

Clearly these two semantic evaluations are logically different.

Although the axioms for ‘‘any of’’ and ‘‘each pf’’ disambiguate such a construction, this rule would need to be learned and would not be obvious to a non-specialist from the text alone. Since this is counter to the objective of Q, mixtures of ‘‘any of’’ and ‘‘each of’’ are not allowed within arguments to the same predicate. The order of semantic evaluation in these situations can be made more clearly using expression aliasing.

C.6 Expression Aliasing

An expression alias is the same as the let statement found in functional programming languages such as ML [10]. The purpose of the alias is to assign a short name to a complex expression in order to make a portion of text more readable.

The Q expression {{x} is {y} in {E}} is semantically equivalent to {E} with y substituted for x. To encourage simpler specifications, the expression E must be a predicate. The predicate {{x} is {y} in {E}} is syntactic sugar for the lambda calculus expression (λ x.E)y. Similarly, the tuple form {{x,y} are {a,b} in {E}} is syntactic sugar for the lambda calculus expression (λ x, y.E)(a, b).

Using expression aliasing, the earlier ‘‘any of’’ / ‘‘each of’’ example can be disambiguated as

{{item} is {each of {apple, tomato}} in {the {item} is a {any of {vegetable, fruit}}}}

which results in a conjunction of disjunctions.

C.7 Argument Permutation

The predicates ‘‘ * are all distinct choices of * in * ’’ and ‘‘ * are

any distinct choices of * in * ’’ are used to construct conjunctions and

disjunctions involving permutations of arguments. An example of the use of this keyword was given above.

{{x} are all distinct choices of {A} in {E}} is syntactically equivalent to

{{x} are {each of {P(A)}} in {E}}, where P(A) is a list of all the permutations of tuples the same size as x uses elements of A. Similarly,

{{x} are any distinct choices of {A} in {E}} is syntactically equivalent to

{{x} are {any of {P(A)}} in {E}}.

C.8 Quantification

Universal and existential quantification are provided by the syntactic forms {for

any {x} {E}}, which is equivalent to ∀ x.E, and {there exists {x} such that

{E}}, which is equivalent to ∃ x.E.

D Test Frames for Flight Plan Creation

D.1 Introduction

The test frames presented in this appendix are base test frames satisfying term coverage for the requirement:

Correct Form.

Test frames are numbered i.j where i is the number of the test class [2] and j is the number of the test frame for that test class.

There are no test frames for test classes 59 and 87. This is because these test classes express facts implied by the specification.

Test class 59 is analogous to the test frame:

Stimuli Response
  1. NOT The flight is along a designated ATS route
  2. ATS flight track points are required by the
     appropriate ATS authority
  3. NOT Use ATS style track points

                                                false

Since the response is false, this implies that the specification asserts that the stimuli can never occur. And this seems consistent with the text of the conditions. An inconsistency would indicate an error in the specification.

Test class 87 is analogous to the test frame:

Stimuli Response
true 1. insert {Item 19 E} - {the four digit fuel
                    endurance in hours and minutes}
                 2. insert {Item 19 A} - {colour of aircraft and
                    significant markings}
                 3. insert {Item 19 C} - {name of pilot in command}

This test frame indicates that the response will always occur. Thus, these response conditions can be appended to each of the other test frames, if desired. Again, this seems consistent with the importance of the information in these fields of the flight plan.

D.2 Base Test Frames

--Test Frame 1.1:
 ROIDs: I7A
 Stimuli Response
   1. The radiotelephony call sign to be
      used by the aircraft will consist
      of {the registration marking of
      the aircraft preceeded by the ICAO
      telephony designator for the aircraft
      operating agency}

                                                1. insert {Item 7} -

{the registration

marking of the
aircraft}

--Test Frame 1.2:
 ROIDs: I7A
 Stimuli Response
   1. The radiotelephony call sign to be
      used by the aircraft will consist
      of {the registration marking of the
      aircraft}

                                                1. insert {Item 7} -

{the registration

                                                   marking of the
                                                   aircraft}

--Test Frame 1.3:
 ROIDs: I7A
 Stimuli Response
   1. NOT The aircraft
      is equipped with
      radio

                            1. insert {Item 7} - {the registration
                               marking of the aircraft}

--Test Frame 2.1:
 ROIDs: I7B
 Stimuli Response
   1. The radiotelephony call sign to be
      used by the aircraft will consist of

{the ICAO telephony designator for

      the operating agency followed by the
      flight identification}

                                                1. insert {Item
                                                   7} - {the ICAO
                                                   telephony
                                                   designator for
                                                   the operating
                                                   agency followed
                                                   by the flight
                                                   identification}

--Test Frame 3.1:
 ROIDs: I8FR
 Stimuli Response
   1. IFR rules 1. insert {Item 8 Flight Rules} - {I}

--Test Frame 4.1:
 ROIDs: I8FR
 Stimuli Response
   1. VFR rules 1. insert {Item 8
                                                   Flight Rules} -

{V}

--Test Frame 5.1:
 ROIDs: I8FR
 Stimuli Response
   1. IFR first 1. insert {Item 8 Flight Rules} - {Y}

--Test Frame 6.1:
 ROIDs: I8FR
 Stimuli Response
   1. VFR first 1. insert {Item 8 Flight Rules} - {Z}

--Test Frame 7.1:
 ROIDs: I8FT
 Stimuli Response
   1. Scheduled Air
      Service

                            1. insert {Item 8 Type of Flight} - {S}

--Test Frame 8.1:
 ROIDs: I8FT
 Stimuli Response
   1. Non-scheduled
      Air Transport
      Operation

                            1. insert {Item 8 Type of Flight} - {N}

--Test Frame 9.1:
 ROIDs: I8FT
 Stimuli Response
   1. General Aviation 1. insert {Item 8 Type of Flight} - {G}

--Test Frame 10.1:
 ROIDs: I8FT
 Stimuli Response
   1. Military 1. insert {Item 8 Type of Flight} - {M}

--Test Frame 11.1:
 ROIDs: I8FT
 Stimuli Response
   1. NOT Scheduled Air Service
   2. NOT Non-scheduled Air Transport
      Operation
   3. NOT General Aviation
   4. NOT Military

                                                1. insert {Item 8
                                                   Type of Flight} -

{X}

--Test Frame 12.1:
 ROIDs: I9N
 Stimuli Response
   1. There is more
      than one aircraft

                            1. insert {Item 9 Number of Aircraft} -

{the number of aircraft}

--Test Frame 13.1:
 ROIDs: I9T
 Stimuli Response
   1. This is a
      formation flight
      with more than
      one type

                            1. insert {Item 9 Type of Aircraft} -

{ZZZZ}

2. insert {Item 18} - {TYP/ Types of
   aircraft preceded by numbers of
   aircraft}

--Test Frame 13.2:
 ROIDs: I9T
 Stimuli Response
   1. NOT There is an
      appropriate ICAO
      type designator

                            1. insert {Item 9 Type of Aircraft} -

{ZZZZ}

                            2. insert {Item 18} - {TYP/ Types of
                               aircraft preceded by numbers of
                               aircraft}

--Test Frame 14.1:
 ROIDs: I9T
 Stimuli Response
   1. There is an appropriate ICAO type
      designator
   2. NOT This is a formation flight with
      more than one type

                                                1. insert {Item
                                                   9 Type of
                                                   Aircraft} - {the
                                                   appropriate ICAO
                                                   type designator}

--Test Frame 15.1:
 ROIDs: I9W
 Stimuli Response
   1. The maximum certified take-off mass
      is {136000} kg or more

                                                1. insert {Item 9
                                                   Wake Turnulence}
                                                   - {/H}

--Test Frame 16.1:
 ROIDs: I9W
 Stimuli Response
   1. The maximum certified take-off mass
      is less than {136000} kg but more
      than {7000} kg

                                                1. insert {Item 9
                                                   Wake Turnulence}
                                                   - {/M}

--Test Frame 17.1:
 ROIDs: I9W
 Stimuli Response
   1. The maximum certified take-off mass
      is {7000} kg or less

                                                1. insert {Item 9
                                                   Wake Turnulence}
                                                   - {/L}

--Test Frame 18.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable

                                                1. insert {Item 10
                                                   CNA} - {S}

--Test Frame 19.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. COM/NAV/approach aid equipment is

{LORAN C}

                                                1. insert {Item 10
                                                   CNA} - {C}

--Test Frame 20.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. COM/NAV/approach aid equipment is

{DME}

                                                1. insert {Item 10
                                                   CNA} - {D}

--Test Frame 21.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. COM/NAV/approach aid equipment is

{ADF}

                                                1. insert {Item 10
                                                   CNA} - {F }

--Test Frame 22.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. COM/NAV/approach aid equipment is

{GNSS}

                                                1. insert {Item 10
                                                   CNA} - {G}

--Test Frame 23.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. COM/NAV/approach aid equipment is {HF
      RTF}

                                                1. insert {Item 10
                                                   CNA} - {H}

--Test Frame 24.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. COM/NAV/approach aid equipment is

{Inertial Navigation}

                                                1. insert {Item 10
                                                   CNA} - {I}

--Test Frame 25.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. COM/NAV/approach aid equipment is

{Data Link}

                                                1. insert {Item 10
                                                   CNA} - {J}
                                                2. insert {Item 18}
                                                   - {DAT/}

--Test Frame 26.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. COM/NAV/approach aid equipment is

{MLS}

                                                1. insert {Item 10
                                                   CNA} - {K}

--Test Frame 27.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. COM/NAV/approach aid equipment is

{ILS}

                                                1. insert {Item 10
                                                   CNA} - {L}

--Test Frame 28.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. COM/NAV/approach aid equipment is

{Omega}

1. insert {Item 10
   CNA} - {M}

--Test Frame 29.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. COM/NAV/approach aid equipment is

{VOR}

                                                1. insert {Item 10
                                                   CNA} - {O}

--Test Frame 30.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. COM/NAV/approach aid equipment is

{RNP type certification}

                                                1. insert {Item 10
                                                   CNA} - {R}

--Test Frame 31.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. COM/NAV/approach aid equipment is

{TACAN}

                                                1. insert {Item 10
                                                   CNA} - {T }

--Test Frame 32.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. COM/NAV/approach aid equipment is

{UHF RTF}

                                                1. insert {Item 10
                                                   CNA} - {U}

--Test Frame 33.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. COM/NAV/approach aid equipment is

{VHF RTF}

1. insert {Item 10
   CNA} - {V}

--Test Frame 34.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. COM/NAV/approach aid equipment is

{other}

                                                1. insert {Item 10
                                                   CNA} - {Z}
                                                2. insert {Item 18}
                                                   - {COM/ or NAV/}

--Test Frame 35.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. {Y} is prescribed by ATS

                                                1. insert {Item 10
                                                   CNA} - {Y}

--Test Frame 36.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. {X} is prescribed by ATS

                                                1. insert {Item 10
                                                   CNA} - {X}

--Test Frame 37.1:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid
      equipment for the route to be flown
      is carried and is serviceable
   2. {W} is prescribed by ATS

                                                1. insert {Item 10
                                                   CNA} - {W}

--Test Frame 38.1:
 ROIDs: I10SE
 Stimuli Response
   1. NOT SSR equipment is present 1. insert {Item 10
                                                   SE} - {N}

--Test Frame 39.1:
 ROIDs: I10SE
 Stimuli Response
   1. SSR transponder mode A 1. insert {Item 10
                                                   SE} - {A}

--Test Frame 40.1:
 ROIDs: I10SE
 Stimuli Response
   1. SSR transponder mode A and mode C 1. insert {Item 10
                                                   SE} - {C}

--Test Frame 41.1:
 ROIDs: I10SE
 Stimuli Response
   1. SSR transponder mode S only 1. insert {Item 10
                                                   SE} - {X}

--Test Frame 42.1:
 ROIDs: I10SE
 Stimuli Response
   1. SSR transponder mode S including
      pressure-altitude trasmission

                                                1. insert {Item 10
                                                   SE} - {P}

--Test Frame 43.1:
 ROIDs: I10SE
 Stimuli Response
   1. SSR transponder mode S including
      aircraft identification trasmission

                                                1. insert {Item 10
                                                   SE} - {I}

--Test Frame 44.1:
 ROIDs: I10SE
 Stimuli Response
   1. SSR transponder mode S including
      pressure-altitude and aicraft
      identification trasmission

                                                1. insert {Item 10
                                                   SE} - {S}

--Test Frame 45.1:
 ROIDs: I10SE
 Stimuli Response
   1. ADS capability 1. insert {Item 10
                                                   SE} - {D}

--Test Frame 46.1:
 ROIDs: I13
 Stimuli Response
   1. The flight plan
      is received from
      an aircraft in
      flight

                            1. insert {Item 13 A} - {AFIL}
                            2. insert {Item 18} - {DEP/ the
                               four-letter location indicator of
                               the location of the ATS unit from
                               which supplementary flight data can
                               be obtained}

--Test Frame 47.1:
 ROIDs: I13
 Stimuli Response
   1. NOT The flight plan is received from
      an aircraft in flight
   2. NOT Location indicator has been
      assigned

                                                1. insert {Item 13
                                                   A} - {ZZZZZ}

                                                2. insert {Item 13}
                                                   - {DEP/ aerodrome
                                                   name}

--Test Frame 48.1:
 ROIDs: I13
 Stimuli Response
   1. NOT The flight plan is received from
      an aircraft in flight
   2. Location indicator has been assigned

                                                1. insert {Item 13
                                                   A} - {the ICAO
                                                   four-letter
                                                   location
                                                   indicator of
                                                   the departure
                                                   aerodrome}

--Test Frame 49.1:
 ROIDs: I13
 Stimuli Response
   1. The flight plan
      was submitted
      before departure

                            1. insert {Item 13 B} - {the estimated
                               off-block time}

--Test Frame 50.1:
 ROIDs: I13
 Stimuli Response
   1. NOT The flight
      plan was
      submitted before
      departure

                            1. insert {Item 13 B} - { {the estimated
                               time} over the first point of the
                               route to which the flight plan
                               applies} OR insert {Item 13 B} - {

{the actual time} over the first

                               point of the route to which the
                               flight plan applies}

--Test Frame 51.1:
 ROIDs: I15A
 Stimuli Response
   1. Mach number is
      prescribed by the
      appropriate ATS
      authority

                            1. insert {Item 15 A} - {the true
                               airspeed for the first or the whole
                               cruising portion of the flight
                               expressed as {M followed by 3 digits
                               of Mach hundredths} }

--Test Frame 52.1:
 ROIDs: I15A
 Stimuli Response
   1. NOT Mach number
      is prescribed by
      the appropriate
      ATS authority

                            1. insert {Item 15 A} - {the true
                               airspeed for the first or the whole
                               cruising portion of the flight
                               expressed as {N followed by 4 digits
                               of knots} } OR insert {Item 15 A} -

{the true airspeed for the first or

                               the whole cruising portion of the
                               flight expressed as {K followed by 4
                               digits of kilometres per hour} }

--Test Frame 53.1:
 ROIDs: I15B
 Stimuli Response
   1. Flight is
      uncontrolled
      VFR

                            1. insert {Item 15 B} - {VFR}

--Test Frame 54.1:
 ROIDs: I15B
 Stimuli Response
   1. NOT Flight is
      uncontrolled VFR

                            1. insert {Item 15 B} - {the planned
                               cruising level for the first or the
                               whole portion of the route to be
                               flown as {A followed by 3 digits
                               of Altitude in tens of metres} } OR
                               insert {Item 15 B} - {the planned
                               cruising level for the first or the
                               whole portion of the route to be
                               flown as {S followed by 4 digits of
                               Standard Metric Level in tens of
                               metres} } OR insert {Item 15 B} -

{the planned cruising level for the

                               first or the whole portion of the
                               route to be flown as {F followed by 3
                               digits of Flight level} }

--Test Frame 55.1:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS
      route
   2. The departure aerodrome is {connected
      to} the ATS route

                                                1. insert {Item
                                                   15 C} - {the
                                                   designator of the
                                                   first ATS route}

--Test Frame 55.2:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS
      route
   2. The departure aerodrome is {located
      on} the ATS route

                                                1. insert {Item
                                                   15 C} - {the
                                                   designator of the
                                                   first ATS route}

--Test Frame 56.1:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS
      route
   2. NOT (The departure aerodrome is

{connected to} the ATS route)

3. NOT (The departure aerodrome is

{located on} the ATS route)

                                                1. insert {Item 15
                                                   C} - {the letters
                                                   DCT followed
                                                   by the point
                                                   of joining the
                                                   first ATS route
                                                   followed by the
                                                   designator of the
                                                   ATS route}

--Test Frame 57.1:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS
      route
   2. A change of {flight rules} is planned
      at {point}
   3. The flight to the {next {point} }
      will be outside a designated route
   4. NOT ( {point} is defined by
      geological co-ordinates)

                                                1. insert {Item 15
                                                   C} - { {point}
                                                   followed by DCT}

--Test Frame 57.2:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS
      route
   2. A change of {ATS route other than
      same direction lower/upper} is
      planned at {point}
   3. The flight to the {next {point} }
      will be outside a designated route
   4. NOT ( {next {point} } is defined by
      geological co-ordinates)

                                                1. insert {Item 15
                                                   C} - { {point}
                                                   followed by DCT}

--Test Frame 57.3:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS
      route
   2. A change of {level} is planned at

{point}

   3. The flight to the {next {point} }
      will be outside a designated route
   4. NOT ( {point} is defined by
      geological co-ordinates)

                                                1. insert {Item 15
                                                   C} - { {point}
                                                   followed by DCT}

--Test Frame 57.4:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS
      route
   2. A change of {speed} is planned at

{point}

   3. The flight to the {next {point} }
      will be outside a designated route
   4. NOT ( {point} is defined by
      geological co-ordinates)

                                                1. insert {Item 15
                                                   C} - { {point}
                                                   followed by DCT}

--Test Frame 58.1:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS
      route
   2. A change of {flight rules} is planned
      at {point}
   3. {next {point} } is defined by
      geological co-ordinates
   4. {point} is defined by geological
      co-ordinates

                                                1. insert {Item 15
                                                   C} - { {point}
                                                   followed by the
                                                   designator of the
                                                   next ATS route
                                                   segment}

--Test Frame 58.2:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS
      route
   2. A change of {ATS route other than
      same direction lower/upper} is
      planned at {point}
   3. NOT (The flight to the {next {point}

} will be outside a designated route)

1. insert {Item 15
   C} - { {point}
   followed by the
   designator of the
   next ATS route
   segment}

--Test Frame 58.3:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS
      route
   2. A change of {level} is planned at

{point}

3. NOT (The flight to the {next {point}

} will be outside a designated route)

                                                1. insert {Item 15
                                                   C} - { {point}
                                                   followed by the
                                                   designator of the
                                                   next ATS route
                                                   segment}

--Test Frame 58.4:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS
      route
   2. A change of {speed} is planned at

{point}

3. NOT (The flight to the {next {point}

} will be outside a designated route)

                                                1. insert {Item 15
                                                   C} - { {point}
                                                   followed by the
                                                   designator of the
                                                   next ATS route
                                                   segment}

--Test Frame 60.1:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated
      ATS route
   2. ATS flight track points are required
      by the appropriate ATS authority
   3. {point A} and {point B} are
      successive points
   4. {point B} is defined by {bearing and
      distance}
   5. {point A} is defined by {bearing and
      distance}

                                                1. insert {Item 15
                                                   C} - {DCT between

{point A} and {point B} }

--Test Frame 61.1:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated
      ATS route
   2. ATS flight track points are required
      by the appropriate ATS authority
   3. {point A} and {point B} are
      successive points
   4. NOT ( {point A} is defined by

{bearing and distance} )

1. insert {Item 15
   C} - { {point
   A} followed by

{point B} }

--Test Frame 61.2:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated
      ATS route
   2. ATS flight track points are required
      by the appropriate ATS authority
   3. {point A} and {point B} are
      successive points
   4. NOT ( {point B} is defined by

{bearing and distance} )

1. insert {Item 15
   C} - { {point
   A} followed by

{point B} }

--Test Frame 62.1:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated
      ATS route
   2. ATS flight track points are required
      by the appropriate ATS authority
   3. {point A} and {point B} are
      successive points
   4. {point B} is defined by {goegraphical
      co-ordinates}
   5. {point A} is defined by {goegraphical
      co-ordinates}

                                                1. insert {Item 15
                                                   C} - {DCT between

{point A} and {point B} }

--Test Frame 63.1:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated
      ATS route
   2. ATS flight track points are required
      by the appropriate ATS authority
   3. {point A} and {point B} are
      successive points
   4. NOT ( {point A} is defined by

{goegraphical co-ordinates} )

1. insert {Item 15
   C} - { {point
   A} followed by

{point B} }

--Test Frame 63.2:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated
      ATS route
   2. ATS flight track points are required
      by the appropriate ATS authority
   3. {point A} and {point B} are
      successive points
   4. NOT ( {point B} is defined by

{goegraphical co-ordinates} )

1. insert {Item 15
   C} - { {point
   A} followed by

{point B} }

--Test Frame 64.1:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated
      ATS route
   2. NOT ATS flight track points are
      required by the appropriate ATS
      authority
   3. NOT (A change of {flight rules} is
      planned at {point} )
   4. NOT (A change of {track} is planned
      at {point} )
   5. NOT (A change of {level} is planned
      at {point} )

   6. NOT (A change of {speed} is planned
      at {point} )

                                                1. NOT (insert {Item
                                                   15 C} - { {point}
                                                   details} )

--Test Frame 64.2:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated
      ATS route
   2. NOT ATS flight track points are
      required by the appropriate ATS
      authority
   3. {point} and {next {point} } are
      normally more than {370km} apart
   4. {point} and {next {point} } are
      normally more than {30 minutes flying
      time} apart

                                                1. NOT (insert {Item
                                                   15 C} - { {point}
                                                   details} )

--Test Frame 65.1:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated
      ATS route
   2. NOT ATS flight track points are
      required by the appropriate ATS
      authority
   3. NOT ( {point} and {next {point} } are
      normally more than {30 minutes flying
      time} apart)

   4. A change of {flight rules} is planned
      at {point}

                                                1. insert {Item 15
                                                   C} - { {point}
                                                   details}

--Test Frame 65.2:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated
      ATS route

   2. NOT ATS flight track points are
      required by the appropriate ATS
      authority
   3. NOT ( {point} and {next {point} } are
      normally more than {370km} apart)
   4. A change of {track} is planned at

{point}

                                                1. insert {Item 15
                                                   C} - { {point}
                                                   details}

--Test Frame 65.3:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated
      ATS route
   2. NOT ATS flight track points are
      required by the appropriate ATS
      authority
   3. NOT ( {point} and {next {point} } are
      normally more than {30 minutes flying
      time} apart)
   4. A change of {level} is planned at

{point}

1. insert {Item 15
   C} - { {point}
   details}

--Test Frame 65.4:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated
      ATS route
   2. NOT ATS flight track points are
      required by the appropriate ATS
      authority
   3. NOT ( {point} and {next {point} } are
      normally more than {30 minutes flying
      time} apart)

   4. A change of {speed} is planned at

{point}

                                                1. insert {Item 15
                                                   C} - { {point}
                                                   details}

--Test Frame 66.1:
 ROIDs: I15C I15C1
 Stimuli Response
   1. NOT The flight
      is along a
      designated ATS
      route
   2. {point} is listed
      in Item 15 C

                            1. the code designator assigned to

{route segment} including where

appropriate the coded designator
assigned to the standard {arrival}
route is associated with {point}
OR the code designator assigned
to {route segment} including where
appropriate the coded designator
assigned to the standard {departure}
route is associated with {point}
OR the code designator assigned to

{route} including where appropriate

the coded designator assigned to
the standard {arrival} route is
associated with {point} OR the
code designator assigned to {route}
including where appropriate the coded
designator assigned to the standard

{departure} route is associated with {point}

--Test Frame 67.1:
 ROIDs: I15C I15C2
 Stimuli Response
   1. NOT The flight
      is along a
      designated ATS
      route

   2. {point} is listed
      in Item 15 C

   3. NOT (A
      significant point
      code designator
      has been assigned
      to {point} )

                            1. 2 figures describing latitude in
                               degrees followed by {S} followed by
                               3 figures describing longitude in
                               degrees followed by {W} is associated
                               with {point} OR 2 figures describing
                               latitude in degrees followed by {S}
                               followed by 3 figures describing
                               longitude in degrees followed by

{E} is associated with {point} OR

2 figures describing latitude in
degrees followed by {N} followed by
3 figures describing longitude in
degrees followed by {W} is associated
with {point} OR 2 figures describing
latitude in degrees followed by {N}
followed by 3 figures describing
longitude in degrees followed by

{E} is associated with {point} OR

4 figures describing latitude in
degrees and tens of units of minutes
followed by {S} followed by 5 figures
describing longitude in degrees and
tens of units of minutes followed
by {W} is associated with {point}
OR 4 figures describing latitude in
degrees and tens of units of minutes
followed by {S} followed by 5 figures
describing longitude in degrees and
tens of units of minutes followed
by {E} is associated with {point}
OR 4 figures describing latitude in
degrees and tens of units of minutes
followed by {N} followed by 5 figures
describing longitude in degrees and
tens of units of minutes followed
by {W} is associated with {point}
OR 4 figures describing latitude
in degrees and tens of units of
minutes followed by {N} followed
by 5 figures describing longitude in
degrees and tens of units of minutes
followed by {E} is associated with

{point} OR the 2 or 3 character

identification of the navigation aid
followed by the 3 figure bearing from
the aid in degrees magnetic followed
by the distance from the aid in 3
figures expressing nautical miles is
associated with {point}

--Test Frame 68.1:
 ROIDs: I15C I15C2
 Stimuli Response
   1. NOT The flight is along a designated
      ATS route
   2. {point} is listed in Item 15 C

   3. A significant point code designator
      has been assigned to {point}

                                                1. the 2 to 5
                                                   characters of the
                                                   assigned coded
                                                   designator is
                                                   associated with

{point}

--Test Frame 69.1:
 ROIDs: I15C I15C3
 Stimuli Response
   1. NOT The flight is along a designated
      ATS route
   2. {point} is listed in Item 15 C
   3. A change of {level} is planned at

{point}

1. an oblique
   stroke and both
   the cruising
   speed and the
   cruising level is
   associated with

{point}

--Test Frame 70.1:
 ROIDs: I15C I15C3
 Stimuli Response
   1. NOT The flight is along a designated
      ATS route

   2. {point} is listed in Item 15 C
   3. A change of {speed - 0.01 Mach or
      more} is planned at {point}

                                                1. an oblique
                                                   stroke and both
                                                   the cruising
                                                   speed and the
                                                   cruising level is
                                                   associated with

{point}

--Test Frame 71.1:
 ROIDs: I15C I15C3
 Stimuli Response
   1. NOT The flight is along a designated
      ATS route
   2. {point} is listed in Item 15 C
   3. A change of {speed - 5pc TAS or more}
      is planned at {point}

                                                1. an oblique
                                                   stroke and both
                                                   the cruising
                                                   speed and the
                                                   cruising level is
                                                   associated with

{point}

--Test Frame 72.1:
 ROIDs: I15C I15C4
 Stimuli Response
   1. NOT The flight is along a designated
      ATS route
   2. {point} is listed in Item 15 C

   3. A change of {flight rules} is planned
      at {point}

   4. IFR to VFR

                                                1. the letters VFR
                                                   are associated
                                                   with {point}

--Test Frame 73.1:
 ROIDs: I15C I15C4
 Stimuli Response
   1. NOT The flight is along a designated
      ATS route

   2. {point} is listed in Item 15 C
   3. A change of {flight rules} is planned
      at {point}
   4. NOT IFR to VFR
   5. VFR to IFR

                                                1. the letters IFR
                                                   are associated
                                                   with {point}

--Test Frame 74.1:
 ROIDs: I15C I15C5
 Stimuli Response
   1. NOT The flight
      is along a
      designated ATS
      route

   2. {point} is listed
      in Item 15 C
   3. A change of

{level - climb}

is planned at

{point}

1. an oblique stroke followed by
   the speed to be maintained during
   cruise climb followed by {the level
   above which cruise climb is planned
   followed by PLUS} is associated with

{point} OR an oblique stroke followed

                               by the speed to be maintained during
                               cruise climb followed by {the two
                               levels defining the layer to be
                               occupied during cruide climb} is
                               associated with {point}

--Test Frame 75.1:
 ROIDs: I16-1
 Stimuli Response
   1. NOT Location
      indicator has
      been assigned

                            1. insert {Item 16 Dest} - {ZZZZ
                               followed by the total estimated
                               elapsed time}
                            2. insert {Item 18} - {DEST/ the name of
                               the aerodrome}

--Test Frame 76.1:
 ROIDs: I16-1
 Stimuli Response
   1. Location
      indicator has
      been assigned

                            1. insert {Item 16 Dest} - {the ICAO
                               four letter location indicator of the
                               destination aerodrome followed by the
                               total estimated elapsed time}

--Test Frame 77.1:
 ROIDs: I16-2
 Stimuli Response
   1. NOT Location
      indicator has
      been assigned
      to the alternate
      aerodrome

                            1. insert {Item 16 Alt} - {ZZZZ}

                            2. insert {Item 18} - {ALTN/ the name of
                               the alternate aerodrome}

--Test Frame 78.1:
 ROIDs: I18-1
 Stimuli Response
   1. {point} is a {FIR boundary}
      prescribed {by the approapriate ATS
      authority}

                                                1. insert {Item 18}
                                                   - {EET/ {point} }

--Test Frame 78.2:
 ROIDs: I18-1
 Stimuli Response
   1. {point} is a {FIR boundary}
      prescribed {on the basis of regional
      air navigation agreements}

                                                1. insert {Item 18}
                                                   - {EET/ {point} }

--Test Frame 78.3:
 ROIDs: I18-1
 Stimuli Response
   1. {point} is a {significant point}
      prescribed {by the approapriate ATS
      authority}

                                                1. insert {Item 18}
                                                   - {EET/ {point} }

--Test Frame 78.4:
 ROIDs: I18-1
 Stimuli Response
   1. {point} is a {significant point}
      prescribed {on the basis of regional
      air navigation agreements}

                                                1. insert {Item 18}
                                                   - {EET/ {point} }

--Test Frame 79.1:
 ROIDs: I18-2
 Stimuli Response
   1. The route is
      revised

                            1. insert {Item 18} - {RIF/route details
                               to the revised destination aerodrome
                               followed by the ICAO four letter
                               location indicator of the aerodrome}

--Test Frame 80.1:
 ROIDs: I18-3
 Stimuli Response
   1. The registration markings of the
      aircraft are different from the
      aircraft identification in Item 7

                                                1. insert

{Item 18} - {REG/registration

                                                   markings of the
                                                   aircraft}

--Test Frame 81.1:
 ROIDs: I18-4
 Stimuli Response
   1. A SELCAL Code is prescribed by the
      appropriate ATS authority

                                                1. insert {Item 18}
                                                   - {SEL/SELCAL
                                                   Code}

--Test Frame 82.1:
 ROIDs: I18-5
 Stimuli Response
   1. NOT The name of the operator
      is obvious from the aircraft
      identification in Item 7

                                                1. insert {Item 18}
                                                   - {OPR/operator
                                                   name}

--Test Frame 83.1:
 ROIDs: I18-6
 Stimuli Response
   1. There is a reason for special
      handling

                                                1. insert {Item 18}
                                                   - {STS/reason for
                                                   special handling}

--Test Frame 84.1:
 ROIDs: I18-7
 Stimuli Response
   1. Aircraft performance data is
      prescribed by the appropriate ATS
      authority

                                                1. insert {Item 18}
                                                   - {PER/Aircraft
                                                   performance data}

--Test Frame 85.1:
 ROIDs: I18-8
 Stimuli Response
   1. {aerodrome} is an en-route alternate
      aerodrome

                                                1. insert {Item
                                                   18} - {RALT/

{aerodrome} }

--Test Frame 86.1:
 ROIDs: I18-9
 Stimuli Response
   1. Any other plain lanugage remarks are
      necessary

                                                1. insert {Item 18}
                                                   - {RMK/any other
                                                   remarks}

--Test Frame 88.1:
 ROIDs: I19P
 Stimuli Response
   1. Number of persons is required by the
      ATS authority
   2. NOT The total number of persons is
      known

                                                1. insert {Item 19
                                                   P} - {TBN}

--Test Frame 89.1:
 ROIDs: I19P
 Stimuli Response
   1. Number of persons is required by the
      ATS authority
   2. The total number of persons is known

                                                1. insert {Item 19
                                                   P} - {the total
                                                   number of persons
                                                   [passengers and
                                                   crew] on board}

--Test Frame 90.1:
 ROIDs: I19ES1
 Stimuli Response
   1. NOT UHF on frequency 243.0 MHz is
      available

                                                1. cross out {Item
                                                   19 R} - {U}

--Test Frame 91.1:
 ROIDs: I19ES1
 Stimuli Response
   1. NOT VHF on frequency 121.5 MHz is
      available

                                                1. cross out {Item
                                                   19 R} - {V}

--Test Frame 92.1:
 ROIDs: I19ES1
 Stimuli Response
   1. NOT Emergency location beacon is
      available

                                                1. cross out {Item
                                                   19 R} - {E}

--Test Frame 93.1:
 ROIDs: I19ES2
 Stimuli Response
   1. NOT Polar equipment is carried 1. cross out {Item
                                                   19 S} - {P}

--Test Frame 94.1:
 ROIDs: I19ES2
 Stimuli Response
   1. NOT Desert equipment is carried 1. cross out {Item
                                                   19 S} - {D}

--Test Frame 95.1:
 ROIDs: I19ES2
 Stimuli Response
   1. NOT Maritime equipment is carried 1. cross out {Item
                                                   19 S} - {M}

--Test Frame 96.1:
 ROIDs: I19ES2
 Stimuli Response
   1. NOT Jungle equipment is carried 1. cross out {Item
                                                   19 S} - {J}

--Test Frame 97.1:
 ROIDs: I19ES3
 Stimuli Response
   1. NOT Life jackets
      are carried

                            1. cross out {Item 19 J} - {V}
                            2. cross out {Item 19 J} - {U}
                            3. cross out {Item 19 J} - {F }
                            4. cross out {Item 19 J} - {L}

--Test Frame 98.1:
 ROIDs: I19ES3
 Stimuli Response
   1. Life jackets are carried
   2. NOT Life jackets are equipped with
      lights

                                                1. cross out {Item
                                                   19 J} - {L}

--Test Frame 99.1:
 ROIDs: I19ES3
 Stimuli Response
   1. Life jackets are carried
   2. NOT Life jackets are equipped with
      fluorescein

                                                1. cross out {Item
                                                   19 J} - {F }

--Test Frame 100.1:
 ROIDs: I19ES3
 Stimuli Response
   1. Life jackets are
      carried

                            1. NOT (cross out {Item 19 J} - {U} ) OR
                               cross out {Item 19 R} - {U}
                            2. NOT (cross out {Item 19 R} - {U} ) OR
                               cross out {Item 19 J} - {U}
                            3. NOT (cross out {Item 19 J} - {V} ) OR
                               cross out {Item 19 R} - {V}
                            4. NOT (cross out {Item 19 R} - {V} ) OR
                               cross out {Item 19 J} - {V}

--Test Frame 101.1:
 ROIDs: I19ES4
 Stimuli Response
   1. NOT Dinghies are
      carried

                            1. cross out {Item 19 D} - {C}
                            2. cross out {Item 19 D} - {D}

--Test Frame 102.1:
 ROIDs: I19ES4
 Stimuli Response
   1. Dinghies are
      carried

                            1. insert {Item 19 D} - {number of
                               dinghies carried}
                            2. insert {Item 19 D} - {total capacity
                               in persons of all dinghies carried}
                            3. insert {Item 19 D} - {colour of
                               dinghies}

--Test Frame 103.1:
 ROIDs: I19ES4
 Stimuli Response
   1. Dinghies are carried
   2. NOT Dinghies are covered

                                                1. cross out {Item
                                                   19 D} - {C}

--Test Frame 104.1:
 ROIDs: I19ES6
 Stimuli Response
   1. NOT There are remarks 1. cross out {Item
                                                   19 N} - {N}

--Test Frame 105.1:
 ROIDs: I19ES6
 Stimuli Response
   1. There are remarks 1. indicate {Item 19 N} - {any other
                               survival equipment carried and any
                               other remarks regarding survival
                               equipment}

E Test Frames for Flight Plan Validation

E.1 Introduction

The test frames presented in this appendix satisfy term coverage for the following requirement:

if not Correct Form then report error.

Base test frames are presented in Section E.2. Differentiated versions of these test frames are presented in Section E.3.

E.2 Base Test Frames

--Test Frame 1.1:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. {point} is listed in Item 15 C
   3. NOT (A significant point code designator has
      been assigned to {point} )
   4. NOT (2 figures describing latitude in degrees
      followed by {S} followed by 3 figures describing
      longitude in degrees followed by {W} is
      associated with {point} )

   5. NOT (2 figures describing latitude in degrees
      followed by {S} followed by 3 figures describing
      longitude in degrees followed by {E} is
      associated with {point} )
   6. NOT (2 figures describing latitude in degrees
      followed by {N} followed by 3 figures describing
      longitude in degrees followed by {W} is
      associated with {point} )
   7. NOT (2 figures describing latitude in degrees
      followed by {N} followed by 3 figures describing
      longitude in degrees followed by {E} is
      associated with {point} )
   8. NOT (4 figures describing latitude in degrees
      and tens of units of minutes followed by {S}
      followed by 5 figures describing longitude in
      degrees and tens of units of minutes followed by

{W} is associated with {point} )

9. NOT (4 figures describing latitude in degrees
   and tens of units of minutes followed by {S}
   followed by 5 figures describing longitude in
   degrees and tens of units of minutes followed by

{E} is associated with {point} )

10. NOT (4 figures describing latitude in degrees
    and tens of units of minutes followed by {N}
    followed by 5 figures describing longitude in
    degrees and tens of units of minutes followed by

{W} is associated with {point} )

11. NOT (4 figures describing latitude in degrees
    and tens of units of minutes followed by {N}
    followed by 5 figures describing longitude in
    degrees and tens of units of minutes followed by

{E} is associated with {point} )

12. NOT (the 2 or 3 character identification of the
    navigation aid followed by the 3 figure bearing
    from the aid in degrees magnetic followed by the
    distance from the aid in 3 figures expressing
    nautical miles is associated with {point} )

                                                        1. report
                                                           error

--Test Frame 1.2:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. NOT (A change of {flight rules} is planned at

{point} )

   3. NOT (A change of {level} is planned at {point} )
   4. NOT (A change of {speed} is planned at {point} )
   5. NOT ATS flight track points are required by the
      appropriate ATS authority
   6. insert {Item 15 C} - { {point} details}
   7. NOT (A change of {track} is planned at {point} )

                                                          1. report
                                                             error

--Test Frame 1.3:
 ROIDs: I8FT
 Stimuli Response
   1. Military
   2. NOT (insert {Item 8 Type of Flight} - {M} )

                                                          1. report
                                                             error

--Test Frame 1.4:
 ROIDs: I8FT
 Stimuli Response
   1. NOT Scheduled Air Service
   2. NOT Non-scheduled Air Transport Operation
   3. NOT General Aviation
   4. NOT Military
   5. NOT (insert {Item 8 Type of Flight} - {X} )

                                                          1. report
                                                             error

--Test Frame 1.5:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS route
   2. A change of {ATS route other than same direction
      lower/upper} is planned at {point}
   3. {next {point} } is defined by geological
      co-ordinates
   4. {point} is defined by geological co-ordinates
   5. NOT (insert {Item 15 C} - { {point} followed by
      the designator of the next ATS route segment} )

                                                          1. report
                                                             error

--Test Frame 1.6:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. ATS flight track points are required by the
      appropriate ATS authority
   3. {point} and {point B} are successive points
   4. {point B} is defined by {bearing and distance}
   5. {point} is defined by {bearing and distance}
   6. NOT (insert {Item 15 C} - {DCT between {point}
      and {point B} } )

                                                          1. report
                                                             error

--Test Frame 1.7:
 ROIDs: I15B
 Stimuli Response
   1. NOT Flight is uncontrolled VFR
   2. NOT (insert {Item 15 B} - {the planned cruising
      level for the first or the whole portion of the
      route to be flown as {A followed by 3 digits of
      Altitude in tens of metres} } )
   3. NOT (insert {Item 15 B} - {the planned cruising
      level for the first or the whole portion of the
      route to be flown as {S followed by 4 digits of
      Standard Metric Level in tens of metres} } )
   4. NOT (insert {Item 15 B} - {the planned cruising
      level for the first or the whole portion of the
      route to be flown as {F followed by 3 digits of
      Flight level} } )

                                                          1. report
                                                             error

--Test Frame 1.8:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. {point} is listed in Item 15 C
   3. NOT (the code designator assigned to {route
      segment} including where appropriate the coded
      designator assigned to the standard {arrival}
      route is associated with {point} )
   4. NOT (the code designator assigned to {route
      segment} including where appropriate the coded
      designator assigned to the standard {departure}
      route is associated with {point} )
   5. NOT (the code designator assigned to {route}
      including where appropriate the coded designator
      assigned to the standard {arrival} route is
      associated with {point} )
   6. NOT (the code designator assigned to {route}
      including where appropriate the coded designator
      assigned to the standard {departure} route is
      associated with {point} )

                                                          1. report
                                                             error

--Test Frame 1.9:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS route
   2. A change of {speed} is planned at {point}
   3. The flight to the {next {point} } will be
      outside a designated route
   4. NOT ( {point} is defined by geological
      co-ordinates)
   5. NOT (insert {Item 15 C} - { {point} followed by
      DCT} )

                                                          1. report
                                                             error

--Test Frame 1.10:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. A change of {flight rules} is planned at {point}
   3. {point} is listed in Item 15 C
   4. NOT IFR to VFR
   5. VFR to IFR
   6. NOT (the letters IFR are associated with {point}
      )

                                                          1. report
                                                             error

--Test Frame 1.11:
 ROIDs: I15A
 Stimuli Response
   1. NOT Mach number is prescribed by the appropriate
      ATS authority
   2. NOT (insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {N followed by 4 digits of
      knots} } )
   3. NOT (insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {K followed by 4 digits of
      kilometres per hour} } )

                                                          1. report
                                                             error

--Test Frame 1.12:
 ROIDs: I13
 Stimuli Response
   1. NOT The flight plan was submitted before
      departure
   2. NOT (insert {Item 13 B} - { {the estimated time}
      over the first point of the route to which the
      flight plan applies} )
   3. NOT (insert {Item 13 B} - { {the actual time}
      over the first point of the route to which the
      flight plan applies} )

                                                          1. report
                                                             error

--Test Frame 1.13:
 ROIDs: I9T
 Stimuli Response
   1. There is an appropriate ICAO type designator
   2. NOT This is a formation flight with more than
      one type
   3. NOT (insert {Item 9 Type of Aircraft} - {the
      appropriate ICAO type designator} )

                                                          1. report
                                                             error

--Test Frame 1.14:
 ROIDs: I19P
 Stimuli Response
   1. Number of persons is required by the ATS
      authority
   2. The total number of persons is known
   3. NOT (insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board} )

                                                          1. report
                                                             error

--Test Frame 1.15:
 ROIDs: I19ES3
 Stimuli Response
   1. NOT (cross out {Item 19 R} - {V} )
   2. Life jackets are carried
   3. cross out {Item 19 J} - {V}

                                                          1. report
                                                             error

--Test Frame 1.16:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS route
   2. NOT (The departure aerodrome is {connected to}
      the ATS route)
   3. NOT (The departure aerodrome is {located on} the
      ATS route)
   4. NOT (insert {Item 15 C} - {the letters DCT
      followed by the point of joining the first ATS
      route followed by the designator of the ATS
      route} )

                                                          1. report
                                                             error

--Test Frame 1.17:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. {point} is listed in Item 15 C
   3. A change of {level - climb} is planned at

{point}

4. NOT (an oblique stroke followed by the speed to
   be maintained during cruise climb followed by

{the level above which cruise climb is planned

   followed by PLUS} is associated with {point} )
5. NOT (an oblique stroke followed by the speed
   to be maintained during cruise climb followed
   by {the two levels defining the layer to be
   occupied during cruide climb} is associated with

{point} )

1. report
   error

--Test Frame 1.18:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. NOT ATS flight track points are required by the
      appropriate ATS authority
   3. NOT (insert {Item 15 C} - { {point} details} )
   4. NOT ( {point} and {next {point} } are normally
      more than {30 minutes flying time} apart)
   5. A change of {track} is planned at {point}

                                                          1. report
                                                             error

--Test Frame 1.19:
 ROIDs: I19ES6
 Stimuli Response
   1. There are remarks
   2. NOT (indicate {Item 19 N} - {any other survival
      equipment carried and any other remarks
      regarding survival equipment} )

                                                          1. report
                                                             error

--Test Frame 1.20:
 ROIDs: I19ES6
 Stimuli Response
   1. NOT There are remarks
   2. NOT (cross out {Item 19 N} - {N} )

                                                          1. report
                                                             error

--Test Frame 1.21:
 ROIDs: I19ES2
 Stimuli Response
   1. NOT Jungle equipment is carried
   2. NOT (cross out {Item 19 S} - {J} )

                                                          1. report
                                                             error

--Test Frame 1.22:
 ROIDs: I19ES2
 Stimuli Response
   1. NOT Maritime equipment is carried
   2. NOT (cross out {Item 19 S} - {M} )

                                                          1. report
                                                             error

--Test Frame 1.23:
 ROIDs: I19ES2
 Stimuli Response
   1. NOT Desert equipment is carried
   2. NOT (cross out {Item 19 S} - {D} )

                                                          1. report
                                                             error

--Test Frame 1.24:
 ROIDs: I19ES2
 Stimuli Response
   1. NOT Polar equipment is carried
   2. NOT (cross out {Item 19 S} - {P} )

                                                          1. report
                                                             error

--Test Frame 1.25:
 ROIDs: I19ES1
 Stimuli Response
   1. NOT Emergency location beacon is available
   2. NOT (cross out {Item 19 R} - {E} )

                                                          1. report
                                                             error

--Test Frame 1.26:
 ROIDs: I18-9
 Stimuli Response
   1. Any other plain lanugage remarks are necessary
   2. NOT (insert {Item 18} - {RMK/any other remarks}
      )

                                                          1. report
                                                             error

--Test Frame 1.27:
 ROIDs: I18-8
 Stimuli Response
   1. {aerodrome} is an en-route alternate aerodrome
   2. NOT (insert {Item 18} - {RALT/ {aerodrome} } )

                                                          1. report
                                                             error

--Test Frame 1.28:
 ROIDs: I18-7
 Stimuli Response
   1. Aircraft performance data is prescribed by the
      appropriate ATS authority
   2. NOT (insert {Item 18} - {PER/Aircraft
      performance data} )

                                                          1. report
                                                             error

--Test Frame 1.29:
 ROIDs: I18-6
 Stimuli Response
   1. There is a reason for special handling
   2. NOT (insert {Item 18} - {STS/reason for special
      handling} )

                                                          1. report
                                                             error

--Test Frame 1.30:
 ROIDs: I18-5
 Stimuli Response
   1. NOT The name of the operator is obvious from the
      aircraft identification in Item 7
   2. NOT (insert {Item 18} - {OPR/operator name} )

                                                          1. report
                                                             error

--Test Frame 1.31:
 ROIDs: I18-4
 Stimuli Response
   1. A SELCAL Code is prescribed by the appropriate
      ATS authority
   2. NOT (insert {Item 18} - {SEL/SELCAL Code} )

                                                          1. report
                                                             error

--Test Frame 1.32:
 ROIDs: I18-3
 Stimuli Response
   1. The registration markings of the aircraft are
      different from the aircraft identification in
      Item 7
   2. NOT (insert {Item 18} - {REG/registration
      markings of the aircraft} )

                                                          1. report
                                                             error

--Test Frame 1.33:
 ROIDs: I18-2
 Stimuli Response
   1. The route is revised
   2. NOT (insert {Item 18} - {RIF/route details to
      the revised destination aerodrome followed by
      the ICAO four letter location indicator of the
      aerodrome} )

                                                          1. report
                                                             error

--Test Frame 1.34:
 ROIDs: I15B
 Stimuli Response
   1. Flight is uncontrolled VFR
   2. NOT (insert {Item 15 B} - {VFR} )

                                                          1. report
                                                             error

--Test Frame 1.35:
 ROIDs: I15A
 Stimuli Response
   1. Mach number is prescribed by the appropriate ATS
      authority
   2. NOT (insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} } )

                                                          1. report
                                                             error

--Test Frame 1.36:
 ROIDs: I13
 Stimuli Response
   1. The flight plan was submitted before departure
   2. NOT (insert {Item 13 B} - {the estimated
      off-block time} )

                                                          1. report
                                                             error

--Test Frame 1.37:
 ROIDs: I10SE
 Stimuli Response
   1. ADS capability
   2. NOT (insert {Item 10 SE} - {D} )

                                                          1. report
                                                             error

--Test Frame 1.38:
 ROIDs: I10SE
 Stimuli Response
   1. SSR transponder mode S including
      pressure-altitude and aicraft identification
      trasmission
   2. NOT (insert {Item 10 SE} - {S} )

                                                          1. report
                                                             error

--Test Frame 1.39:
 ROIDs: I10SE
 Stimuli Response
   1. SSR transponder mode S including aircraft
      identification trasmission
   2. NOT (insert {Item 10 SE} - {I} )

                                                          1. report
                                                             error

--Test Frame 1.40:
 ROIDs: I10SE
 Stimuli Response
   1. SSR transponder mode S including
      pressure-altitude trasmission
   2. NOT (insert {Item 10 SE} - {P} )

                                                          1. report
                                                             error

--Test Frame 1.41:
 ROIDs: I10SE
 Stimuli Response
   1. SSR transponder mode S only
   2. NOT (insert {Item 10 SE} - {X} )

                                                          1. report
                                                             error

--Test Frame 1.42:
 ROIDs: I10SE
 Stimuli Response
   1. SSR transponder mode A and mode C
   2. NOT (insert {Item 10 SE} - {C} )

                                                          1. report
                                                             error

--Test Frame 1.43:
 ROIDs: I10SE
 Stimuli Response
   1. SSR transponder mode A
   2. NOT (insert {Item 10 SE} - {A} )

                                                          1. report
                                                             error

--Test Frame 1.44:
 ROIDs: I10SE
 Stimuli Response
   1. NOT SSR equipment is present
   2. NOT (insert {Item 10 SE} - {N} )

                                                          1. report
                                                             error

--Test Frame 1.45:
 ROIDs: I9W
 Stimuli Response
   1. The maximum certified take-off mass is {7000} kg
      or less
   2. NOT (insert {Item 9 Wake Turnulence} - {/L} )

                                                          1. report
                                                             error

--Test Frame 1.46:
 ROIDs: I9W
 Stimuli Response
   1. The maximum certified take-off mass is less than

{136000} kg but more than {7000} kg

   2. NOT (insert {Item 9 Wake Turnulence} - {/M} )

                                                          1. report
                                                             error

--Test Frame 1.47:
 ROIDs: I9W
 Stimuli Response
   1. The maximum certified take-off mass is {136000}
      kg or more
   2. NOT (insert {Item 9 Wake Turnulence} - {/H} )

                                                          1. report
                                                             error

--Test Frame 1.48:
 ROIDs: I9N
 Stimuli Response
   1. There is more than one aircraft
   2. NOT (insert {Item 9 Number of Aircraft} - {the
      number of aircraft} )

                                                          1. report
                                                             error

--Test Frame 1.49:
 ROIDs: I8FT
 Stimuli Response
   1. Scheduled Air Service
   2. NOT (insert {Item 8 Type of Flight} - {S} )

                                                          1. report
                                                             error

--Test Frame 1.50:
 ROIDs: I8FR
 Stimuli Response
   1. VFR first
   2. NOT (insert {Item 8 Flight Rules} - {Z} )

                                                          1. report
                                                             error

--Test Frame 1.51:
 ROIDs: I8FR
 Stimuli Response
   1. IFR first
   2. NOT (insert {Item 8 Flight Rules} - {Y} )

                                                          1. report
                                                             error

--Test Frame 1.52:
 ROIDs: I8FR
 Stimuli Response
   1. VFR rules
   2. NOT (insert {Item 8 Flight Rules} - {V} )

                                                          1. report
                                                             error

--Test Frame 1.53:
 ROIDs: I8FR
 Stimuli Response
   1. IFR rules
   2. NOT (insert {Item 8 Flight Rules} - {I} )

                                                          1. report
                                                             error

--Test Frame 1.54:
 ROIDs: I7B
 Stimuli Response
   1. The radiotelephony call sign to be used by the
      aircraft will consist of {the ICAO telephony
      designator for the operating agency followed by
      the flight identification}
   2. NOT (insert {Item 7} - {the ICAO telephony
      designator for the operating agency followed
      by the flight identification} )

                                                          1. report
                                                             error

--Test Frame 1.55:
 ROIDs: I19ES4
 Stimuli Response
   1. NOT (cross out {Item 19 D} - {C} )
   2. NOT Dinghies are covered

                                                          1. report
                                                             error

--Test Frame 1.56:
 ROIDs: I19ES4
 Stimuli Response
   1. NOT Dinghies are carried
   2. NOT (cross out {Item 19 D} - {D} )

                                                          1. report
                                                             error

--Test Frame 1.57:
 ROIDs: I19ES3
 Stimuli Response
   1. NOT (cross out {Item 19 J} - {L} )
   2. NOT Life jackets are equipped with lights

                                                          1. report
                                                             error

--Test Frame 1.58:
 ROIDs: I19ES3
 Stimuli Response
   1. NOT (cross out {Item 19 J} - {F } )
   2. NOT Life jackets are equipped with fluorescein

                                                          1. report
                                                             error

--Test Frame 1.59:
 ROIDs: I16-2
 Stimuli Response
   1. NOT Location indicator has been assigned to the
      alternate aerodrome
   2. NOT (insert {Item 18} - {ALTN/ the name of the
      alternate aerodrome} )

                                                          1. report
                                                             error

--Test Frame 1.60:
 ROIDs: I16-1
 Stimuli Response
   1. Location indicator has been assigned
   2. NOT (insert {Item 16 Dest} - {the ICAO four
      letter location indicator of the destination
      aerodrome followed by the total estimated
      elapsed time} )

                                                          1. report
                                                             error

--Test Frame 1.61:
 ROIDs: I13
 Stimuli Response
   1. The flight plan is received from an aircraft in
      flight
   2. NOT (insert {Item 18} - {DEP/ the four-letter
      location indicator of the location of the ATS
      unit from which supplementary flight data can be
      obtained} )

                                                          1. report
                                                             error

--Test Frame 1.62:
 ROIDs: I19ES4
 Stimuli Response
   1. Dinghies are carried
   2. NOT (insert {Item 19 D} - {colour of dinghies} )

                                                          1. report
                                                             error

--Test Frame 1.63:
 ROIDs: I19ES3
 Stimuli Response
   1. cross out {Item 19 R} - {U}
   2. NOT (cross out {Item 19 J} - {U} )

                                                          1. report
                                                             error

--Test Frame 1.64:
 ROIDs: I19ES3
 Stimuli Response
   1. cross out {Item 19 R} - {V}
   2. NOT (cross out {Item 19 J} - {V} )

                                                          1. report
                                                             error

--Test Frame 1.65:
 ROIDs: I19ES1
 Stimuli Response
   1. NOT UHF on frequency 243.0 MHz is available
   2. NOT (cross out {Item 19 R} - {U} )

                                                          1. report
                                                             error

--Test Frame 1.66:
 ROIDs: I19P
 Stimuli Response
   1. Number of persons is required by the ATS
      authority
   2. NOT The total number of persons is known
   3. NOT (insert {Item 19 P} - {TBN} )

                                                          1. report
                                                             error

--Test Frame 1.67:
 ROIDs: I9T
 Stimuli Response
   1. This is a formation flight with more than one
      type
   2. NOT (insert {Item 18} - {TYP/ Types of aircraft
      preceded by numbers of aircraft} )

                                                          1. report
                                                             error

--Test Frame 1.68:
 ROIDs: I9T
 Stimuli Response
   1. NOT There is an appropriate ICAO type designator
   2. NOT (insert {Item 9 Type of Aircraft} - {ZZZZ} )

                                                          1. report
                                                             error

--Test Frame 1.69:
 ROIDs: I7A
 Stimuli Response
   1. The radiotelephony call sign to be used by the
      aircraft will consist of {the registration
      marking of the aircraft preceeded by the ICAO
      telephony designator for the aircraft operating
      agency}
   2. NOT (insert {Item 7} - {the registration marking
      of the aircraft} )

                                                          1. report
                                                             error

--Test Frame 1.70:
 ROIDs: I18-1
 Stimuli Response
   1. {point} is a {FIR boundary} prescribed {by the
      approapriate ATS authority}
   2. NOT (insert {Item 18} - {EET/ {point} } )

                                                          1. report
                                                             error

--Test Frame 1.71:
 ROIDs: I16-1
 Stimuli Response
   1. NOT Location indicator has been assigned
   2. NOT (insert {Item 18} - {DEST/ the name of the
      aerodrome} )

                                                          1. report
                                                             error

--Test Frame 1.72:
 ROIDs: I8FT
 Stimuli Response
   1. Non-scheduled Air Transport Operation
   2. NOT (insert {Item 8 Type of Flight} - {N} )

                                                          1. report
                                                             error

--Test Frame 1.73:
 ROIDs: I8FT
 Stimuli Response
   1. General Aviation
   2. NOT (insert {Item 8 Type of Flight} - {G} )

                                                          1. report
                                                             error

--Test Frame 1.74:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS route
   2. The departure aerodrome is {connected to} the
      ATS route
   3. NOT (insert {Item 15 C} - {the designator of the
      first ATS route} )

                                                          1. report
                                                             error

--Test Frame 1.75:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. NOT (insert {Item 10 CNA} - {S} )

                                                          1. report
                                                             error

--Test Frame 1.76:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. {point} is listed in Item 15 C
   3. A significant point code designator has been
      assigned to {point}
   4. NOT (the 2 to 5 characters of the assigned coded
      designator is associated with {point} )

                                                          1. report
                                                             error

--Test Frame 1.77:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS route
   2. A change of {level} is planned at {point}
   3. NOT (The flight to the {next {point} } will be
      outside a designated route)
   4. NOT (insert {Item 15 C} - { {point} followed by
      the designator of the next ATS route segment} )

                                                          1. report
                                                             error

--Test Frame 1.78:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. {point} is listed in Item 15 C
   3. NOT (an oblique stroke and both the cruising
      speed and the cruising level is associated with

{point} )

   4. A change of {speed - 0.01 Mach or more} is
      planned at {point}

                                                          1. report
                                                             error

--Test Frame 1.79:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. NOT ATS flight track points are required by the
      appropriate ATS authority
   3. insert {Item 15 C} - { {point} details}
   4. {point} and {next {point} } are normally more
      than {370km} apart
   5. {point} and {next {point} } are normally more
      than {30 minutes flying time} apart

                                                          1. report
                                                             error

--Test Frame 1.80:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. ATS flight track points are required by the
      appropriate ATS authority
   3. {point} and {point B} are successive points
   4. NOT (insert {Item 15 C} - {DCT between {point}
      and {point B} } )
   5. {point B} is defined by {goegraphical
      co-ordinates}
   6. {point} is defined by {goegraphical
      co-ordinates}

                                                          1. report
                                                             error

--Test Frame 1.81:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. ATS flight track points are required by the
      appropriate ATS authority
   3. {point} and {point B} are successive points
   4. NOT (insert {Item 15 C} - { {point} followed by

{point B} } )

   5. NOT ( {point} is defined by {goegraphical
      co-ordinates} )

                                                          1. report
                                                             error

--Test Frame 1.82:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. A change of {flight rules} is planned at {point}
   3. {point} is listed in Item 15 C
   4. IFR to VFR
   5. NOT (the letters VFR are associated with {point}
      )

                                                          1. report
                                                             error

--Test Frame 1.83:
 ROIDs: I19ES7
 Stimuli Response
   1. NOT (insert {Item 19 C} - {name of pilot in
      command} )

                                                          1. report
                                                             error

--Test Frame 1.84:
 ROIDs: I19ES5
 Stimuli Response
   1. NOT (insert {Item 19 A} - {colour of aircraft
      and significant markings} )

                                                          1. report
                                                             error

--Test Frame 1.85:
 ROIDs: I19E
 Stimuli Response
   1. NOT (insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes} )

                                                          1. report
                                                             error

--Test Frame 1.86:
 ROIDs: I16-2
 Stimuli Response
   1. NOT Location indicator has been assigned to the
      alternate aerodrome
   2. NOT (insert {Item 16 Alt} - {ZZZZ} )

                                                          1. report
                                                             error

--Test Frame 1.87:
 ROIDs: I13
 Stimuli Response
   1. The flight plan is received from an aircraft in
      flight
   2. NOT (insert {Item 13 A} - {AFIL} )

                                                          1. report
                                                             error

--Test Frame 1.88:
 ROIDs: I19ES4
 Stimuli Response
   1. Dinghies are carried
   2. NOT (insert {Item 19 D} - {total capacity in
      persons of all dinghies carried} )

                                                          1. report
                                                             error

--Test Frame 1.89:
 ROIDs: I19ES4
 Stimuli Response
   1. Dinghies are carried
   2. NOT (insert {Item 19 D} - {number of dinghies
      carried} )

                                                          1. report
                                                             error

--Test Frame 1.90:
 ROIDs: I19ES1
 Stimuli Response
   1. NOT VHF on frequency 121.5 MHz is available
   2. NOT (cross out {Item 19 R} - {V} )

                                                          1. report
                                                             error

--Test Frame 1.91:
 ROIDs: I7A
 Stimuli Response
   1. The radiotelephony call sign to be used by
      the aircraft will consist of {the registration
      marking of the aircraft}
   2. NOT (insert {Item 7} - {the registration marking
      of the aircraft} )

                                                          1. report
                                                             error

--Test Frame 1.92:
 ROIDs: I7A
 Stimuli Response
   1. NOT The aircraft is equipped with radio
   2. NOT (insert {Item 7} - {the registration marking
      of the aircraft} )

                                                          1. report
                                                             error

--Test Frame 1.93:
 ROIDs: I19ES3
 Stimuli Response
   1. NOT (cross out {Item 19 R} - {U} )
   2. Life jackets are carried
   3. cross out {Item 19 J} - {U}

                                                          1. report
                                                             error

--Test Frame 1.94:
 ROIDs: I18-1
 Stimuli Response
   1. {point} is a {FIR boundary} prescribed {on the
      basis of regional air navigation agreements}
   2. NOT (insert {Item 18} - {EET/ {point} } )

                                                          1. report
                                                             error

--Test Frame 1.95:
 ROIDs: I18-1
 Stimuli Response
   1. {point} is a {significant point} prescribed {by
      the approapriate ATS authority}
   2. NOT (insert {Item 18} - {EET/ {point} } )

                                                          1. report
                                                             error

--Test Frame 1.96:
 ROIDs: I18-1
 Stimuli Response
   1. {point} is a {significant point} prescribed {on
      the basis of regional air navigation agreements}
   2. NOT (insert {Item 18} - {EET/ {point} } )

                                                          1. report
                                                             error

--Test Frame 1.97:
 ROIDs: I16-1
 Stimuli Response
   1. NOT Location indicator has been assigned
   2. NOT (insert {Item 16 Dest} - {ZZZZ followed by
      the total estimated elapsed time} )

                                                          1. report
                                                             error

--Test Frame 1.98:
 ROIDs: I19ES3
 Stimuli Response
   1. NOT Life jackets are carried
   2. NOT (cross out {Item 19 J} - {L} )

                                                          1. report
                                                             error

--Test Frame 1.99:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS route
   2. The departure aerodrome is {located on} the ATS
      route
   3. NOT (insert {Item 15 C} - {the designator of the
      first ATS route} )

                                                          1. report
                                                             error

--Test Frame 1.100:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. ATS flight track points are required by the
      appropriate ATS authority
   3. NOT Use ATS style track points

                                                          1. report
                                                             error

--Test Frame 1.101:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. {point} is listed in Item 15 C
   3. NOT (an oblique stroke and both the cruising
      speed and the cruising level is associated with

{point} )

4. A change of {speed - 5pc TAS or more} is planned
   at {point}

                                                       1. report
                                                          error

--Test Frame 1.102:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS route
   2. A change of {ATS route other than same direction
      lower/upper} is planned at {point}
   3. The flight to the {next {point} } will be
      outside a designated route
   4. NOT ( {next {point} } is defined by geological
      co-ordinates)
   5. NOT (insert {Item 15 C} - { {point} followed by
      DCT} )

                                                          1. report
                                                             error

--Test Frame 1.103:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. ATS flight track points are required by the
      appropriate ATS authority
   3. {point} and {point B} are successive points
   4. NOT (insert {Item 15 C} - { {point} followed by

{point B} } )

   5. NOT ( {point B} is defined by {goegraphical
      co-ordinates} )

                                                          1. report
                                                             error

--Test Frame 1.104:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. ATS flight track points are required by the
      appropriate ATS authority
   3. {point} and {point B} are successive points
   4. NOT ( {point} is defined by {bearing and
      distance} )
   5. NOT (insert {Item 15 C} - { {point} followed by

{point B} } )

1. report
   error

--Test Frame 1.105:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. ATS flight track points are required by the
      appropriate ATS authority
   3. {point} and {point B} are successive points
   4. NOT ( {point B} is defined by {bearing and
      distance} )
   5. NOT (insert {Item 15 C} - { {point} followed by

{point B} } )

                                                          1. report
                                                             error

--Test Frame 1.106:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. NOT ATS flight track points are required by the
      appropriate ATS authority
   3. NOT (insert {Item 15 C} - { {point} details} )
   4. NOT ( {point} and {next {point} } are normally
      more than {370km} apart)
   5. A change of {track} is planned at {point}

                                                          1. report
                                                             error

--Test Frame 1.107:
 ROIDs: I13 I16-1
 Stimuli Response
   1. NOT The flight plan is received from an aircraft
      in flight
   2. Location indicator has been assigned
   3. NOT (insert {Item 13 A} - {the ICAO four-letter
      location indicator of the departure aerodrome} )

                                                          1. report
                                                             error

--Test Frame 1.108:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. {W} is prescribed by ATS
   3. NOT (insert {Item 10 CNA} - {W} )

                                                          1. report
                                                             error

--Test Frame 1.109:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. {X} is prescribed by ATS
   3. NOT (insert {Item 10 CNA} - {X} )

                                                          1. report
                                                             error

--Test Frame 1.110:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. {Y} is prescribed by ATS
   3. NOT (insert {Item 10 CNA} - {Y} )

                                                          1. report
                                                             error

--Test Frame 1.111:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {VHF RTF}
   3. NOT (insert {Item 10 CNA} - {V} )

                                                          1. report
                                                             error

--Test Frame 1.112:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {UHF RTF}
   3. NOT (insert {Item 10 CNA} - {U} )

                                                          1. report
                                                             error

--Test Frame 1.113:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {TACAN}
   3. NOT (insert {Item 10 CNA} - {T } )

                                                          1. report
                                                             error

--Test Frame 1.114:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {RNP type
      certification}
   3. NOT (insert {Item 10 CNA} - {R} )

                                                          1. report
                                                             error

--Test Frame 1.115:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {VOR}
   3. NOT (insert {Item 10 CNA} - {O} )

                                                          1. report
                                                             error

--Test Frame 1.116:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {Omega}
   3. NOT (insert {Item 10 CNA} - {M} )

                                                          1. report
                                                             error

--Test Frame 1.117:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {ILS}
   3. NOT (insert {Item 10 CNA} - {L} )

                                                          1. report
                                                             error

--Test Frame 1.118:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {MLS}
   3. NOT (insert {Item 10 CNA} - {K} )

                                                          1. report
                                                             error

--Test Frame 1.119:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {Inertial
      Navigation}
   3. NOT (insert {Item 10 CNA} - {I} )

                                                          1. report
                                                             error

--Test Frame 1.120:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {HF RTF}
   3. NOT (insert {Item 10 CNA} - {H} )

                                                          1. report
                                                             error

--Test Frame 1.121:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {GNSS}
   3. NOT (insert {Item 10 CNA} - {G} )

                                                          1. report
                                                             error

--Test Frame 1.122:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {ADF}
   3. NOT (insert {Item 10 CNA} - {F } )

                                                          1. report
                                                             error

--Test Frame 1.123:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {DME}
   3. NOT (insert {Item 10 CNA} - {D} )

                                                          1. report
                                                             error

--Test Frame 1.124:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {LORAN C}
   3. NOT (insert {Item 10 CNA} - {C} )

                                                          1. report
                                                             error

--Test Frame 1.125:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {other}
   3. NOT (insert {Item 18} - {COM/ or NAV/} )

                                                          1. report
                                                             error

--Test Frame 1.126:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {Data Link}
   3. NOT (insert {Item 18} - {DAT/} )

                                                          1. report
                                                             error

--Test Frame 1.127:
 ROIDs: I13 I16-1
 Stimuli Response
   1. NOT The flight plan is received from an aircraft
      in flight
   2. NOT Location indicator has been assigned
   3. NOT (insert {Item 13} - {DEP/ aerodrome name} )

                                                          1. report
                                                             error

--Test Frame 1.128:
 ROIDs: I13 I16-1
 Stimuli Response
   1. NOT The flight plan is received from an aircraft
      in flight
   2. NOT Location indicator has been assigned
   3. NOT (insert {Item 13 A} - {ZZZZZ} )

                                                          1. report
                                                             error

--Test Frame 1.129:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable

   2. COM/NAV/approach aid equipment is {other}

   3. NOT (insert {Item 10 CNA} - {Z} )

                                                          1. report
                                                             error

--Test Frame 1.130:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable

   2. COM/NAV/approach aid equipment is {Data Link}

   3. NOT (insert {Item 10 CNA} - {J} )

                                                          1. report
                                                             error

E.3 Differentiated Test Frames

Computing the differentiated test frames in full detail is impractical. To reduce the time required to generate test frames, the differentiated test frames were produced by expanding portions of the specification and generating test frames for that portion.

Some of the differentiated test frames do not have any requirement identifiers (ROIDs) attached to them. This can occur when non-primitives form the base, or non-differentiating, portion of the test frame. Requirement identifiers attached to conditions that differentiate the test frame are not listed with the test frame. This is because only the base conditions are relevant for coverage purposes. Therefore, those test frames below that do not list any requirement identifiers can be eliminated. Such test frames are redundant since there is another test frame where a non-primitive in the base is expanded to its underlying primitives and this other test frame with list any attached requirement identifiers.

E.3.1 Aircraft Identification

--Test Frame 1.1:
 Stimuli Response
   1. NOT Supplementary Information is correct
   2. • insert {Item 7} - {the registration marking of
      the aircraft}
   3. • insert {Item 7} - {the ICAO telephony
      designator for the operating agency followed
      by the flight identification}
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct

                                                          1. report
                                                             error

--Test Frame 1.2:
 Stimuli Response
   1. NOT Other Information is correct
   2. • insert {Item 7} - {the registration marking of
      the aircraft}
   3. • insert {Item 7} - {the ICAO telephony
      designator for the operating agency followed
      by the flight identification}
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.3:
 Stimuli Response
   1. NOT Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   2. • insert {Item 7} - {the registration marking of
      the aircraft}
   3. • insert {Item 7} - {the ICAO telephony
      designator for the operating agency followed
      by the flight identification}
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Other Information is correct
  10. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.4:
 Stimuli Response
   1. NOT Route is correct
   2. • insert {Item 7} - {the registration marking of
      the aircraft}
   3. • insert {Item 7} - {the ICAO telephony
      designator for the operating agency followed
      by the flight identification}
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   9. • Other Information is correct
  10. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.5:
 Stimuli Response
   1. NOT Departure Aerodrome and time are correct
   2. • insert {Item 7} - {the registration marking of
      the aircraft}
   3. • insert {Item 7} - {the ICAO telephony
      designator for the operating agency followed
      by the flight identification}
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Route is correct
   8. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   9. • Other Information is correct
  10. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.6:
 Stimuli Response
   1. NOT Equipment is correct
   2. • insert {Item 7} - {the registration marking of
      the aircraft}
   3. • insert {Item 7} - {the ICAO telephony
      designator for the operating agency followed
      by the flight identification}
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Departure Aerodrome and time are correct
   7. • Route is correct
   8. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   9. • Other Information is correct
  10. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.7:
 Stimuli Response
   1. NOT Number and Type of Aircraft and Wake
      Turbulence Category is correct
   2. • insert {Item 7} - {the registration marking of
      the aircraft}
   3. • insert {Item 7} - {the ICAO telephony
      designator for the operating agency followed
      by the flight identification}
   4. • FlightRules and Type of Flight is correct
   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Route is correct
   8. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   9. • Other Information is correct
  10. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.8:
 Stimuli Response
   1. NOT FlightRules and Type of Flight is correct
   2. • insert {Item 7} - {the registration marking of
      the aircraft}
   3. • insert {Item 7} - {the ICAO telephony
      designator for the operating agency followed
      by the flight identification}
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Route is correct
   8. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   9. • Other Information is correct
  10. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.9:
 ROIDs: I7B
 Stimuli Response
   1. The radiotelephony call sign to be used by the
      aircraft will consist of {the ICAO telephony
      designator for the operating agency followed by
      the flight identification}
   2. NOT (insert {Item 7} - {the ICAO telephony
      designator for the operating agency followed
      by the flight identification} )
   3. • insert {Item 7} - {the registration marking of
      the aircraft}
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.10:
 ROIDs: I7A
 Stimuli Response
   1. The radiotelephony call sign to be used by the
      aircraft will consist of {the registration
      marking of the aircraft preceeded by the ICAO
      telephony designator for the aircraft operating
      agency}
   2. NOT (insert {Item 7} - {the registration marking
      of the aircraft} )
   3. • NOT (The radiotelephony call sign to be
      used by the aircraft will consist of {the
      registration marking of the aircraft} )
   4. • The aircraft is equipped with radio
   5. • insert {Item 7} - {the ICAO telephony
      designator for the operating agency followed
      by the flight identification}
   6. • FlightRules and Type of Flight is correct
   7. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   8. • Equipment is correct
   9. • Departure Aerodrome and time are correct
  10. • Route is correct
  11. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  12. • Other Information is correct
  13. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.11:
 ROIDs: I7A
 Stimuli Response
   1. The radiotelephony call sign to be used by
      the aircraft will consist of {the registration
      marking of the aircraft}
   2. NOT (insert {Item 7} - {the registration marking
      of the aircraft} )
   3. • NOT (The radiotelephony call sign to be
      used by the aircraft will consist of {the
      registration marking of the aircraft preceeded
      by the ICAO telephony designator for the
      aircraft operating agency} )
   4. • The aircraft is equipped with radio
   5. • insert {Item 7} - {the ICAO telephony
      designator for the operating agency followed
      by the flight identification}
   6. • FlightRules and Type of Flight is correct
   7. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   8. • Equipment is correct
   9. • Departure Aerodrome and time are correct
  10. • Route is correct
  11. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  12. • Other Information is correct
  13. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.12:
 ROIDs: I7A
 Stimuli Response
   1. NOT The aircraft is equipped with radio
   2. NOT (insert {Item 7} - {the registration marking
      of the aircraft} )
   3. • NOT (The radiotelephony call sign to be
      used by the aircraft will consist of {the
      registration marking of the aircraft preceeded
      by the ICAO telephony designator for the
      aircraft operating agency} )
   4. • NOT (The radiotelephony call sign to be
      used by the aircraft will consist of {the
      registration marking of the aircraft} )
   5. • insert {Item 7} - {the ICAO telephony
      designator for the operating agency followed
      by the flight identification}
   6. • FlightRules and Type of Flight is correct
   7. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   8. • Equipment is correct
   9. • Departure Aerodrome and time are correct
  10. • Route is correct
  11. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  12. • Other Information is correct
  13. • Supplementary Information is correct

                                                          1. report
                                                             error

E.3.2 FlightRules and Type of Flight

--Test Frame 1.1:
 Stimuli Response
   1. NOT Supplementary Information is correct
   2. • Aircraft Identification is correct
   3. • insert {Item 8 Flight Rules} - {I}
   4. • insert {Item 8 Flight Rules} - {V}
   5. • insert {Item 8 Flight Rules} - {Y}
   6. • insert {Item 8 Flight Rules} - {Z}
   7. • Scheduled Air Service
   8. • insert {Item 8 Type of Flight} - {S}
   9. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
  10. • Equipment is correct
  11. • Departure Aerodrome and time are correct
  12. • Route is correct
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct

                                                          1. report
                                                             error

--Test Frame 1.2:
 Stimuli Response
   1. NOT Other Information is correct
   2. • Aircraft Identification is correct
   3. • insert {Item 8 Flight Rules} - {I}
   4. • insert {Item 8 Flight Rules} - {V}
   5. • insert {Item 8 Flight Rules} - {Y}
   6. • insert {Item 8 Flight Rules} - {Z}
   7. • Scheduled Air Service
   8. • insert {Item 8 Type of Flight} - {S}
   9. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
  10. • Equipment is correct
  11. • Departure Aerodrome and time are correct
  12. • Route is correct
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.3:
 Stimuli Response
   1. NOT Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   2. • Aircraft Identification is correct
   3. • insert {Item 8 Flight Rules} - {I}
   4. • insert {Item 8 Flight Rules} - {V}
   5. • insert {Item 8 Flight Rules} - {Y}
   6. • insert {Item 8 Flight Rules} - {Z}
   7. • Scheduled Air Service
   8. • insert {Item 8 Type of Flight} - {S}
   9. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
  10. • Equipment is correct
  11. • Departure Aerodrome and time are correct
  12. • Route is correct
  13. • Other Information is correct
  14. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.4:
 Stimuli Response
   1. NOT Route is correct
   2. • Aircraft Identification is correct
   3. • insert {Item 8 Flight Rules} - {I}
   4. • insert {Item 8 Flight Rules} - {V}
   5. • insert {Item 8 Flight Rules} - {Y}
   6. • insert {Item 8 Flight Rules} - {Z}
   7. • Scheduled Air Service
   8. • insert {Item 8 Type of Flight} - {S}
   9. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
  10. • Equipment is correct
  11. • Departure Aerodrome and time are correct
  12. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  13. • Other Information is correct
  14. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.5:
 Stimuli Response
   1. NOT Departure Aerodrome and time are correct
   2. • Aircraft Identification is correct
   3. • insert {Item 8 Flight Rules} - {I}
   4. • insert {Item 8 Flight Rules} - {V}
   5. • insert {Item 8 Flight Rules} - {Y}
   6. • insert {Item 8 Flight Rules} - {Z}
   7. • Scheduled Air Service
   8. • insert {Item 8 Type of Flight} - {S}
   9. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
  10. • Equipment is correct
  11. • Route is correct
  12. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  13. • Other Information is correct
  14. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.6:
 Stimuli Response
   1. NOT Equipment is correct
   2. • Aircraft Identification is correct
   3. • insert {Item 8 Flight Rules} - {I}
   4. • insert {Item 8 Flight Rules} - {V}
   5. • insert {Item 8 Flight Rules} - {Y}
   6. • insert {Item 8 Flight Rules} - {Z}
   7. • Scheduled Air Service
   8. • insert {Item 8 Type of Flight} - {S}
   9. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
  10. • Departure Aerodrome and time are correct
  11. • Route is correct
  12. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  13. • Other Information is correct
  14. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.7:
 Stimuli Response
   1. NOT Number and Type of Aircraft and Wake
      Turbulence Category is correct
   2. • Aircraft Identification is correct
   3. • insert {Item 8 Flight Rules} - {I}
   4. • insert {Item 8 Flight Rules} - {V}
   5. • insert {Item 8 Flight Rules} - {Y}
   6. • insert {Item 8 Flight Rules} - {Z}
   7. • Scheduled Air Service
   8. • insert {Item 8 Type of Flight} - {S}
   9. • Equipment is correct
  10. • Departure Aerodrome and time are correct
  11. • Route is correct
  12. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  13. • Other Information is correct
  14. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.8:
 Stimuli Response
   1. NOT Aircraft Identification is correct
   2. • insert {Item 8 Flight Rules} - {I}
   3. • insert {Item 8 Flight Rules} - {V}
   4. • insert {Item 8 Flight Rules} - {Y}
   5. • insert {Item 8 Flight Rules} - {Z}
   6. • Scheduled Air Service
   7. • insert {Item 8 Type of Flight} - {S}
   8. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   9. • Equipment is correct
  10. • Departure Aerodrome and time are correct
  11. • Route is correct
  12. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  13. • Other Information is correct
  14. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.9:
 ROIDs: I8FT
 Stimuli Response
   1. Military
   2. NOT (insert {Item 8 Type of Flight} - {M} )
   3. • Aircraft Identification is correct
   4. • insert {Item 8 Flight Rules} - {I}
   5. • insert {Item 8 Flight Rules} - {V}
   6. • insert {Item 8 Flight Rules} - {Y}
   7. • insert {Item 8 Flight Rules} - {Z}
   8. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   9. • Equipment is correct
  10. • Departure Aerodrome and time are correct
  11. • Route is correct
  12. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  13. • Other Information is correct
  14. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.10:
 ROIDs: I8FT
 Stimuli Response
   1. NOT Scheduled Air Service
   2. NOT Non-scheduled Air Transport Operation
   3. NOT General Aviation
   4. NOT Military
   5. NOT (insert {Item 8 Type of Flight} - {X} )
   6. • Aircraft Identification is correct
   7. • insert {Item 8 Flight Rules} - {I}
   8. • insert {Item 8 Flight Rules} - {V}
   9. • insert {Item 8 Flight Rules} - {Y}
  10. • insert {Item 8 Flight Rules} - {Z}
  11. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
  12. • Equipment is correct
  13. • Departure Aerodrome and time are correct
  14. • Route is correct
  15. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  16. • Other Information is correct
  17. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.11:
 ROIDs: I8FT
 Stimuli Response
   1. Scheduled Air Service
   2. NOT (insert {Item 8 Type of Flight} - {S} )
   3. • Aircraft Identification is correct
   4. • insert {Item 8 Flight Rules} - {I}
   5. • insert {Item 8 Flight Rules} - {V}
   6. • insert {Item 8 Flight Rules} - {Y}
   7. • insert {Item 8 Flight Rules} - {Z}
   8. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   9. • Equipment is correct
  10. • Departure Aerodrome and time are correct
  11. • Route is correct
  12. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  13. • Other Information is correct
  14. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.12:
 ROIDs: I8FR
 Stimuli Response
   1. VFR first
   2. NOT (insert {Item 8 Flight Rules} - {Z} )
   3. • Aircraft Identification is correct
   4. • insert {Item 8 Flight Rules} - {I}
   5. • insert {Item 8 Flight Rules} - {V}
   6. • insert {Item 8 Flight Rules} - {Y}
   7. • Scheduled Air Service
   8. • insert {Item 8 Type of Flight} - {S}
   9. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
  10. • Equipment is correct
  11. • Departure Aerodrome and time are correct
  12. • Route is correct
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.13:
 ROIDs: I8FR
 Stimuli Response
   1. IFR first
   2. NOT (insert {Item 8 Flight Rules} - {Y} )
   3. • Aircraft Identification is correct
   4. • insert {Item 8 Flight Rules} - {I}
   5. • insert {Item 8 Flight Rules} - {V}
   6. • insert {Item 8 Flight Rules} - {Z}
   7. • Scheduled Air Service
   8. • insert {Item 8 Type of Flight} - {S}
   9. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
  10. • Equipment is correct
  11. • Departure Aerodrome and time are correct
  12. • Route is correct
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.14:
 ROIDs: I8FR
 Stimuli Response
   1. VFR rules
   2. NOT (insert {Item 8 Flight Rules} - {V} )
   3. • Aircraft Identification is correct
   4. • insert {Item 8 Flight Rules} - {I}
   5. • insert {Item 8 Flight Rules} - {Y}
   6. • insert {Item 8 Flight Rules} - {Z}
   7. • Scheduled Air Service
   8. • insert {Item 8 Type of Flight} - {S}
   9. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
  10. • Equipment is correct
  11. • Departure Aerodrome and time are correct
  12. • Route is correct
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.15:
 ROIDs: I8FR
 Stimuli Response
   1. IFR rules
   2. NOT (insert {Item 8 Flight Rules} - {I} )
   3. • Aircraft Identification is correct
   4. • insert {Item 8 Flight Rules} - {V}
   5. • insert {Item 8 Flight Rules} - {Y}
   6. • insert {Item 8 Flight Rules} - {Z}
   7. • Scheduled Air Service
   8. • insert {Item 8 Type of Flight} - {S}
   9. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
  10. • Equipment is correct
  11. • Departure Aerodrome and time are correct
  12. • Route is correct
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.16:
 ROIDs: I8FT
 Stimuli Response
   1. Non-scheduled Air Transport Operation
   2. NOT (insert {Item 8 Type of Flight} - {N} )
   3. • Aircraft Identification is correct
   4. • insert {Item 8 Flight Rules} - {I}
   5. • insert {Item 8 Flight Rules} - {V}
   6. • insert {Item 8 Flight Rules} - {Y}
   7. • insert {Item 8 Flight Rules} - {Z}
   8. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   9. • Equipment is correct
  10. • Departure Aerodrome and time are correct
  11. • Route is correct
  12. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  13. • Other Information is correct
  14. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.17:
 ROIDs: I8FT
 Stimuli Response
   1. General Aviation
   2. NOT (insert {Item 8 Type of Flight} - {G} )
   3. • Aircraft Identification is correct
   4. • insert {Item 8 Flight Rules} - {I}
   5. • insert {Item 8 Flight Rules} - {V}
   6. • insert {Item 8 Flight Rules} - {Y}
   7. • insert {Item 8 Flight Rules} - {Z}
   8. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   9. • Equipment is correct
  10. • Departure Aerodrome and time are correct
  11. • Route is correct
  12. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  13. • Other Information is correct
  14. • Supplementary Information is correct

                                                          1. report
                                                             error

E.3.3 Number and Type of Aircraft and Wake Turbulence Category

--Test Frame 1.1:
 Stimuli Response
   1. NOT Supplementary Information is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • insert {Item 9 Number of Aircraft} - {the
      number of aircraft}
   5. • There is an appropriate ICAO type designator
   6. • This is a formation flight with more than one
      type
   7. • insert {Item 18} - {TYP/ Types of aircraft
      preceded by numbers of aircraft}
   8. • insert {Item 9 Wake Turnulence} - {/H}
   9. • insert {Item 9 Wake Turnulence} - {/M}
  10. • insert {Item 9 Wake Turnulence} - {/L}
  11. • Equipment is correct
  12. • Departure Aerodrome and time are correct
  13. • Route is correct
  14. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  15. • Other Information is correct

                                                          1. report
                                                             error

--Test Frame 1.2:
 Stimuli Response
   1. NOT Other Information is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • insert {Item 9 Number of Aircraft} - {the
      number of aircraft}
   5. • There is an appropriate ICAO type designator
   6. • This is a formation flight with more than one
      type
   7. • insert {Item 18} - {TYP/ Types of aircraft
      preceded by numbers of aircraft}
   8. • insert {Item 9 Wake Turnulence} - {/H}
   9. • insert {Item 9 Wake Turnulence} - {/M}
  10. • insert {Item 9 Wake Turnulence} - {/L}
  11. • Equipment is correct
  12. • Departure Aerodrome and time are correct
  13. • Route is correct
  14. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  15. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.3:
 Stimuli Response
   1. NOT Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • insert {Item 9 Number of Aircraft} - {the
      number of aircraft}
   5. • There is an appropriate ICAO type designator
   6. • This is a formation flight with more than one
      type
   7. • insert {Item 18} - {TYP/ Types of aircraft
      preceded by numbers of aircraft}
   8. • insert {Item 9 Wake Turnulence} - {/H}
   9. • insert {Item 9 Wake Turnulence} - {/M}
  10. • insert {Item 9 Wake Turnulence} - {/L}
  11. • Equipment is correct
  12. • Departure Aerodrome and time are correct
  13. • Route is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.4:
 Stimuli Response
   1. NOT Route is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • insert {Item 9 Number of Aircraft} - {the
      number of aircraft}
   5. • There is an appropriate ICAO type designator
   6. • This is a formation flight with more than one
      type
   7. • insert {Item 18} - {TYP/ Types of aircraft
      preceded by numbers of aircraft}
   8. • insert {Item 9 Wake Turnulence} - {/H}
   9. • insert {Item 9 Wake Turnulence} - {/M}
  10. • insert {Item 9 Wake Turnulence} - {/L}
  11. • Equipment is correct
  12. • Departure Aerodrome and time are correct
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.5:
 Stimuli Response
   1. NOT Departure Aerodrome and time are correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • insert {Item 9 Number of Aircraft} - {the
      number of aircraft}
   5. • There is an appropriate ICAO type designator
   6. • This is a formation flight with more than one
      type
   7. • insert {Item 18} - {TYP/ Types of aircraft
      preceded by numbers of aircraft}
   8. • insert {Item 9 Wake Turnulence} - {/H}
   9. • insert {Item 9 Wake Turnulence} - {/M}
  10. • insert {Item 9 Wake Turnulence} - {/L}
  11. • Equipment is correct
  12. • Route is correct
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.6:
 Stimuli Response
   1. NOT Equipment is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • insert {Item 9 Number of Aircraft} - {the
      number of aircraft}
   5. • There is an appropriate ICAO type designator
   6. • This is a formation flight with more than one
      type
   7. • insert {Item 18} - {TYP/ Types of aircraft
      preceded by numbers of aircraft}
   8. • insert {Item 9 Wake Turnulence} - {/H}
   9. • insert {Item 9 Wake Turnulence} - {/M}
  10. • insert {Item 9 Wake Turnulence} - {/L}
  11. • Departure Aerodrome and time are correct
  12. • Route is correct
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.7:
 Stimuli Response
   1. NOT FlightRules and Type of Flight is correct
   2. • Aircraft Identification is correct
   3. • insert {Item 9 Number of Aircraft} - {the
      number of aircraft}
   4. • There is an appropriate ICAO type designator
   5. • This is a formation flight with more than one
      type
   6. • insert {Item 18} - {TYP/ Types of aircraft
      preceded by numbers of aircraft}
   7. • insert {Item 9 Wake Turnulence} - {/H}
   8. • insert {Item 9 Wake Turnulence} - {/M}
   9. • insert {Item 9 Wake Turnulence} - {/L}
  10. • Equipment is correct
  11. • Departure Aerodrome and time are correct
  12. • Route is correct
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.8:
 Stimuli Response
   1. NOT Aircraft Identification is correct
   2. • FlightRules and Type of Flight is correct
   3. • insert {Item 9 Number of Aircraft} - {the
      number of aircraft}
   4. • There is an appropriate ICAO type designator
   5. • This is a formation flight with more than one
      type
   6. • insert {Item 18} - {TYP/ Types of aircraft
      preceded by numbers of aircraft}
   7. • insert {Item 9 Wake Turnulence} - {/H}
   8. • insert {Item 9 Wake Turnulence} - {/M}
   9. • insert {Item 9 Wake Turnulence} - {/L}
  10. • Equipment is correct
  11. • Departure Aerodrome and time are correct
  12. • Route is correct
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.9:
 ROIDs: I9T
 Stimuli Response
   1. There is an appropriate ICAO type designator
   2. NOT This is a formation flight with more than
      one type
   3. NOT (insert {Item 9 Type of Aircraft} - {the
      appropriate ICAO type designator} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • insert {Item 9 Number of Aircraft} - {the
      number of aircraft}
   7. • insert {Item 9 Wake Turnulence} - {/H}
   8. • insert {Item 9 Wake Turnulence} - {/M}
   9. • insert {Item 9 Wake Turnulence} - {/L}
  10. • Equipment is correct
  11. • Departure Aerodrome and time are correct
  12. • Route is correct
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.10:
 ROIDs: I9W
 Stimuli Response
   1. The maximum certified take-off mass is {7000} kg
      or less
   2. NOT (insert {Item 9 Wake Turnulence} - {/L} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • insert {Item 9 Number of Aircraft} - {the
      number of aircraft}
   6. • There is an appropriate ICAO type designator
   7. • This is a formation flight with more than one
      type
   8. • insert {Item 18} - {TYP/ Types of aircraft
      preceded by numbers of aircraft}
   9. • insert {Item 9 Wake Turnulence} - {/H}
  10. • insert {Item 9 Wake Turnulence} - {/M}
  11. • Equipment is correct
  12. • Departure Aerodrome and time are correct
  13. • Route is correct
  14. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  15. • Other Information is correct
  16. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.11:
 ROIDs: I9W
 Stimuli Response
   1. The maximum certified take-off mass is less than

{136000} kg but more than {7000} kg

 2. NOT (insert {Item 9 Wake Turnulence} - {/M} )
 3. • Aircraft Identification is correct
 4. • FlightRules and Type of Flight is correct
 5. • insert {Item 9 Number of Aircraft} - {the
    number of aircraft}
 6. • There is an appropriate ICAO type designator
 7. • This is a formation flight with more than one
    type
 8. • insert {Item 18} - {TYP/ Types of aircraft
    preceded by numbers of aircraft}
 9. • insert {Item 9 Wake Turnulence} - {/H}
10. • insert {Item 9 Wake Turnulence} - {/L}
11. • Equipment is correct
12. • Departure Aerodrome and time are correct
13. • Route is correct
14. • Destination Aerodrome and Total Estimated
    Elapsed Time is correct
15. • Other Information is correct
16. • Supplementary Information is correct

                                                        1. report
                                                           error

--Test Frame 1.12:
 ROIDs: I9W
 Stimuli Response
   1. The maximum certified take-off mass is {136000}
      kg or more
   2. NOT (insert {Item 9 Wake Turnulence} - {/H} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • insert {Item 9 Number of Aircraft} - {the
      number of aircraft}
   6. • There is an appropriate ICAO type designator
   7. • This is a formation flight with more than one
      type
   8. • insert {Item 18} - {TYP/ Types of aircraft
      preceded by numbers of aircraft}
   9. • insert {Item 9 Wake Turnulence} - {/M}
  10. • insert {Item 9 Wake Turnulence} - {/L}
  11. • Equipment is correct
  12. • Departure Aerodrome and time are correct
  13. • Route is correct
  14. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  15. • Other Information is correct
  16. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.13:
 ROIDs: I9N
 Stimuli Response
   1. There is more than one aircraft
   2. NOT (insert {Item 9 Number of Aircraft} - {the
      number of aircraft} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • There is an appropriate ICAO type designator
   6. • This is a formation flight with more than one
      type
   7. • insert {Item 18} - {TYP/ Types of aircraft
      preceded by numbers of aircraft}
   8. • insert {Item 9 Wake Turnulence} - {/H}
   9. • insert {Item 9 Wake Turnulence} - {/M}
  10. • insert {Item 9 Wake Turnulence} - {/L}
  11. • Equipment is correct
  12. • Departure Aerodrome and time are correct
  13. • Route is correct
  14. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  15. • Other Information is correct
  16. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.14:
 ROIDs: I9T
 Stimuli Response
   1. This is a formation flight with more than one
      type
   2. NOT (insert {Item 18} - {TYP/ Types of aircraft
      preceded by numbers of aircraft} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • insert {Item 9 Number of Aircraft} - {the
      number of aircraft}
   6. • There is an appropriate ICAO type designator
   7. • insert {Item 9 Wake Turnulence} - {/H}
   8. • insert {Item 9 Wake Turnulence} - {/M}
   9. • insert {Item 9 Wake Turnulence} - {/L}
  10. • Equipment is correct
  11. • Departure Aerodrome and time are correct
  12. • Route is correct
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.15:
 ROIDs: I9T
 Stimuli Response
   1. NOT There is an appropriate ICAO type designator
   2. NOT (insert {Item 9 Type of Aircraft} - {ZZZZ} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • insert {Item 9 Number of Aircraft} - {the
      number of aircraft}
   6. • insert {Item 18} - {TYP/ Types of aircraft
      preceded by numbers of aircraft}
   7. • insert {Item 9 Wake Turnulence} - {/H}
   8. • insert {Item 9 Wake Turnulence} - {/M}
   9. • insert {Item 9 Wake Turnulence} - {/L}
  10. • Equipment is correct
  11. • Departure Aerodrome and time are correct
  12. • Route is correct
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct

                                                          1. report
                                                             error

E.3.4 Equipment

--Test Frame 1.1:
 Stimuli Response
   1. NOT Supplementary Information is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • insert {Item 10 CNA} - {S}
   6. • insert {Item 10 CNA} - {C}
   7. • insert {Item 10 CNA} - {D}
   8. • insert {Item 10 CNA} - {G}
   9. • insert {Item 10 CNA} - {H}
  10. • insert {Item 10 CNA} - {I}
  11. • insert {Item 10 CNA} - {J}
  12. • insert {Item 18} - {DAT/}
  13. • insert {Item 10 CNA} - {K}
  14. • Equipment [Part 2] is correct
  15. • Equipment [Part E] is correct
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct

                                                          1. report
                                                             error

--Test Frame 1.2:
 Stimuli Response
   1. NOT Other Information is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • insert {Item 10 CNA} - {S}
   6. • insert {Item 10 CNA} - {C}
   7. • insert {Item 10 CNA} - {D}
   8. • insert {Item 10 CNA} - {G}
   9. • insert {Item 10 CNA} - {H}
  10. • insert {Item 10 CNA} - {I}
  11. • insert {Item 10 CNA} - {J}
  12. • insert {Item 18} - {DAT/}
  13. • insert {Item 10 CNA} - {K}
  14. • Equipment [Part 2] is correct
  15. • Equipment [Part E] is correct
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.3:
 Stimuli Response
   1. NOT Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • insert {Item 10 CNA} - {S}
   6. • insert {Item 10 CNA} - {C}
   7. • insert {Item 10 CNA} - {D}
   8. • insert {Item 10 CNA} - {G}
   9. • insert {Item 10 CNA} - {H}
  10. • insert {Item 10 CNA} - {I}
  11. • insert {Item 10 CNA} - {J}
  12. • insert {Item 18} - {DAT/}
  13. • insert {Item 10 CNA} - {K}
  14. • Equipment [Part 2] is correct
  15. • Equipment [Part E] is correct
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Other Information is correct
  19. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.4:
 Stimuli Response
   1. NOT Route is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • insert {Item 10 CNA} - {S}
   6. • insert {Item 10 CNA} - {C}
   7. • insert {Item 10 CNA} - {D}
   8. • insert {Item 10 CNA} - {G}
   9. • insert {Item 10 CNA} - {H}
  10. • insert {Item 10 CNA} - {I}
  11. • insert {Item 10 CNA} - {J}
  12. • insert {Item 18} - {DAT/}
  13. • insert {Item 10 CNA} - {K}
  14. • Equipment [Part 2] is correct
  15. • Equipment [Part E] is correct
  16. • Departure Aerodrome and time are correct
  17. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  18. • Other Information is correct
  19. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.5:
 Stimuli Response
   1. NOT Departure Aerodrome and time are correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • insert {Item 10 CNA} - {S}
   6. • insert {Item 10 CNA} - {C}
   7. • insert {Item 10 CNA} - {D}
   8. • insert {Item 10 CNA} - {G}
   9. • insert {Item 10 CNA} - {H}
  10. • insert {Item 10 CNA} - {I}
  11. • insert {Item 10 CNA} - {J}
  12. • insert {Item 18} - {DAT/}
  13. • insert {Item 10 CNA} - {K}
  14. • Equipment [Part 2] is correct
  15. • Equipment [Part E] is correct
  16. • Route is correct
  17. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  18. • Other Information is correct
  19. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.6:
 Stimuli Response
   1. NOT Equipment [Part E] is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • insert {Item 10 CNA} - {S}
   6. • insert {Item 10 CNA} - {C}
   7. • insert {Item 10 CNA} - {D}
   8. • insert {Item 10 CNA} - {G}
   9. • insert {Item 10 CNA} - {H}
  10. • insert {Item 10 CNA} - {I}
  11. • insert {Item 10 CNA} - {J}
  12. • insert {Item 18} - {DAT/}
  13. • insert {Item 10 CNA} - {K}
  14. • Equipment [Part 2] is correct
  15. • Departure Aerodrome and time are correct
  16. • Route is correct
  17. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  18. • Other Information is correct
  19. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.7:
 Stimuli Response
   1. NOT Number and Type of Aircraft and Wake
      Turbulence Category is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • insert {Item 10 CNA} - {S}
   5. • insert {Item 10 CNA} - {C}
   6. • insert {Item 10 CNA} - {D}
   7. • insert {Item 10 CNA} - {G}
   8. • insert {Item 10 CNA} - {H}
   9. • insert {Item 10 CNA} - {I}
  10. • insert {Item 10 CNA} - {J}
  11. • insert {Item 18} - {DAT/}
  12. • insert {Item 10 CNA} - {K}
  13. • Equipment [Part 2] is correct
  14. • Equipment [Part E] is correct
  15. • Departure Aerodrome and time are correct
  16. • Route is correct
  17. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  18. • Other Information is correct
  19. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.8:
 Stimuli Response
   1. NOT FlightRules and Type of Flight is correct
   2. • Aircraft Identification is correct
   3. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   4. • insert {Item 10 CNA} - {S}
   5. • insert {Item 10 CNA} - {C}
   6. • insert {Item 10 CNA} - {D}
   7. • insert {Item 10 CNA} - {G}
   8. • insert {Item 10 CNA} - {H}
   9. • insert {Item 10 CNA} - {I}
  10. • insert {Item 10 CNA} - {J}
  11. • insert {Item 18} - {DAT/}
  12. • insert {Item 10 CNA} - {K}
  13. • Equipment [Part 2] is correct
  14. • Equipment [Part E] is correct
  15. • Departure Aerodrome and time are correct
  16. • Route is correct
  17. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  18. • Other Information is correct
  19. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.9:
 Stimuli Response
   1. NOT Aircraft Identification is correct
   2. • FlightRules and Type of Flight is correct
   3. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   4. • insert {Item 10 CNA} - {S}
   5. • insert {Item 10 CNA} - {C}
   6. • insert {Item 10 CNA} - {D}
   7. • insert {Item 10 CNA} - {G}
   8. • insert {Item 10 CNA} - {H}
   9. • insert {Item 10 CNA} - {I}
  10. • insert {Item 10 CNA} - {J}
  11. • insert {Item 18} - {DAT/}
  12. • insert {Item 10 CNA} - {K}
  13. • Equipment [Part 2] is correct
  14. • Equipment [Part E] is correct
  15. • Departure Aerodrome and time are correct
  16. • Route is correct
  17. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  18. • Other Information is correct
  19. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.10:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. NOT Equipment [Part 2] is correct
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • insert {Item 10 CNA} - {S}
   7. • insert {Item 10 CNA} - {C}
   8. • insert {Item 10 CNA} - {D}
   9. • insert {Item 10 CNA} - {G}
  10. • insert {Item 10 CNA} - {H}
  11. • insert {Item 10 CNA} - {I}
  12. • insert {Item 10 CNA} - {J}
  13. • insert {Item 18} - {DAT/}
  14. • insert {Item 10 CNA} - {K}
  15. • Equipment [Part E] is correct
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.11:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. NOT (insert {Item 10 CNA} - {S} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • insert {Item 10 CNA} - {C}
   7. • insert {Item 10 CNA} - {D}
   8. • insert {Item 10 CNA} - {F }
   9. • insert {Item 10 CNA} - {G}
  10. • insert {Item 10 CNA} - {H}
  11. • insert {Item 10 CNA} - {I}
  12. • insert {Item 10 CNA} - {J}
  13. • insert {Item 18} - {DAT/}
  14. • insert {Item 10 CNA} - {K}
  15. • insert {Item 10 CNA} - {L}
  16. • Equipment [Part 2] is correct
  17. • Equipment [Part E] is correct
  18. • Departure Aerodrome and time are correct
  19. • Route is correct
  20. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  21. • Other Information is correct
  22. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.12:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {ILS}
   3. NOT (insert {Item 10 CNA} - {L} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • insert {Item 10 CNA} - {C}
   9. • insert {Item 10 CNA} - {D}
  10. • insert {Item 10 CNA} - {G}
  11. • insert {Item 10 CNA} - {H}
  12. • insert {Item 10 CNA} - {I}
  13. • insert {Item 10 CNA} - {J}
  14. • insert {Item 18} - {DAT/}
  15. • insert {Item 10 CNA} - {K}
  16. • Equipment [Part 2] is correct
  17. • Equipment [Part E] is correct
  18. • Departure Aerodrome and time are correct
  19. • Route is correct
  20. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  21. • Other Information is correct
  22. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.13:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {MLS}
   3. NOT (insert {Item 10 CNA} - {K} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • insert {Item 10 CNA} - {C}
   9. • insert {Item 10 CNA} - {D}
  10. • insert {Item 10 CNA} - {G}
  11. • insert {Item 10 CNA} - {H}
  12. • insert {Item 10 CNA} - {I}
  13. • insert {Item 10 CNA} - {J}
  14. • insert {Item 18} - {DAT/}
  15. • Equipment [Part 2] is correct
  16. • Equipment [Part E] is correct
  17. • Departure Aerodrome and time are correct
  18. • Route is correct
  19. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  20. • Other Information is correct
  21. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.14:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {Inertial
      Navigation}
   3. NOT (insert {Item 10 CNA} - {I} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • insert {Item 10 CNA} - {C}
   9. • insert {Item 10 CNA} - {D}
  10. • insert {Item 10 CNA} - {G}
  11. • insert {Item 10 CNA} - {H}
  12. • insert {Item 10 CNA} - {J}
  13. • insert {Item 18} - {DAT/}
  14. • insert {Item 10 CNA} - {K}
  15. • Equipment [Part 2] is correct
  16. • Equipment [Part E] is correct
  17. • Departure Aerodrome and time are correct
  18. • Route is correct
  19. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  20. • Other Information is correct
  21. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.15:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {HF RTF}
   3. NOT (insert {Item 10 CNA} - {H} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • insert {Item 10 CNA} - {C}
   9. • insert {Item 10 CNA} - {D}
  10. • insert {Item 10 CNA} - {G}
  11. • insert {Item 10 CNA} - {I}
  12. • insert {Item 10 CNA} - {J}
  13. • insert {Item 18} - {DAT/}
  14. • insert {Item 10 CNA} - {K}
  15. • Equipment [Part 2] is correct
  16. • Equipment [Part E] is correct
  17. • Departure Aerodrome and time are correct
  18. • Route is correct
  19. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  20. • Other Information is correct
  21. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.16:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {GNSS}
   3. NOT (insert {Item 10 CNA} - {G} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • insert {Item 10 CNA} - {C}
   9. • insert {Item 10 CNA} - {D}
  10. • insert {Item 10 CNA} - {H}
  11. • insert {Item 10 CNA} - {I}
  12. • insert {Item 10 CNA} - {J}
  13. • insert {Item 18} - {DAT/}
  14. • insert {Item 10 CNA} - {K}
  15. • Equipment [Part 2] is correct
  16. • Equipment [Part E] is correct
  17. • Departure Aerodrome and time are correct
  18. • Route is correct
  19. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  20. • Other Information is correct
  21. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.17:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {ADF}
   3. NOT (insert {Item 10 CNA} - {F } )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • insert {Item 10 CNA} - {C}
   9. • insert {Item 10 CNA} - {D}
  10. • insert {Item 10 CNA} - {G}
  11. • insert {Item 10 CNA} - {H}
  12. • insert {Item 10 CNA} - {I}
  13. • insert {Item 10 CNA} - {J}
  14. • insert {Item 18} - {DAT/}
  15. • insert {Item 10 CNA} - {K}
  16. • Equipment [Part 2] is correct
  17. • Equipment [Part E] is correct
  18. • Departure Aerodrome and time are correct
  19. • Route is correct
  20. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  21. • Other Information is correct
  22. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.18:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {DME}
   3. NOT (insert {Item 10 CNA} - {D} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • insert {Item 10 CNA} - {C}
   9. • insert {Item 10 CNA} - {G}
  10. • insert {Item 10 CNA} - {H}
  11. • insert {Item 10 CNA} - {I}
  12. • insert {Item 10 CNA} - {J}
  13. • insert {Item 18} - {DAT/}
  14. • insert {Item 10 CNA} - {K}
  15. • Equipment [Part 2] is correct
  16. • Equipment [Part E] is correct
  17. • Departure Aerodrome and time are correct
  18. • Route is correct
  19. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  20. • Other Information is correct
  21. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.19:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {LORAN C}
   3. NOT (insert {Item 10 CNA} - {C} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • insert {Item 10 CNA} - {D}
   9. • insert {Item 10 CNA} - {G}
  10. • insert {Item 10 CNA} - {H}
  11. • insert {Item 10 CNA} - {I}
  12. • insert {Item 10 CNA} - {J}
  13. • insert {Item 18} - {DAT/}
  14. • insert {Item 10 CNA} - {K}
  15. • Equipment [Part 2] is correct
  16. • Equipment [Part E] is correct
  17. • Departure Aerodrome and time are correct
  18. • Route is correct
  19. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  20. • Other Information is correct
  21. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.20:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {Data Link}
   3. NOT (insert {Item 18} - {DAT/} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • insert {Item 10 CNA} - {C}
   9. • insert {Item 10 CNA} - {D}
  10. • insert {Item 10 CNA} - {G}
  11. • insert {Item 10 CNA} - {H}
  12. • insert {Item 10 CNA} - {I}
  13. • insert {Item 10 CNA} - {J}
  14. • insert {Item 10 CNA} - {K}
  15. • Equipment [Part 2] is correct
  16. • Equipment [Part E] is correct
  17. • Departure Aerodrome and time are correct
  18. • Route is correct
  19. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  20. • Other Information is correct
  21. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.21:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {Data Link}
   3. NOT (insert {Item 10 CNA} - {J} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • insert {Item 10 CNA} - {C}
   9. • insert {Item 10 CNA} - {D}
  10. • insert {Item 10 CNA} - {G}
  11. • insert {Item 10 CNA} - {H}
  12. • insert {Item 10 CNA} - {I}
  13. • insert {Item 18} - {DAT/}
  14. • insert {Item 10 CNA} - {K}
  15. • Equipment [Part 2] is correct
  16. • Equipment [Part E] is correct
  17. • Departure Aerodrome and time are correct
  18. • Route is correct
  19. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  20. • Other Information is correct
  21. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.1:
 Stimuli Response
   1. NOT Supplementary Information is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • insert {Item 10 CNA} - {S}
   6. • Equipment [Part 1] is correct
   7. • insert {Item 10 CNA} - {M}
   8. • insert {Item 10 CNA} - {R}
   9. • insert {Item 10 CNA} - {T }
  10. • insert {Item 10 CNA} - {U}
  11. • insert {Item 10 CNA} - {Z}
  12. • insert {Item 18} - {COM/ or NAV/}
  13. • insert {Item 10 CNA} - {Y}
  14. • insert {Item 10 CNA} - {X}
  15. • insert {Item 10 CNA} - {W}
  16. • Equipment [Part E] is correct
  17. • Departure Aerodrome and time are correct
  18. • Route is correct
  19. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  20. • Other Information is correct

                                                          1. report
                                                             error

--Test Frame 1.2:
 Stimuli Response
   1. NOT Other Information is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • insert {Item 10 CNA} - {S}
   6. • Equipment [Part 1] is correct
   7. • insert {Item 10 CNA} - {M}
   8. • insert {Item 10 CNA} - {R}
   9. • insert {Item 10 CNA} - {T }
  10. • insert {Item 10 CNA} - {U}
  11. • insert {Item 10 CNA} - {Z}
  12. • insert {Item 18} - {COM/ or NAV/}
  13. • insert {Item 10 CNA} - {Y}
  14. • insert {Item 10 CNA} - {X}
  15. • insert {Item 10 CNA} - {W}
  16. • Equipment [Part E] is correct
  17. • Departure Aerodrome and time are correct
  18. • Route is correct
  19. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.3:
 Stimuli Response
   1. NOT Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • insert {Item 10 CNA} - {S}
   6. • Equipment [Part 1] is correct
   7. • insert {Item 10 CNA} - {M}
   8. • insert {Item 10 CNA} - {R}
   9. • insert {Item 10 CNA} - {T }
  10. • insert {Item 10 CNA} - {U}
  11. • insert {Item 10 CNA} - {Z}
  12. • insert {Item 18} - {COM/ or NAV/}
  13. • insert {Item 10 CNA} - {Y}
  14. • insert {Item 10 CNA} - {X}
  15. • insert {Item 10 CNA} - {W}
  16. • Equipment [Part E] is correct
  17. • Departure Aerodrome and time are correct
  18. • Route is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.4:
 Stimuli Response
   1. NOT Route is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • insert {Item 10 CNA} - {S}
   6. • Equipment [Part 1] is correct
   7. • insert {Item 10 CNA} - {M}
   8. • insert {Item 10 CNA} - {R}
   9. • insert {Item 10 CNA} - {T }
  10. • insert {Item 10 CNA} - {U}
  11. • insert {Item 10 CNA} - {Z}
  12. • insert {Item 18} - {COM/ or NAV/}
  13. • insert {Item 10 CNA} - {Y}
  14. • insert {Item 10 CNA} - {X}
  15. • insert {Item 10 CNA} - {W}
  16. • Equipment [Part E] is correct
  17. • Departure Aerodrome and time are correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.5:
 Stimuli Response
   1. NOT Departure Aerodrome and time are correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • insert {Item 10 CNA} - {S}
   6. • Equipment [Part 1] is correct
   7. • insert {Item 10 CNA} - {M}
   8. • insert {Item 10 CNA} - {R}
   9. • insert {Item 10 CNA} - {T }
  10. • insert {Item 10 CNA} - {U}
  11. • insert {Item 10 CNA} - {Z}
  12. • insert {Item 18} - {COM/ or NAV/}
  13. • insert {Item 10 CNA} - {Y}
  14. • insert {Item 10 CNA} - {X}
  15. • insert {Item 10 CNA} - {W}
  16. • Equipment [Part E] is correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.6:
 Stimuli Response
   1. NOT Equipment [Part E] is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • insert {Item 10 CNA} - {S}
   6. • Equipment [Part 1] is correct
   7. • insert {Item 10 CNA} - {M}
   8. • insert {Item 10 CNA} - {R}
   9. • insert {Item 10 CNA} - {T }
  10. • insert {Item 10 CNA} - {U}
  11. • insert {Item 10 CNA} - {Z}
  12. • insert {Item 18} - {COM/ or NAV/}
  13. • insert {Item 10 CNA} - {Y}
  14. • insert {Item 10 CNA} - {X}
  15. • insert {Item 10 CNA} - {W}
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.7:
 Stimuli Response
   1. NOT Number and Type of Aircraft and Wake
      Turbulence Category is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • insert {Item 10 CNA} - {S}
   5. • Equipment [Part 1] is correct
   6. • insert {Item 10 CNA} - {M}
   7. • insert {Item 10 CNA} - {R}
   8. • insert {Item 10 CNA} - {T }
   9. • insert {Item 10 CNA} - {U}
  10. • insert {Item 10 CNA} - {Z}
  11. • insert {Item 18} - {COM/ or NAV/}
  12. • insert {Item 10 CNA} - {Y}
  13. • insert {Item 10 CNA} - {X}
  14. • insert {Item 10 CNA} - {W}
  15. • Equipment [Part E] is correct
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.8:
 Stimuli Response
   1. NOT FlightRules and Type of Flight is correct
   2. • Aircraft Identification is correct
   3. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   4. • insert {Item 10 CNA} - {S}
   5. • Equipment [Part 1] is correct
   6. • insert {Item 10 CNA} - {M}
   7. • insert {Item 10 CNA} - {R}
   8. • insert {Item 10 CNA} - {T }
   9. • insert {Item 10 CNA} - {U}
  10. • insert {Item 10 CNA} - {Z}
  11. • insert {Item 18} - {COM/ or NAV/}
  12. • insert {Item 10 CNA} - {Y}
  13. • insert {Item 10 CNA} - {X}
  14. • insert {Item 10 CNA} - {W}
  15. • Equipment [Part E] is correct
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.9:
 Stimuli Response
   1. NOT Aircraft Identification is correct
   2. • FlightRules and Type of Flight is correct
   3. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   4. • insert {Item 10 CNA} - {S}
   5. • Equipment [Part 1] is correct
   6. • insert {Item 10 CNA} - {M}
   7. • insert {Item 10 CNA} - {R}
   8. • insert {Item 10 CNA} - {T }
   9. • insert {Item 10 CNA} - {U}
  10. • insert {Item 10 CNA} - {Z}
  11. • insert {Item 18} - {COM/ or NAV/}
  12. • insert {Item 10 CNA} - {Y}
  13. • insert {Item 10 CNA} - {X}
  14. • insert {Item 10 CNA} - {W}
  15. • Equipment [Part E] is correct
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.10:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. NOT Equipment [Part 1] is correct
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • insert {Item 10 CNA} - {S}
   7. • insert {Item 10 CNA} - {M}
   8. • insert {Item 10 CNA} - {R}
   9. • insert {Item 10 CNA} - {T }
  10. • insert {Item 10 CNA} - {U}
  11. • insert {Item 10 CNA} - {Z}
  12. • insert {Item 18} - {COM/ or NAV/}
  13. • insert {Item 10 CNA} - {Y}
  14. • insert {Item 10 CNA} - {X}
  15. • insert {Item 10 CNA} - {W}
  16. • Equipment [Part E] is correct
  17. • Departure Aerodrome and time are correct
  18. • Route is correct
  19. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  20. • Other Information is correct
  21. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.11:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. NOT (insert {Item 10 CNA} - {S} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment [Part 1] is correct
   7. • insert {Item 10 CNA} - {M}
   8. • insert {Item 10 CNA} - {O}
   9. • insert {Item 10 CNA} - {R}
  10. • insert {Item 10 CNA} - {T }
  11. • insert {Item 10 CNA} - {U}
  12. • insert {Item 10 CNA} - {V}
  13. • insert {Item 10 CNA} - {Z}
  14. • insert {Item 18} - {COM/ or NAV/}
  15. • insert {Item 10 CNA} - {Y}
  16. • insert {Item 10 CNA} - {X}
  17. • insert {Item 10 CNA} - {W}
  18. • Equipment [Part E] is correct
  19. • Departure Aerodrome and time are correct
  20. • Route is correct
  21. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  22. • Other Information is correct
  23. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.12:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. {W} is prescribed by ATS
   3. NOT (insert {Item 10 CNA} - {W} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • Equipment [Part 1] is correct
   9. • insert {Item 10 CNA} - {M}
  10. • insert {Item 10 CNA} - {R}
  11. • insert {Item 10 CNA} - {T }
  12. • insert {Item 10 CNA} - {U}
  13. • insert {Item 10 CNA} - {Z}
  14. • insert {Item 18} - {COM/ or NAV/}
  15. • insert {Item 10 CNA} - {Y}
  16. • insert {Item 10 CNA} - {X}
  17. • Equipment [Part E] is correct
  18. • Departure Aerodrome and time are correct
  19. • Route is correct
  20. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  21. • Other Information is correct
  22. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.13:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. {X} is prescribed by ATS
   3. NOT (insert {Item 10 CNA} - {X} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • Equipment [Part 1] is correct
   9. • insert {Item 10 CNA} - {M}
  10. • insert {Item 10 CNA} - {R}
  11. • insert {Item 10 CNA} - {T }
  12. • insert {Item 10 CNA} - {U}
  13. • insert {Item 10 CNA} - {Z}
  14. • insert {Item 18} - {COM/ or NAV/}
  15. • insert {Item 10 CNA} - {Y}
  16. • insert {Item 10 CNA} - {W}
  17. • Equipment [Part E] is correct
  18. • Departure Aerodrome and time are correct
  19. • Route is correct
  20. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  21. • Other Information is correct
  22. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.14:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. {Y} is prescribed by ATS
   3. NOT (insert {Item 10 CNA} - {Y} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • Equipment [Part 1] is correct
   9. • insert {Item 10 CNA} - {M}
  10. • insert {Item 10 CNA} - {R}
  11. • insert {Item 10 CNA} - {T }
  12. • insert {Item 10 CNA} - {U}
  13. • insert {Item 10 CNA} - {Z}
  14. • insert {Item 18} - {COM/ or NAV/}
  15. • insert {Item 10 CNA} - {X}
  16. • insert {Item 10 CNA} - {W}
  17. • Equipment [Part E] is correct
  18. • Departure Aerodrome and time are correct
  19. • Route is correct
  20. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  21. • Other Information is correct
  22. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.15:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {VHF RTF}
   3. NOT (insert {Item 10 CNA} - {V} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • Equipment [Part 1] is correct
   9. • insert {Item 10 CNA} - {M}
  10. • insert {Item 10 CNA} - {R}
  11. • insert {Item 10 CNA} - {T }
  12. • insert {Item 10 CNA} - {U}
  13. • insert {Item 10 CNA} - {Z}
  14. • insert {Item 18} - {COM/ or NAV/}
  15. • insert {Item 10 CNA} - {Y}
  16. • insert {Item 10 CNA} - {X}
  17. • insert {Item 10 CNA} - {W}
  18. • Equipment [Part E] is correct
  19. • Departure Aerodrome and time are correct
  20. • Route is correct
  21. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  22. • Other Information is correct
  23. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.16:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {UHF RTF}
   3. NOT (insert {Item 10 CNA} - {U} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • Equipment [Part 1] is correct
   9. • insert {Item 10 CNA} - {M}
  10. • insert {Item 10 CNA} - {R}
  11. • insert {Item 10 CNA} - {T }
  12. • insert {Item 10 CNA} - {Z}
  13. • insert {Item 18} - {COM/ or NAV/}
  14. • insert {Item 10 CNA} - {Y}
  15. • insert {Item 10 CNA} - {X}
  16. • insert {Item 10 CNA} - {W}
  17. • Equipment [Part E] is correct
  18. • Departure Aerodrome and time are correct
  19. • Route is correct
  20. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  21. • Other Information is correct
  22. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.17:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {TACAN}
   3. NOT (insert {Item 10 CNA} - {T } )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • Equipment [Part 1] is correct
   9. • insert {Item 10 CNA} - {M}
  10. • insert {Item 10 CNA} - {R}
  11. • insert {Item 10 CNA} - {U}
  12. • insert {Item 10 CNA} - {Z}
  13. • insert {Item 18} - {COM/ or NAV/}
  14. • insert {Item 10 CNA} - {Y}
  15. • insert {Item 10 CNA} - {X}
  16. • insert {Item 10 CNA} - {W}
  17. • Equipment [Part E] is correct
  18. • Departure Aerodrome and time are correct
  19. • Route is correct
  20. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  21. • Other Information is correct
  22. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.18:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {RNP type
      certification}
   3. NOT (insert {Item 10 CNA} - {R} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • Equipment [Part 1] is correct
   9. • insert {Item 10 CNA} - {M}
  10. • insert {Item 10 CNA} - {T }
  11. • insert {Item 10 CNA} - {U}
  12. • insert {Item 10 CNA} - {Z}
  13. • insert {Item 18} - {COM/ or NAV/}
  14. • insert {Item 10 CNA} - {Y}
  15. • insert {Item 10 CNA} - {X}
  16. • insert {Item 10 CNA} - {W}
  17. • Equipment [Part E] is correct
  18. • Departure Aerodrome and time are correct
  19. • Route is correct
  20. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  21. • Other Information is correct
  22. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.19:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {VOR}
   3. NOT (insert {Item 10 CNA} - {O} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • Equipment [Part 1] is correct
   9. • insert {Item 10 CNA} - {M}
  10. • insert {Item 10 CNA} - {R}
  11. • insert {Item 10 CNA} - {T }
  12. • insert {Item 10 CNA} - {U}
  13. • insert {Item 10 CNA} - {Z}
  14. • insert {Item 18} - {COM/ or NAV/}
  15. • insert {Item 10 CNA} - {Y}
  16. • insert {Item 10 CNA} - {X}
  17. • insert {Item 10 CNA} - {W}
  18. • Equipment [Part E] is correct
  19. • Departure Aerodrome and time are correct
  20. • Route is correct
  21. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  22. • Other Information is correct
  23. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.20:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {Omega}
   3. NOT (insert {Item 10 CNA} - {M} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • Equipment [Part 1] is correct
   9. • insert {Item 10 CNA} - {R}
  10. • insert {Item 10 CNA} - {T }
  11. • insert {Item 10 CNA} - {U}
  12. • insert {Item 10 CNA} - {Z}
  13. • insert {Item 18} - {COM/ or NAV/}
  14. • insert {Item 10 CNA} - {Y}
  15. • insert {Item 10 CNA} - {X}
  16. • insert {Item 10 CNA} - {W}
  17. • Equipment [Part E] is correct
  18. • Departure Aerodrome and time are correct
  19. • Route is correct
  20. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  21. • Other Information is correct
  22. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.21:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {other}
   3. NOT (insert {Item 18} - {COM/ or NAV/} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • Equipment [Part 1] is correct
   9. • insert {Item 10 CNA} - {M}
  10. • insert {Item 10 CNA} - {R}
  11. • insert {Item 10 CNA} - {T }
  12. • insert {Item 10 CNA} - {U}
  13. • insert {Item 10 CNA} - {Z}
  14. • insert {Item 10 CNA} - {Y}
  15. • insert {Item 10 CNA} - {X}
  16. • insert {Item 10 CNA} - {W}
  17. • Equipment [Part E] is correct
  18. • Departure Aerodrome and time are correct
  19. • Route is correct
  20. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  21. • Other Information is correct
  22. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.22:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. COM/NAV/approach aid equipment is {other}
   3. NOT (insert {Item 10 CNA} - {Z} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • insert {Item 10 CNA} - {S}
   8. • Equipment [Part 1] is correct
   9. • insert {Item 10 CNA} - {M}
  10. • insert {Item 10 CNA} - {R}
  11. • insert {Item 10 CNA} - {T }
  12. • insert {Item 10 CNA} - {U}
  13. • insert {Item 18} - {COM/ or NAV/}
  14. • insert {Item 10 CNA} - {Y}
  15. • insert {Item 10 CNA} - {X}
  16. • insert {Item 10 CNA} - {W}
  17. • Equipment [Part E] is correct
  18. • Departure Aerodrome and time are correct
  19. • Route is correct
  20. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  21. • Other Information is correct
  22. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.1:
 Stimuli Response
   1. NOT Supplementary Information is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • insert {Item 10 CNA} - {S}
   6. • Equipment [Part 1] is correct
   7. • Equipment [Part 2] is correct
   8. • SSR equipment is present
   9. • insert {Item 10 SE} - {A}
  10. • insert {Item 10 SE} - {C}
  11. • insert {Item 10 SE} - {X}
  12. • insert {Item 10 SE} - {P}
  13. • insert {Item 10 SE} - {I}
  14. • insert {Item 10 SE} - {S}
  15. • insert {Item 10 SE} - {D}
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct

                                                          1. report
                                                             error

--Test Frame 1.2:
 Stimuli Response
   1. NOT Other Information is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • insert {Item 10 CNA} - {S}
   6. • Equipment [Part 1] is correct
   7. • Equipment [Part 2] is correct
   8. • SSR equipment is present
   9. • insert {Item 10 SE} - {A}
  10. • insert {Item 10 SE} - {C}
  11. • insert {Item 10 SE} - {X}
  12. • insert {Item 10 SE} - {P}
  13. • insert {Item 10 SE} - {I}
  14. • insert {Item 10 SE} - {S}
  15. • insert {Item 10 SE} - {D}
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.3:
 Stimuli Response
   1. NOT Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • insert {Item 10 CNA} - {S}
   6. • Equipment [Part 1] is correct
   7. • Equipment [Part 2] is correct
   8. • SSR equipment is present
   9. • insert {Item 10 SE} - {A}
  10. • insert {Item 10 SE} - {C}
  11. • insert {Item 10 SE} - {X}
  12. • insert {Item 10 SE} - {P}
  13. • insert {Item 10 SE} - {I}
  14. • insert {Item 10 SE} - {S}
  15. • insert {Item 10 SE} - {D}
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Other Information is correct
  19. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.4:
 Stimuli Response
   1. NOT Route is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • insert {Item 10 CNA} - {S}
   6. • Equipment [Part 1] is correct
   7. • Equipment [Part 2] is correct
   8. • SSR equipment is present
   9. • insert {Item 10 SE} - {A}
  10. • insert {Item 10 SE} - {C}
  11. • insert {Item 10 SE} - {X}
  12. • insert {Item 10 SE} - {P}
  13. • insert {Item 10 SE} - {I}
  14. • insert {Item 10 SE} - {S}
  15. • insert {Item 10 SE} - {D}
  16. • Departure Aerodrome and time are correct
  17. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  18. • Other Information is correct
  19. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.5:
 Stimuli Response
   1. NOT Departure Aerodrome and time are correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • insert {Item 10 CNA} - {S}
   6. • Equipment [Part 1] is correct
   7. • Equipment [Part 2] is correct
   8. • SSR equipment is present
   9. • insert {Item 10 SE} - {A}
  10. • insert {Item 10 SE} - {C}
  11. • insert {Item 10 SE} - {X}
  12. • insert {Item 10 SE} - {P}
  13. • insert {Item 10 SE} - {I}
  14. • insert {Item 10 SE} - {S}
  15. • insert {Item 10 SE} - {D}
  16. • Route is correct
  17. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  18. • Other Information is correct
  19. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.6:
 Stimuli Response
   1. NOT Number and Type of Aircraft and Wake
      Turbulence Category is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • insert {Item 10 CNA} - {S}
   5. • Equipment [Part 1] is correct
   6. • Equipment [Part 2] is correct
   7. • SSR equipment is present
   8. • insert {Item 10 SE} - {A}
   9. • insert {Item 10 SE} - {C}
  10. • insert {Item 10 SE} - {X}
  11. • insert {Item 10 SE} - {P}
  12. • insert {Item 10 SE} - {I}
  13. • insert {Item 10 SE} - {S}
  14. • insert {Item 10 SE} - {D}
  15. • Departure Aerodrome and time are correct
  16. • Route is correct
  17. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  18. • Other Information is correct
  19. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.7:
 Stimuli Response
   1. NOT FlightRules and Type of Flight is correct
   2. • Aircraft Identification is correct
   3. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   4. • insert {Item 10 CNA} - {S}
   5. • Equipment [Part 1] is correct
   6. • Equipment [Part 2] is correct
   7. • SSR equipment is present
   8. • insert {Item 10 SE} - {A}
   9. • insert {Item 10 SE} - {C}
  10. • insert {Item 10 SE} - {X}
  11. • insert {Item 10 SE} - {P}
  12. • insert {Item 10 SE} - {I}
  13. • insert {Item 10 SE} - {S}
  14. • insert {Item 10 SE} - {D}
  15. • Departure Aerodrome and time are correct
  16. • Route is correct
  17. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  18. • Other Information is correct
  19. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.8:
 Stimuli Response
   1. NOT Aircraft Identification is correct
   2. • FlightRules and Type of Flight is correct
   3. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   4. • insert {Item 10 CNA} - {S}
   5. • Equipment [Part 1] is correct
   6. • Equipment [Part 2] is correct
   7. • SSR equipment is present
   8. • insert {Item 10 SE} - {A}
   9. • insert {Item 10 SE} - {C}
  10. • insert {Item 10 SE} - {X}
  11. • insert {Item 10 SE} - {P}
  12. • insert {Item 10 SE} - {I}
  13. • insert {Item 10 SE} - {S}
  14. • insert {Item 10 SE} - {D}
  15. • Departure Aerodrome and time are correct
  16. • Route is correct
  17. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  18. • Other Information is correct
  19. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.9:
 ROIDs: I10SE
 Stimuli Response
   1. ADS capability
   2. NOT (insert {Item 10 SE} - {D} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • insert {Item 10 CNA} - {S}
   7. • Equipment [Part 1] is correct
   8. • Equipment [Part 2] is correct
   9. • SSR equipment is present
  10. • insert {Item 10 SE} - {A}
  11. • insert {Item 10 SE} - {C}
  12. • insert {Item 10 SE} - {X}
  13. • insert {Item 10 SE} - {P}
  14. • insert {Item 10 SE} - {I}
  15. • insert {Item 10 SE} - {S}
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.10:
 ROIDs: I10SE
 Stimuli Response
   1. SSR transponder mode S including
      pressure-altitude and aicraft identification
      trasmission
   2. NOT (insert {Item 10 SE} - {S} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • insert {Item 10 CNA} - {S}
   7. • Equipment [Part 1] is correct
   8. • Equipment [Part 2] is correct
   9. • SSR equipment is present
  10. • insert {Item 10 SE} - {A}
  11. • insert {Item 10 SE} - {C}
  12. • insert {Item 10 SE} - {X}
  13. • insert {Item 10 SE} - {P}
  14. • insert {Item 10 SE} - {I}
  15. • insert {Item 10 SE} - {D}
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.11:
 ROIDs: I10SE
 Stimuli Response
   1. SSR transponder mode S including aircraft
      identification trasmission
   2. NOT (insert {Item 10 SE} - {I} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • insert {Item 10 CNA} - {S}
   7. • Equipment [Part 1] is correct
   8. • Equipment [Part 2] is correct
   9. • SSR equipment is present
  10. • insert {Item 10 SE} - {A}
  11. • insert {Item 10 SE} - {C}
  12. • insert {Item 10 SE} - {X}
  13. • insert {Item 10 SE} - {P}
  14. • insert {Item 10 SE} - {S}
  15. • insert {Item 10 SE} - {D}
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.12:
 ROIDs: I10SE
 Stimuli Response
   1. SSR transponder mode S including
      pressure-altitude trasmission
   2. NOT (insert {Item 10 SE} - {P} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • insert {Item 10 CNA} - {S}
   7. • Equipment [Part 1] is correct
   8. • Equipment [Part 2] is correct
   9. • SSR equipment is present
  10. • insert {Item 10 SE} - {A}
  11. • insert {Item 10 SE} - {C}
  12. • insert {Item 10 SE} - {X}
  13. • insert {Item 10 SE} - {I}
  14. • insert {Item 10 SE} - {S}
  15. • insert {Item 10 SE} - {D}
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.13:
 ROIDs: I10SE
 Stimuli Response
   1. SSR transponder mode S only
   2. NOT (insert {Item 10 SE} - {X} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • insert {Item 10 CNA} - {S}
   7. • Equipment [Part 1] is correct
   8. • Equipment [Part 2] is correct
   9. • SSR equipment is present
  10. • insert {Item 10 SE} - {A}
  11. • insert {Item 10 SE} - {C}
  12. • insert {Item 10 SE} - {P}
  13. • insert {Item 10 SE} - {I}
  14. • insert {Item 10 SE} - {S}
  15. • insert {Item 10 SE} - {D}
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.14:
 ROIDs: I10SE
 Stimuli Response
   1. SSR transponder mode A and mode C
   2. NOT (insert {Item 10 SE} - {C} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • insert {Item 10 CNA} - {S}
   7. • Equipment [Part 1] is correct
   8. • Equipment [Part 2] is correct
   9. • SSR equipment is present
  10. • insert {Item 10 SE} - {A}
  11. • insert {Item 10 SE} - {X}
  12. • insert {Item 10 SE} - {P}
  13. • insert {Item 10 SE} - {I}
  14. • insert {Item 10 SE} - {S}
  15. • insert {Item 10 SE} - {D}
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.15:
 ROIDs: I10SE
 Stimuli Response
   1. SSR transponder mode A
   2. NOT (insert {Item 10 SE} - {A} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • insert {Item 10 CNA} - {S}
   7. • Equipment [Part 1] is correct
   8. • Equipment [Part 2] is correct
   9. • SSR equipment is present
  10. • insert {Item 10 SE} - {C}
  11. • insert {Item 10 SE} - {X}
  12. • insert {Item 10 SE} - {P}
  13. • insert {Item 10 SE} - {I}
  14. • insert {Item 10 SE} - {S}
  15. • insert {Item 10 SE} - {D}
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.16:
 ROIDs: I10SE
 Stimuli Response
   1. NOT SSR equipment is present
   2. NOT (insert {Item 10 SE} - {N} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • insert {Item 10 CNA} - {S}
   7. • Equipment [Part 1] is correct
   8. • Equipment [Part 2] is correct
   9. • insert {Item 10 SE} - {A}
  10. • insert {Item 10 SE} - {C}
  11. • insert {Item 10 SE} - {X}
  12. • insert {Item 10 SE} - {P}
  13. • insert {Item 10 SE} - {I}
  14. • insert {Item 10 SE} - {S}
  15. • insert {Item 10 SE} - {D}
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.17:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. NOT Equipment [Part 2] is correct
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • insert {Item 10 CNA} - {S}
   7. • Equipment [Part 1] is correct
   8. • SSR equipment is present
   9. • insert {Item 10 SE} - {A}
  10. • insert {Item 10 SE} - {C}
  11. • insert {Item 10 SE} - {X}
  12. • insert {Item 10 SE} - {P}
  13. • insert {Item 10 SE} - {I}
  14. • insert {Item 10 SE} - {S}
  15. • insert {Item 10 SE} - {D}
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.18:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. NOT Equipment [Part 1] is correct
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • insert {Item 10 CNA} - {S}
   7. • Equipment [Part 2] is correct
   8. • SSR equipment is present
   9. • insert {Item 10 SE} - {A}
  10. • insert {Item 10 SE} - {C}
  11. • insert {Item 10 SE} - {X}
  12. • insert {Item 10 SE} - {P}
  13. • insert {Item 10 SE} - {I}
  14. • insert {Item 10 SE} - {S}
  15. • insert {Item 10 SE} - {D}
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.19:
 ROIDs: I10
 Stimuli Response
   1. Standard COM/NAV/approach aid equipment for the
      route to be flown is carried and is serviceable
   2. NOT (insert {Item 10 CNA} - {S} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment [Part 1] is correct
   7. • Equipment [Part 2] is correct
   8. • SSR equipment is present
   9. • insert {Item 10 SE} - {A}
  10. • insert {Item 10 SE} - {C}
  11. • insert {Item 10 SE} - {X}
  12. • insert {Item 10 SE} - {P}
  13. • insert {Item 10 SE} - {I}
  14. • insert {Item 10 SE} - {S}
  15. • insert {Item 10 SE} - {D}
  16. • Departure Aerodrome and time are correct
  17. • Route is correct
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

E.3.5 Departure Aerodrome and Time

--Test Frame 1.1:
 Stimuli Response
   1. NOT Supplementary Information is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • The flight plan is received from an aircraft
      in flight
   7. • insert {Item 13 A} - {AFIL}
   8. • insert {Item 18} - {DEP/ the four-letter
      location indicator of the location of the ATS
      unit from which supplementary flight data can be
      obtained}
   9. • The flight plan was submitted before departure
  10. • insert {Item 13 B} - {the estimated off-block
      time}
  11. • Route is correct
  12. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  13. • Other Information is correct

                                                          1. report
                                                             error

--Test Frame 1.2:
 Stimuli Response
   1. NOT Other Information is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • The flight plan is received from an aircraft
      in flight
   7. • insert {Item 13 A} - {AFIL}
   8. • insert {Item 18} - {DEP/ the four-letter
      location indicator of the location of the ATS
      unit from which supplementary flight data can be
      obtained}
   9. • The flight plan was submitted before departure
  10. • insert {Item 13 B} - {the estimated off-block
      time}
  11. • Route is correct
  12. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  13. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.3:
 Stimuli Response
   1. NOT Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • The flight plan is received from an aircraft
      in flight
   7. • insert {Item 13 A} - {AFIL}
   8. • insert {Item 18} - {DEP/ the four-letter
      location indicator of the location of the ATS
      unit from which supplementary flight data can be
      obtained}
   9. • The flight plan was submitted before departure
  10. • insert {Item 13 B} - {the estimated off-block
      time}
  11. • Route is correct
  12. • Other Information is correct
  13. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.4:
 Stimuli Response
   1. NOT Route is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • The flight plan is received from an aircraft
      in flight
   7. • insert {Item 13 A} - {AFIL}
   8. • insert {Item 18} - {DEP/ the four-letter
      location indicator of the location of the ATS
      unit from which supplementary flight data can be
      obtained}
   9. • The flight plan was submitted before departure
  10. • insert {Item 13 B} - {the estimated off-block
      time}
  11. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  12. • Other Information is correct
  13. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.5:
 Stimuli Response
   1. NOT Equipment is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • The flight plan is received from an aircraft
      in flight
   6. • insert {Item 13 A} - {AFIL}
   7. • insert {Item 18} - {DEP/ the four-letter
      location indicator of the location of the ATS
      unit from which supplementary flight data can be
      obtained}
   8. • The flight plan was submitted before departure
   9. • insert {Item 13 B} - {the estimated off-block
      time}
  10. • Route is correct
  11. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  12. • Other Information is correct
  13. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.6:
 Stimuli Response
   1. NOT Number and Type of Aircraft and Wake
      Turbulence Category is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Equipment is correct
   5. • The flight plan is received from an aircraft
      in flight
   6. • insert {Item 13 A} - {AFIL}
   7. • insert {Item 18} - {DEP/ the four-letter
      location indicator of the location of the ATS
      unit from which supplementary flight data can be
      obtained}
   8. • The flight plan was submitted before departure
   9. • insert {Item 13 B} - {the estimated off-block
      time}
  10. • Route is correct
  11. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  12. • Other Information is correct
  13. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.7:
 Stimuli Response
   1. NOT FlightRules and Type of Flight is correct
   2. • Aircraft Identification is correct
   3. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   4. • Equipment is correct
   5. • The flight plan is received from an aircraft
      in flight
   6. • insert {Item 13 A} - {AFIL}
   7. • insert {Item 18} - {DEP/ the four-letter
      location indicator of the location of the ATS
      unit from which supplementary flight data can be
      obtained}
   8. • The flight plan was submitted before departure
   9. • insert {Item 13 B} - {the estimated off-block
      time}
  10. • Route is correct
  11. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  12. • Other Information is correct
  13. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.8:
 Stimuli Response
   1. NOT Aircraft Identification is correct
   2. • FlightRules and Type of Flight is correct
   3. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   4. • Equipment is correct
   5. • The flight plan is received from an aircraft
      in flight
   6. • insert {Item 13 A} - {AFIL}
   7. • insert {Item 18} - {DEP/ the four-letter
      location indicator of the location of the ATS
      unit from which supplementary flight data can be
      obtained}
   8. • The flight plan was submitted before departure
   9. • insert {Item 13 B} - {the estimated off-block
      time}
  10. • Route is correct
  11. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  12. • Other Information is correct
  13. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.9:
 ROIDs: I13
 Stimuli Response
   1. NOT The flight plan was submitted before
      departure
   2. NOT (insert {Item 13 B} - { {the estimated time}
      over the first point of the route to which the
      flight plan applies} )
   3. NOT (insert {Item 13 B} - { {the actual time}
      over the first point of the route to which the
      flight plan applies} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • Equipment is correct
   8. • The flight plan is received from an aircraft
      in flight
   9. • insert {Item 13 A} - {AFIL}
  10. • insert {Item 18} - {DEP/ the four-letter
      location indicator of the location of the ATS
      unit from which supplementary flight data can be
      obtained}
  11. • Route is correct
  12. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  13. • Other Information is correct
  14. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.10:
 ROIDs: I13
 Stimuli Response
   1. NOT The flight plan is received from an aircraft
      in flight
   2. Location indicator has been assigned
   3. NOT (insert {Item 13 A} - {the ICAO four-letter
      location indicator of the departure aerodrome} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • Equipment is correct
   8. • The flight plan was submitted before departure
   9. • insert {Item 13 B} - {the estimated off-block
      time}
  10. • Route is correct
  11. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  12. • Other Information is correct
  13. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.11:
 ROIDs: I13
 Stimuli Response
   1. The flight plan was submitted before departure
   2. NOT (insert {Item 13 B} - {the estimated
      off-block time} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • The flight plan is received from an aircraft
      in flight
   8. • insert {Item 13 A} - {AFIL}
   9. • insert {Item 18} - {DEP/ the four-letter
      location indicator of the location of the ATS
      unit from which supplementary flight data can be
      obtained}
  10. • Route is correct
  11. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  12. • Other Information is correct
  13. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.12:
 ROIDs: I13
 Stimuli Response
   1. The flight plan is received from an aircraft in
      flight
   2. NOT (insert {Item 18} - {DEP/ the four-letter
      location indicator of the location of the ATS
      unit from which supplementary flight data can be
      obtained} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • insert {Item 13 A} - {AFIL}
   8. • The flight plan was submitted before departure
   9. • insert {Item 13 B} - {the estimated off-block
      time}
  10. • Route is correct
  11. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  12. • Other Information is correct
  13. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.13:
 ROIDs: I13
 Stimuli Response
   1. NOT The flight plan is received from an aircraft
      in flight
   2. NOT Location indicator has been assigned
   3. NOT (insert {Item 13} - {DEP/ aerodrome name} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • Equipment is correct
   8. • insert {Item 13 A} - {ZZZZZ}
   9. • The flight plan was submitted before departure
  10. • insert {Item 13 B} - {the estimated off-block
      time}
  11. • Route is correct
  12. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  13. • Other Information is correct
  14. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.14:
 ROIDs: I13
 Stimuli Response
   1. The flight plan is received from an aircraft in
      flight
   2. NOT (insert {Item 13 A} - {AFIL} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • insert {Item 18} - {DEP/ the four-letter
      location indicator of the location of the ATS
      unit from which supplementary flight data can be
      obtained}
   8. • The flight plan was submitted before departure
   9. • insert {Item 13 B} - {the estimated off-block
      time}
  10. • Route is correct
  11. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  12. • Other Information is correct
  13. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.15:
 ROIDs: I13
 Stimuli Response
   1. NOT The flight plan is received from an aircraft
      in flight
   2. NOT Location indicator has been assigned
   3. NOT (insert {Item 13 A} - {ZZZZZ} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • Equipment is correct
   8. • insert {Item 13} - {DEP/ aerodrome name}
   9. • The flight plan was submitted before departure
  10. • insert {Item 13 B} - {the estimated off-block
      time}
  11. • Route is correct
  12. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  13. • Other Information is correct
  14. • Supplementary Information is correct

                                                          1. report
                                                             error

E.3.6 Route

--Test Frame 1.1:
 Stimuli Response
   1. NOT Supplementary Information is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct

   6. • Departure Aerodrome and time are correct
   7. • Mach number is prescribed by the appropriate
      ATS authority
   8. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
   9. • Flight is uncontrolled VFR
  10. • insert {Item 15 B} - {VFR}

  11. • The flight is along a designated ATS route
  12. • The departure aerodrome is {connected to} the
      ATS route
  13. • insert {Item 15 C} - {the designator of the
      first ATS route}

  14. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct

  15. • Other Information is correct
  16. • forall point. NOT (A change of {ATS route
      other than same direction lower/upper} is
      planned at {point} ) OR NOT ( {next {point} }
      is defined by geological co-ordinates) OR NOT (

{point} is defined by geological co-ordinates)

    OR insert {Item 15 C} - { {point} followed by
    the designator of the next ATS route segment}
17. • forall point. NOT (A change of {speed} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

    route) OR {point} is defined by geological
    co-ordinates OR insert {Item 15 C} - { {point}
    followed by DCT}

18. • forall point. NOT (A change of {level} is
    planned at {point} ) OR The flight to the {next

{point} } will be outside a designated route OR

    insert {Item 15 C} - { {point} followed by the
    designator of the next ATS route segment}

19. • forall point. NOT (A change of {ATS route
    other than same direction lower/upper} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {next {point} } is defined by
geological co-ordinates OR insert {Item 15 C}
- { {point} followed by DCT}

                                                    1. report
                                                       error

--Test Frame 1.2:
 Stimuli Response
   1. NOT Other Information is correct
   2. • Aircraft Identification is correct

   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Mach number is prescribed by the appropriate
      ATS authority
   8. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }

   9. • Flight is uncontrolled VFR
  10. • insert {Item 15 B} - {VFR}
  11. • The flight is along a designated ATS route
  12. • The departure aerodrome is {connected to} the
      ATS route
  13. • insert {Item 15 C} - {the designator of the
      first ATS route}
  14. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  15. • Supplementary Information is correct
  16. • forall point. NOT (A change of {ATS route
      other than same direction lower/upper} is
      planned at {point} ) OR NOT ( {next {point} }
      is defined by geological co-ordinates) OR NOT (

{point} is defined by geological co-ordinates)

    OR insert {Item 15 C} - { {point} followed by
    the designator of the next ATS route segment}

17. • forall point. NOT (A change of {speed} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

    route) OR {point} is defined by geological
    co-ordinates OR insert {Item 15 C} - { {point}
    followed by DCT}
18. • forall point. NOT (A change of {level} is
    planned at {point} ) OR The flight to the {next

{point} } will be outside a designated route OR

    insert {Item 15 C} - { {point} followed by the
    designator of the next ATS route segment}
19. • forall point. NOT (A change of {ATS route
    other than same direction lower/upper} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {next {point} } is defined by
geological co-ordinates OR insert {Item 15 C}
- { {point} followed by DCT}

                                                    1. report
                                                       error

--Test Frame 1.3:
 Stimuli Response
   1. NOT Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct

   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct

   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Mach number is prescribed by the appropriate
      ATS authority
   8. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
   9. • Flight is uncontrolled VFR
  10. • insert {Item 15 B} - {VFR}

  11. • The flight is along a designated ATS route
  12. • The departure aerodrome is {connected to} the
      ATS route
  13. • insert {Item 15 C} - {the designator of the
      first ATS route}
  14. • Other Information is correct
  15. • Supplementary Information is correct
  16. • forall point. NOT (A change of {ATS route
      other than same direction lower/upper} is
      planned at {point} ) OR NOT ( {next {point} }
      is defined by geological co-ordinates) OR NOT (

{point} is defined by geological co-ordinates)

    OR insert {Item 15 C} - { {point} followed by
    the designator of the next ATS route segment}

17. • forall point. NOT (A change of {speed} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

    route) OR {point} is defined by geological
    co-ordinates OR insert {Item 15 C} - { {point}
    followed by DCT}
18. • forall point. NOT (A change of {level} is
    planned at {point} ) OR The flight to the {next

{point} } will be outside a designated route OR

    insert {Item 15 C} - { {point} followed by the
    designator of the next ATS route segment}
19. • forall point. NOT (A change of {ATS route
    other than same direction lower/upper} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {next {point} } is defined by
geological co-ordinates OR insert {Item 15 C}
- { {point} followed by DCT}

                                                    1. report
                                                       error

--Test Frame 1.4:
 Stimuli Response
   1. NOT Departure Aerodrome and time are correct
   2. • Aircraft Identification is correct

   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Mach number is prescribed by the appropriate
      ATS authority
   7. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
   8. • Flight is uncontrolled VFR

   9. • insert {Item 15 B} - {VFR}
  10. • The flight is along a designated ATS route
  11. • The departure aerodrome is {connected to} the
      ATS route
  12. • insert {Item 15 C} - {the designator of the
      first ATS route}
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct
  16. • forall point. NOT (A change of {ATS route
      other than same direction lower/upper} is
      planned at {point} ) OR NOT ( {next {point} }
      is defined by geological co-ordinates) OR NOT (

{point} is defined by geological co-ordinates)

    OR insert {Item 15 C} - { {point} followed by
    the designator of the next ATS route segment}

17. • forall point. NOT (A change of {speed} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

    route) OR {point} is defined by geological
    co-ordinates OR insert {Item 15 C} - { {point}
    followed by DCT}
18. • forall point. NOT (A change of {level} is
    planned at {point} ) OR The flight to the {next

{point} } will be outside a designated route OR

    insert {Item 15 C} - { {point} followed by the
    designator of the next ATS route segment}
19. • forall point. NOT (A change of {ATS route
    other than same direction lower/upper} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {next {point} } is defined by
geological co-ordinates OR insert {Item 15 C}
- { {point} followed by DCT}

                                                    1. report
                                                       error

--Test Frame 1.5:
 Stimuli Response
   1. NOT Equipment is correct
   2. • Aircraft Identification is correct

   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Departure Aerodrome and time are correct
   6. • Mach number is prescribed by the appropriate
      ATS authority
   7. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
   8. • Flight is uncontrolled VFR

   9. • insert {Item 15 B} - {VFR}
  10. • The flight is along a designated ATS route
  11. • The departure aerodrome is {connected to} the
      ATS route
  12. • insert {Item 15 C} - {the designator of the
      first ATS route}
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct
  16. • forall point. NOT (A change of {ATS route
      other than same direction lower/upper} is
      planned at {point} ) OR NOT ( {next {point} }
      is defined by geological co-ordinates) OR NOT (

{point} is defined by geological co-ordinates)

    OR insert {Item 15 C} - { {point} followed by
    the designator of the next ATS route segment}

17. • forall point. NOT (A change of {speed} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

    route) OR {point} is defined by geological
    co-ordinates OR insert {Item 15 C} - { {point}
    followed by DCT}
18. • forall point. NOT (A change of {level} is
    planned at {point} ) OR The flight to the {next

{point} } will be outside a designated route OR

    insert {Item 15 C} - { {point} followed by the
    designator of the next ATS route segment}
19. • forall point. NOT (A change of {ATS route
    other than same direction lower/upper} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {next {point} } is defined by
geological co-ordinates OR insert {Item 15 C}
- { {point} followed by DCT}

                                                    1. report
                                                       error

--Test Frame 1.6:
 Stimuli Response
   1. NOT Number and Type of Aircraft and Wake
      Turbulence Category is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct

   4. • Equipment is correct
   5. • Departure Aerodrome and time are correct
   6. • Mach number is prescribed by the appropriate
      ATS authority
   7. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
   8. • Flight is uncontrolled VFR

   9. • insert {Item 15 B} - {VFR}
  10. • The flight is along a designated ATS route
  11. • The departure aerodrome is {connected to} the
      ATS route
  12. • insert {Item 15 C} - {the designator of the
      first ATS route}
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct
  16. • forall point. NOT (A change of {ATS route
      other than same direction lower/upper} is
      planned at {point} ) OR NOT ( {next {point} }
      is defined by geological co-ordinates) OR NOT (

{point} is defined by geological co-ordinates)

    OR insert {Item 15 C} - { {point} followed by
    the designator of the next ATS route segment}

17. • forall point. NOT (A change of {speed} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

    route) OR {point} is defined by geological
    co-ordinates OR insert {Item 15 C} - { {point}
    followed by DCT}
18. • forall point. NOT (A change of {level} is
    planned at {point} ) OR The flight to the {next

{point} } will be outside a designated route OR

    insert {Item 15 C} - { {point} followed by the
    designator of the next ATS route segment}
19. • forall point. NOT (A change of {ATS route
    other than same direction lower/upper} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {next {point} } is defined by
geological co-ordinates OR insert {Item 15 C}
- { {point} followed by DCT}

                                                    1. report
                                                       error

--Test Frame 1.7:
 Stimuli Response
   1. NOT FlightRules and Type of Flight is correct
   2. • Aircraft Identification is correct

   3. • Number and Type of Aircraft and Wake
      Turbulence Category is correct

   4. • Equipment is correct
   5. • Departure Aerodrome and time are correct
   6. • Mach number is prescribed by the appropriate
      ATS authority
   7. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
   8. • Flight is uncontrolled VFR

   9. • insert {Item 15 B} - {VFR}
  10. • The flight is along a designated ATS route
  11. • The departure aerodrome is {connected to} the
      ATS route
  12. • insert {Item 15 C} - {the designator of the
      first ATS route}
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct
  16. • forall point. NOT (A change of {ATS route
      other than same direction lower/upper} is
      planned at {point} ) OR NOT ( {next {point} }
      is defined by geological co-ordinates) OR NOT (

{point} is defined by geological co-ordinates)

    OR insert {Item 15 C} - { {point} followed by
    the designator of the next ATS route segment}

17. • forall point. NOT (A change of {speed} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

    route) OR {point} is defined by geological
    co-ordinates OR insert {Item 15 C} - { {point}
    followed by DCT}
18. • forall point. NOT (A change of {level} is
    planned at {point} ) OR The flight to the {next

{point} } will be outside a designated route OR

    insert {Item 15 C} - { {point} followed by the
    designator of the next ATS route segment}
19. • forall point. NOT (A change of {ATS route
    other than same direction lower/upper} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {next {point} } is defined by
geological co-ordinates OR insert {Item 15 C}
- { {point} followed by DCT}

                                                    1. report
                                                       error

--Test Frame 1.8:
 Stimuli Response
   1. NOT Aircraft Identification is correct
   2. • FlightRules and Type of Flight is correct

   3. • Number and Type of Aircraft and Wake
      Turbulence Category is correct

   4. • Equipment is correct
   5. • Departure Aerodrome and time are correct
   6. • Mach number is prescribed by the appropriate
      ATS authority
   7. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
   8. • Flight is uncontrolled VFR

   9. • insert {Item 15 B} - {VFR}
  10. • The flight is along a designated ATS route
  11. • The departure aerodrome is {connected to} the
      ATS route
  12. • insert {Item 15 C} - {the designator of the
      first ATS route}
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct
  16. • forall point. NOT (A change of {ATS route
      other than same direction lower/upper} is
      planned at {point} ) OR NOT ( {next {point} }
      is defined by geological co-ordinates) OR NOT (

{point} is defined by geological co-ordinates)

    OR insert {Item 15 C} - { {point} followed by
    the designator of the next ATS route segment}

17. • forall point. NOT (A change of {speed} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

    route) OR {point} is defined by geological
    co-ordinates OR insert {Item 15 C} - { {point}
    followed by DCT}
18. • forall point. NOT (A change of {level} is
    planned at {point} ) OR The flight to the {next

{point} } will be outside a designated route OR

    insert {Item 15 C} - { {point} followed by the
    designator of the next ATS route segment}
19. • forall point. NOT (A change of {ATS route
    other than same direction lower/upper} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {next {point} } is defined by
geological co-ordinates OR insert {Item 15 C}
- { {point} followed by DCT}

                                                    1. report
                                                       error

--Test Frame 1.9:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route

   2. {point} is listed in Item 15 C
   3. NOT (A significant point code designator has
      been assigned to {point} )
   4. NOT (2 figures describing latitude in degrees
      followed by {S} followed by 3 figures describing
      longitude in degrees followed by {W} is
      associated with {point} )
   5. NOT (2 figures describing latitude in degrees
      followed by {S} followed by 3 figures describing
      longitude in degrees followed by {E} is
      associated with {point} )
   6. NOT (2 figures describing latitude in degrees
      followed by {N} followed by 3 figures describing
      longitude in degrees followed by {W} is
      associated with {point} )

   7. NOT (2 figures describing latitude in degrees
      followed by {N} followed by 3 figures describing
      longitude in degrees followed by {E} is
      associated with {point} )
   8. NOT (4 figures describing latitude in degrees
      and tens of units of minutes followed by {S}
      followed by 5 figures describing longitude in
      degrees and tens of units of minutes followed by

{W} is associated with {point} )

9. NOT (4 figures describing latitude in degrees
   and tens of units of minutes followed by {S}
   followed by 5 figures describing longitude in
   degrees and tens of units of minutes followed by

{E} is associated with {point} )

10. NOT (4 figures describing latitude in degrees
    and tens of units of minutes followed by {N}
    followed by 5 figures describing longitude in
    degrees and tens of units of minutes followed by

{W} is associated with {point} )

11. NOT (4 figures describing latitude in degrees
    and tens of units of minutes followed by {N}
    followed by 5 figures describing longitude in
    degrees and tens of units of minutes followed by

{E} is associated with {point} )

12. NOT (the 2 or 3 character identification of the
    navigation aid followed by the 3 figure bearing
    from the aid in degrees magnetic followed by the
    distance from the aid in 3 figures expressing
    nautical miles is associated with {point} )

                                                        1. report
                                                           error

--Test Frame 1.9: (continued)
 ROIDs: I15C
 Stimuli Response
  13. • Aircraft Identification is correct
  14. • FlightRules and Type of Flight is correct
  15. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
  16. • Equipment is correct
  17. • Departure Aerodrome and time are correct
  18. • Mach number is prescribed by the appropriate
      ATS authority
  19. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
  20. • Flight is uncontrolled VFR
  21. • insert {Item 15 B} - {VFR}
  22. • ATS flight track points are required by the
      appropriate ATS authority
  23. • Use ATS style track points
  24. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  25. • Other Information is correct
  26. • Supplementary Information is correct
  27. • forall point. A change of {flight rules} is
      planned at {point} OR A change of {level} is
      planned at {point} OR A change of {speed} is
      planned at {point} OR ATS flight track points
      are required by the appropriate ATS authority OR
      NOT (insert {Item 15 C} - { {point} details} )
      OR A change of {track} is planned at {point}
  28. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR NOT (

{point B} is defined by {bearing and distance}

) OR NOT ( {point} is defined by {bearing and
distance} ) OR insert {Item 15 C} - {DCT between

{point} and {point B} }

--Test Frame 1.9: (continued)
 ROIDs: I15C
 Stimuli Response
  29. • forall point. NOT ( {point} is listed in Item
      15 C) OR the code designator assigned to {route
      segment} including where appropriate the coded
      designator assigned to the standard {arrival}
      route is associated with {point} OR the code
      designator assigned to {route segment} including
      where appropriate the coded designator assigned
      to the standard {departure} route is associated
      with {point} OR the code designator assigned to

{route} including where appropriate the coded

designator assigned to the standard {arrival}
route is associated with {point} OR the code
designator assigned to {route} including where
appropriate the coded designator assigned to the
standard {departure} route is associated with

{point}

30. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR IFR to VFR OR NOT VFR
    to IFR OR the letters IFR are associated with

{point}

31. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A change of {level - climb}
    is planned at {point} ) OR an oblique stroke
    followed by the speed to be maintained during
    cruise climb followed by {the level above
    which cruise climb is planned followed by
    PLUS} is associated with {point} OR an oblique
    stroke followed by the speed to be maintained
    during cruise climb followed by {the two levels
    defining the layer to be occupied during cruide
    climb} is associated with {point}

32. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A significant point code
    designator has been assigned to {point} ) OR
    the 2 to 5 characters of the assigned coded
    designator is associated with {point}

33. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 0.01 Mach

    or more} is planned at {point} )
34. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - {DCT between {point} and {point B} } OR NOT ( {point B} is defined by {goegraphical

co-ordinates} ) OR NOT ( {point} is defined by

{goegraphical co-ordinates} )

--Test Frame 1.9: (continued)
 ROIDs: I15C
 Stimuli Response
  35. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point

    B} } OR {point} is defined by {goegraphical
    co-ordinates}

36. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR NOT IFR to VFR OR the
    letters VFR are associated with {point}
37. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 5pc TAS or

    more} is planned at {point} )

38. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point B} } OR {point B} is defined by {goegraphical

    co-ordinates}

39. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point}
    is defined by {bearing and distance} OR insert

{Item 15 C} - { {point} followed by {point B} }

40. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point
    B} is defined by {bearing and distance} OR
    insert {Item 15 C} - { {point} followed by

{point B} }

--Test Frame 1.10:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. NOT (A change of {flight rules} is planned at

{point} )

 3. NOT (A change of {level} is planned at {point} )
 4. NOT (A change of {speed} is planned at {point} )
 5. NOT ATS flight track points are required by the
    appropriate ATS authority
 6. insert {Item 15 C} - { {point} details}
 7. NOT (A change of {track} is planned at {point} )
 8. • Aircraft Identification is correct
 9. • FlightRules and Type of Flight is correct
10. • Number and Type of Aircraft and Wake
    Turbulence Category is correct
11. • Equipment is correct
12. • Departure Aerodrome and time are correct
13. • Mach number is prescribed by the appropriate
    ATS authority
14. • insert {Item 15 A} - {the true airspeed for
    the first or the whole cruising portion of the
    flight expressed as {M followed by 3 digits of
    Mach hundredths} }
15. • Flight is uncontrolled VFR
16. • insert {Item 15 B} - {VFR}
17. • Destination Aerodrome and Total Estimated
    Elapsed Time is correct
18. • Other Information is correct
19. • Supplementary Information is correct

                                                        1. report
                                                           error

--Test Frame 1.10: (continued)
 ROIDs: I15C
 Stimuli Response
  20. • forall point. NOT ( {point} is listed in Item
      15 C) OR A significant point code designator
      has been assigned to {point} OR 2 figures
      describing latitude in degrees followed by

{S} followed by 3 figures describing longitude

in degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {S} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 2 figures

describing latitude in degrees followed by {N}
followed by 3 figures describing longitude in
degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {N} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 4 figures

describing latitude in degrees and tens of units
of minutes followed by {S} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{S} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR 4 figures
describing latitude in degrees and tens of units
of minutes followed by {N} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{N} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR the 2 or 3
character identification of the navigation aid
followed by the 3 figure bearing from the aid in
degrees magnetic followed by the distance from
the aid in 3 figures expressing nautical miles
is associated with {point}

--Test Frame 1.10: (continued)
 ROIDs: I15C
 Stimuli Response
  21. • forall point. NOT ( {point} is listed in Item
      15 C) OR the code designator assigned to {route
      segment} including where appropriate the coded
      designator assigned to the standard {arrival}
      route is associated with {point} OR the code
      designator assigned to {route segment} including
      where appropriate the coded designator assigned
      to the standard {departure} route is associated
      with {point} OR the code designator assigned to

{route} including where appropriate the coded

designator assigned to the standard {arrival}
route is associated with {point} OR the code
designator assigned to {route} including where
appropriate the coded designator assigned to the
standard {departure} route is associated with

{point}

22. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR IFR to VFR OR NOT VFR
    to IFR OR the letters IFR are associated with

{point}

23. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A change of {level - climb}
    is planned at {point} ) OR an oblique stroke
    followed by the speed to be maintained during
    cruise climb followed by {the level above
    which cruise climb is planned followed by
    PLUS} is associated with {point} OR an oblique
    stroke followed by the speed to be maintained
    during cruise climb followed by {the two levels
    defining the layer to be occupied during cruide
    climb} is associated with {point}

24. • forall point. insert {Item 15 C} - { {point}
    details} OR {point} and {next {point} } are
    normally more than {30 minutes flying time}
    apart OR NOT (A change of {track} is planned at

{point} )

25. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A significant point code
    designator has been assigned to {point} ) OR
    the 2 to 5 characters of the assigned coded
    designator is associated with {point}
26. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 0.01 Mach

or more} is planned at {point} )

--Test Frame 1.10: (continued)
 ROIDs: I15C
 Stimuli Response
  27. • forall point. NOT (insert {Item 15 C} -

{ {point} details} ) OR NOT ( {point} and {next {point} } are normally more than {370km}

    apart) OR NOT ( {point} and {next {point} } are
    normally more than {30 minutes flying time}
    apart)
28. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR NOT IFR to VFR OR the
    letters VFR are associated with {point}
29. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 5pc TAS or

    more} is planned at {point} )
30. • forall point. insert {Item 15 C} - { {point}
    details} OR {point} and {next {point} } are
    normally more than {370km} apart OR NOT (A
    change of {track} is planned at {point} )

--Test Frame 1.11:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS route

   2. A change of {ATS route other than same direction
      lower/upper} is planned at {point}

   3. {next {point} } is defined by geological
      co-ordinates

   4. {point} is defined by geological co-ordinates
   5. NOT (insert {Item 15 C} - { {point} followed by
      the designator of the next ATS route segment} )
   6. • Aircraft Identification is correct
   7. • FlightRules and Type of Flight is correct
   8. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   9. • Equipment is correct
  10. • Departure Aerodrome and time are correct

  11. • Mach number is prescribed by the appropriate
      ATS authority

  12. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
  13. • Flight is uncontrolled VFR
  14. • insert {Item 15 B} - {VFR}
  15. • The departure aerodrome is {connected to} the
      ATS route
  16. • insert {Item 15 C} - {the designator of the
      first ATS route}
  17. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  18. • Other Information is correct

  19. • Supplementary Information is correct
  20. • forall point. NOT (A change of {speed} is
      planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

    route) OR {point} is defined by geological
    co-ordinates OR insert {Item 15 C} - { {point}
    followed by DCT}
21. • forall point. NOT (A change of {level} is
    planned at {point} ) OR The flight to the {next

{point} } will be outside a designated route OR

    insert {Item 15 C} - { {point} followed by the
    designator of the next ATS route segment}
22. • forall point. NOT (A change of {ATS route
    other than same direction lower/upper} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {next {point} } is defined by
geological co-ordinates OR insert {Item 15 C}
- { {point} followed by DCT}

                                                    1. report
                                                       error

--Test Frame 1.12:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. ATS flight track points are required by the
      appropriate ATS authority
   3. {point} and {point B} are successive points
   4. {point B} is defined by {bearing and distance}
   5. {point} is defined by {bearing and distance}
   6. NOT (insert {Item 15 C} - {DCT between {point}
      and {point B} } )
   7. • Aircraft Identification is correct
   8. • FlightRules and Type of Flight is correct
   9. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
  10. • Equipment is correct
  11. • Departure Aerodrome and time are correct
  12. • Mach number is prescribed by the appropriate
      ATS authority
  13. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
  14. • Flight is uncontrolled VFR
  15. • insert {Item 15 B} - {VFR}
  16. • Use ATS style track points
  17. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  18. • Other Information is correct
  19. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.12: (continued)
 ROIDs: I15C
 Stimuli Response
  20. • forall point. NOT ( {point} is listed in Item
      15 C) OR A significant point code designator
      has been assigned to {point} OR 2 figures
      describing latitude in degrees followed by

{S} followed by 3 figures describing longitude

in degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {S} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 2 figures

describing latitude in degrees followed by {N}
followed by 3 figures describing longitude in
degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {N} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 4 figures

describing latitude in degrees and tens of units
of minutes followed by {S} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{S} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR 4 figures
describing latitude in degrees and tens of units
of minutes followed by {N} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{N} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR the 2 or 3
character identification of the navigation aid
followed by the 3 figure bearing from the aid in
degrees magnetic followed by the distance from
the aid in 3 figures expressing nautical miles
is associated with {point}

--Test Frame 1.12: (continued)
 ROIDs: I15C
 Stimuli Response
  21. • forall point. A change of {flight rules} is
      planned at {point} OR A change of {level} is
      planned at {point} OR A change of {speed} is
      planned at {point} OR ATS flight track points
      are required by the appropriate ATS authority OR
      NOT (insert {Item 15 C} - { {point} details} )
      OR A change of {track} is planned at {point}
  22. • forall point. NOT ( {point} is listed in Item
      15 C) OR the code designator assigned to {route
      segment} including where appropriate the coded
      designator assigned to the standard {arrival}
      route is associated with {point} OR the code
      designator assigned to {route segment} including
      where appropriate the coded designator assigned
      to the standard {departure} route is associated
      with {point} OR the code designator assigned to

{route} including where appropriate the coded

designator assigned to the standard {arrival}
route is associated with {point} OR the code
designator assigned to {route} including where
appropriate the coded designator assigned to the
standard {departure} route is associated with

{point}

23. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR IFR to VFR OR NOT VFR
    to IFR OR the letters IFR are associated with

{point}

24. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A change of {level - climb}
    is planned at {point} ) OR an oblique stroke
    followed by the speed to be maintained during
    cruise climb followed by {the level above
    which cruise climb is planned followed by
    PLUS} is associated with {point} OR an oblique
    stroke followed by the speed to be maintained
    during cruise climb followed by {the two levels
    defining the layer to be occupied during cruide
    climb} is associated with {point}
25. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A significant point code
    designator has been assigned to {point} ) OR
    the 2 to 5 characters of the assigned coded
    designator is associated with {point}
26. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 0.01 Mach

or more} is planned at {point} )

--Test Frame 1.12: (continued)
 ROIDs: I15C
 Stimuli Response
  27. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR insert

{Item 15 C} - {DCT between {point} and {point B} } OR NOT ( {point B} is defined by {goegraphical

co-ordinates} ) OR NOT ( {point} is defined by

{goegraphical co-ordinates} )

28. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point

    B} } OR {point} is defined by {goegraphical
    co-ordinates}
29. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR NOT IFR to VFR OR the
    letters VFR are associated with {point}
30. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 5pc TAS or

    more} is planned at {point} )
31. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point B} } OR {point B} is defined by {goegraphical

    co-ordinates}
32. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point}
    is defined by {bearing and distance} OR insert

{Item 15 C} - { {point} followed by {point B} }

33. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point
    B} is defined by {bearing and distance} OR
    insert {Item 15 C} - { {point} followed by

{point B} }

--Test Frame 1.13:
 ROIDs: I15B
 Stimuli Response
   1. NOT Flight is uncontrolled VFR

   2. NOT (insert {Item 15 B} - {the planned cruising
      level for the first or the whole portion of the
      route to be flown as {A followed by 3 digits of
      Altitude in tens of metres} } )
   3. NOT (insert {Item 15 B} - {the planned cruising
      level for the first or the whole portion of the
      route to be flown as {S followed by 4 digits of
      Standard Metric Level in tens of metres} } )
   4. NOT (insert {Item 15 B} - {the planned cruising
      level for the first or the whole portion of the
      route to be flown as {F followed by 3 digits of
      Flight level} } )
   5. • Aircraft Identification is correct

   6. • FlightRules and Type of Flight is correct
   7. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   8. • Equipment is correct
   9. • Departure Aerodrome and time are correct
  10. • Mach number is prescribed by the appropriate
      ATS authority
  11. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }

  12. • The flight is along a designated ATS route
  13. • The departure aerodrome is {connected to} the
      ATS route
  14. • insert {Item 15 C} - {the designator of the
      first ATS route}
  15. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct

  16. • Other Information is correct
  17. • Supplementary Information is correct
  18. • forall point. NOT (A change of {ATS route
      other than same direction lower/upper} is
      planned at {point} ) OR NOT ( {next {point} }
      is defined by geological co-ordinates) OR NOT (

{point} is defined by geological co-ordinates)

OR insert {Item 15 C} - { {point} followed by
the designator of the next ATS route segment}

                                                    1. report
                                                       error

--Test Frame 1.13: (continued)
 ROIDs: I15B
 Stimuli Response
  19. • forall point. NOT (A change of {speed} is
      planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

    route) OR {point} is defined by geological
    co-ordinates OR insert {Item 15 C} - { {point}
    followed by DCT}
20. • forall point. NOT (A change of {level} is
    planned at {point} ) OR The flight to the {next

{point} } will be outside a designated route OR

    insert {Item 15 C} - { {point} followed by the
    designator of the next ATS route segment}
21. • forall point. NOT (A change of {ATS route
    other than same direction lower/upper} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {next {point} } is defined by
geological co-ordinates OR insert {Item 15 C}
- { {point} followed by DCT}

--Test Frame 1.14:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. {point} is listed in Item 15 C
   3. NOT (the code designator assigned to {route
      segment} including where appropriate the coded
      designator assigned to the standard {arrival}
      route is associated with {point} )
   4. NOT (the code designator assigned to {route
      segment} including where appropriate the coded
      designator assigned to the standard {departure}
      route is associated with {point} )
   5. NOT (the code designator assigned to {route}
      including where appropriate the coded designator
      assigned to the standard {arrival} route is
      associated with {point} )
   6. NOT (the code designator assigned to {route}
      including where appropriate the coded designator
      assigned to the standard {departure} route is
      associated with {point} )
   7. • Aircraft Identification is correct
   8. • FlightRules and Type of Flight is correct
   9. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
  10. • Equipment is correct
  11. • Departure Aerodrome and time are correct
  12. • Mach number is prescribed by the appropriate
      ATS authority
  13. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
  14. • Flight is uncontrolled VFR
  15. • insert {Item 15 B} - {VFR}
  16. • ATS flight track points are required by the
      appropriate ATS authority
  17. • Use ATS style track points
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct

                                                          1. report
                                                             error

--Test Frame 1.14: (continued)
 ROIDs: I15C
 Stimuli Response
  19. • Other Information is correct

  20. • Supplementary Information is correct
  21. • forall point. NOT ( {point} is listed in Item
      15 C) OR A significant point code designator
      has been assigned to {point} OR 2 figures
      describing latitude in degrees followed by

{S} followed by 3 figures describing longitude

in degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {S} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 2 figures

describing latitude in degrees followed by {N}
followed by 3 figures describing longitude in
degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {N} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 4 figures

describing latitude in degrees and tens of units
of minutes followed by {S} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{S} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR 4 figures
describing latitude in degrees and tens of units
of minutes followed by {N} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{N} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR the 2 or 3
character identification of the navigation aid
followed by the 3 figure bearing from the aid in
degrees magnetic followed by the distance from
the aid in 3 figures expressing nautical miles
is associated with {point}

--Test Frame 1.14: (continued)
 ROIDs: I15C
 Stimuli Response
  22. • forall point. A change of {flight rules} is
      planned at {point} OR A change of {level} is
      planned at {point} OR A change of {speed} is
      planned at {point} OR ATS flight track points
      are required by the appropriate ATS authority OR
      NOT (insert {Item 15 C} - { {point} details} )
      OR A change of {track} is planned at {point}
  23. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR NOT (

{point B} is defined by {bearing and distance}

) OR NOT ( {point} is defined by {bearing and
distance} ) OR insert {Item 15 C} - {DCT between

{point} and {point B} }

24. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR IFR to VFR OR NOT VFR
    to IFR OR the letters IFR are associated with

{point}

25. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A change of {level - climb}
    is planned at {point} ) OR an oblique stroke
    followed by the speed to be maintained during
    cruise climb followed by {the level above
    which cruise climb is planned followed by
    PLUS} is associated with {point} OR an oblique
    stroke followed by the speed to be maintained
    during cruise climb followed by {the two levels
    defining the layer to be occupied during cruide
    climb} is associated with {point}
26. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A significant point code
    designator has been assigned to {point} ) OR
    the 2 to 5 characters of the assigned coded
    designator is associated with {point}
27. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 0.01 Mach

    or more} is planned at {point} )
28. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - {DCT between {point} and {point B} } OR NOT ( {point B} is defined by {goegraphical

co-ordinates} ) OR NOT ( {point} is defined by

{goegraphical co-ordinates} )

--Test Frame 1.14: (continued)
 ROIDs: I15C
 Stimuli Response
  29. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point

    B} } OR {point} is defined by {goegraphical
    co-ordinates}

30. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR NOT IFR to VFR OR the
    letters VFR are associated with {point}
31. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 5pc TAS or

    more} is planned at {point} )

32. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point B} } OR {point B} is defined by {goegraphical

    co-ordinates}

33. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point}
    is defined by {bearing and distance} OR insert

{Item 15 C} - { {point} followed by {point B} }

34. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point
    B} is defined by {bearing and distance} OR
    insert {Item 15 C} - { {point} followed by

{point B} }

--Test Frame 1.15:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS route

   2. A change of {speed} is planned at {point}
   3. The flight to the {next {point} } will be
      outside a designated route
   4. NOT ( {point} is defined by geological
      co-ordinates)
   5. NOT (insert {Item 15 C} - { {point} followed by
      DCT} )
   6. • Aircraft Identification is correct
   7. • FlightRules and Type of Flight is correct
   8. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   9. • Equipment is correct
  10. • Departure Aerodrome and time are correct

  11. • Mach number is prescribed by the appropriate
      ATS authority

  12. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
  13. • Flight is uncontrolled VFR
  14. • insert {Item 15 B} - {VFR}
  15. • The departure aerodrome is {connected to} the
      ATS route
  16. • insert {Item 15 C} - {the designator of the
      first ATS route}
  17. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  18. • Other Information is correct

  19. • Supplementary Information is correct
  20. • forall point. NOT (A change of {ATS route
      other than same direction lower/upper} is
      planned at {point} ) OR NOT ( {next {point} }
      is defined by geological co-ordinates) OR NOT (

{point} is defined by geological co-ordinates)

    OR insert {Item 15 C} - { {point} followed by
    the designator of the next ATS route segment}
21. • forall point. NOT (A change of {level} is
    planned at {point} ) OR The flight to the {next

{point} } will be outside a designated route OR

    insert {Item 15 C} - { {point} followed by the
    designator of the next ATS route segment}
22. • forall point. NOT (A change of {ATS route
    other than same direction lower/upper} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {next {point} } is defined by
geological co-ordinates OR insert {Item 15 C}
- { {point} followed by DCT}

                                                    1. report
                                                       error

--Test Frame 1.16:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. A change of {flight rules} is planned at {point}
   3. {point} is listed in Item 15 C
   4. NOT IFR to VFR
   5. VFR to IFR
   6. NOT (the letters IFR are associated with {point}
      )
   7. • Aircraft Identification is correct
   8. • FlightRules and Type of Flight is correct
   9. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
  10. • Equipment is correct
  11. • Departure Aerodrome and time are correct
  12. • Mach number is prescribed by the appropriate
      ATS authority
  13. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
  14. • Flight is uncontrolled VFR
  15. • insert {Item 15 B} - {VFR}
  16. • ATS flight track points are required by the
      appropriate ATS authority
  17. • Use ATS style track points
  18. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  19. • Other Information is correct
  20. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.16: (continued)
 ROIDs: I15C
 Stimuli Response
  21. • forall point. NOT ( {point} is listed in Item
      15 C) OR A significant point code designator
      has been assigned to {point} OR 2 figures
      describing latitude in degrees followed by

{S} followed by 3 figures describing longitude

in degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {S} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 2 figures

describing latitude in degrees followed by {N}
followed by 3 figures describing longitude in
degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {N} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 4 figures

describing latitude in degrees and tens of units
of minutes followed by {S} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{S} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR 4 figures
describing latitude in degrees and tens of units
of minutes followed by {N} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{N} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR the 2 or 3
character identification of the navigation aid
followed by the 3 figure bearing from the aid in
degrees magnetic followed by the distance from
the aid in 3 figures expressing nautical miles
is associated with {point}

--Test Frame 1.16: (continued)
 ROIDs: I15C
 Stimuli Response
  22. • forall point. A change of {flight rules} is
      planned at {point} OR A change of {level} is
      planned at {point} OR A change of {speed} is
      planned at {point} OR ATS flight track points
      are required by the appropriate ATS authority OR
      NOT (insert {Item 15 C} - { {point} details} )
      OR A change of {track} is planned at {point}
  23. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR NOT (

{point B} is defined by {bearing and distance}

) OR NOT ( {point} is defined by {bearing and
distance} ) OR insert {Item 15 C} - {DCT between

{point} and {point B} }

24. • forall point. NOT ( {point} is listed in Item
    15 C) OR the code designator assigned to {route
    segment} including where appropriate the coded
    designator assigned to the standard {arrival}
    route is associated with {point} OR the code
    designator assigned to {route segment} including
    where appropriate the coded designator assigned
    to the standard {departure} route is associated
    with {point} OR the code designator assigned to

{route} including where appropriate the coded

designator assigned to the standard {arrival}
route is associated with {point} OR the code
designator assigned to {route} including where
appropriate the coded designator assigned to the
standard {departure} route is associated with

{point}

25. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A change of {level - climb}
    is planned at {point} ) OR an oblique stroke
    followed by the speed to be maintained during
    cruise climb followed by {the level above
    which cruise climb is planned followed by
    PLUS} is associated with {point} OR an oblique
    stroke followed by the speed to be maintained
    during cruise climb followed by {the two levels
    defining the layer to be occupied during cruide
    climb} is associated with {point}

26. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A significant point code
    designator has been assigned to {point} ) OR
    the 2 to 5 characters of the assigned coded
    designator is associated with {point}

--Test Frame 1.16: (continued)
 ROIDs: I15C
 Stimuli Response
  27. • forall point. NOT ( {point} is listed in Item
      15 C) OR an oblique stroke and both the cruising
      speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 0.01 Mach

    or more} is planned at {point} )

28. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - {DCT between {point} and {point B} } OR NOT ( {point B} is defined by {goegraphical

co-ordinates} ) OR NOT ( {point} is defined by

{goegraphical co-ordinates} )

29. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point

    B} } OR {point} is defined by {goegraphical
    co-ordinates}
30. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR NOT IFR to VFR OR the
    letters VFR are associated with {point}
31. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 5pc TAS or

    more} is planned at {point} )
32. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point B} } OR {point B} is defined by {goegraphical

    co-ordinates}
33. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point}
    is defined by {bearing and distance} OR insert

{Item 15 C} - { {point} followed by {point B} }

34. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point
    B} is defined by {bearing and distance} OR
    insert {Item 15 C} - { {point} followed by

{point B} }

--Test Frame 1.17:
 ROIDs: I15A
 Stimuli Response
   1. NOT Mach number is prescribed by the appropriate
      ATS authority
   2. NOT (insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {N followed by 4 digits of
      knots} } )

   3. NOT (insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {K followed by 4 digits of
      kilometres per hour} } )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • Equipment is correct

   8. • Departure Aerodrome and time are correct
   9. • Flight is uncontrolled VFR
  10. • insert {Item 15 B} - {VFR}
  11. • The flight is along a designated ATS route

  12. • The departure aerodrome is {connected to} the
      ATS route

  13. • insert {Item 15 C} - {the designator of the
      first ATS route}

  14. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  15. • Other Information is correct

  16. • Supplementary Information is correct
  17. • forall point. NOT (A change of {ATS route
      other than same direction lower/upper} is
      planned at {point} ) OR NOT ( {next {point} }
      is defined by geological co-ordinates) OR NOT (

{point} is defined by geological co-ordinates)

    OR insert {Item 15 C} - { {point} followed by
    the designator of the next ATS route segment}
18. • forall point. NOT (A change of {speed} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {point} is defined by geological
co-ordinates OR insert {Item 15 C} - { {point}
followed by DCT}

                                                    1. report
                                                       error

--Test Frame 1.17: (continued)
 ROIDs: I15A
 Stimuli Response
  19. • forall point. NOT (A change of {level} is
      planned at {point} ) OR The flight to the {next

{point} } will be outside a designated route OR

    insert {Item 15 C} - { {point} followed by the
    designator of the next ATS route segment}

20. • forall point. NOT (A change of {ATS route
    other than same direction lower/upper} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {next {point} } is defined by
geological co-ordinates OR insert {Item 15 C}
- { {point} followed by DCT}

--Test Frame 1.18:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS route

   2. NOT (The departure aerodrome is {connected to}
      the ATS route)

   3. NOT (The departure aerodrome is {located on} the
      ATS route)

   4. NOT (insert {Item 15 C} - {the letters DCT
      followed by the point of joining the first ATS
      route followed by the designator of the ATS
      route} )
   5. • Aircraft Identification is correct
   6. • FlightRules and Type of Flight is correct
   7. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   8. • Equipment is correct

   9. • Departure Aerodrome and time are correct
  10. • Mach number is prescribed by the appropriate
      ATS authority

  11. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
  12. • Flight is uncontrolled VFR
  13. • insert {Item 15 B} - {VFR}

  14. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  15. • Other Information is correct

  16. • Supplementary Information is correct
  17. • forall point. NOT (A change of {ATS route
      other than same direction lower/upper} is
      planned at {point} ) OR NOT ( {next {point} }
      is defined by geological co-ordinates) OR NOT (

{point} is defined by geological co-ordinates)

    OR insert {Item 15 C} - { {point} followed by
    the designator of the next ATS route segment}
18. • forall point. NOT (A change of {speed} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {point} is defined by geological
co-ordinates OR insert {Item 15 C} - { {point}
followed by DCT}

                                                    1. report
                                                       error

--Test Frame 1.18: (continued)
 ROIDs: I15C
 Stimuli Response
  19. • forall point. NOT (A change of {level} is
      planned at {point} ) OR The flight to the {next

{point} } will be outside a designated route OR

    insert {Item 15 C} - { {point} followed by the
    designator of the next ATS route segment}

20. • forall point. NOT (A change of {ATS route
    other than same direction lower/upper} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {next {point} } is defined by
geological co-ordinates OR insert {Item 15 C}
- { {point} followed by DCT}

--Test Frame 1.19:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. {point} is listed in Item 15 C
   3. A change of {level - climb} is planned at

{point}

4. NOT (an oblique stroke followed by the speed to
   be maintained during cruise climb followed by

{the level above which cruise climb is planned

   followed by PLUS} is associated with {point} )
5. NOT (an oblique stroke followed by the speed
   to be maintained during cruise climb followed
   by {the two levels defining the layer to be
   occupied during cruide climb} is associated with

{point} )

 6. • Aircraft Identification is correct
 7. • FlightRules and Type of Flight is correct
 8. • Number and Type of Aircraft and Wake
    Turbulence Category is correct
 9. • Equipment is correct
10. • Departure Aerodrome and time are correct
11. • Mach number is prescribed by the appropriate
    ATS authority
12. • insert {Item 15 A} - {the true airspeed for
    the first or the whole cruising portion of the
    flight expressed as {M followed by 3 digits of
    Mach hundredths} }
13. • Flight is uncontrolled VFR
14. • insert {Item 15 B} - {VFR}
15. • ATS flight track points are required by the
    appropriate ATS authority
16. • Use ATS style track points
17. • Destination Aerodrome and Total Estimated
    Elapsed Time is correct
18. • Other Information is correct
19. • Supplementary Information is correct

                                                        1. report
                                                           error

--Test Frame 1.19: (continued)
 ROIDs: I15C
 Stimuli Response
  20. • forall point. NOT ( {point} is listed in Item
      15 C) OR A significant point code designator
      has been assigned to {point} OR 2 figures
      describing latitude in degrees followed by

{S} followed by 3 figures describing longitude

in degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {S} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 2 figures

describing latitude in degrees followed by {N}
followed by 3 figures describing longitude in
degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {N} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 4 figures

describing latitude in degrees and tens of units
of minutes followed by {S} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{S} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR 4 figures
describing latitude in degrees and tens of units
of minutes followed by {N} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{N} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR the 2 or 3
character identification of the navigation aid
followed by the 3 figure bearing from the aid in
degrees magnetic followed by the distance from
the aid in 3 figures expressing nautical miles
is associated with {point}

--Test Frame 1.19: (continued)
 ROIDs: I15C
 Stimuli Response
  21. • forall point. A change of {flight rules} is
      planned at {point} OR A change of {level} is
      planned at {point} OR A change of {speed} is
      planned at {point} OR ATS flight track points
      are required by the appropriate ATS authority OR
      NOT (insert {Item 15 C} - { {point} details} )
      OR A change of {track} is planned at {point}
  22. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR NOT (

{point B} is defined by {bearing and distance}

) OR NOT ( {point} is defined by {bearing and
distance} ) OR insert {Item 15 C} - {DCT between

{point} and {point B} }

23. • forall point. NOT ( {point} is listed in Item
    15 C) OR the code designator assigned to {route
    segment} including where appropriate the coded
    designator assigned to the standard {arrival}
    route is associated with {point} OR the code
    designator assigned to {route segment} including
    where appropriate the coded designator assigned
    to the standard {departure} route is associated
    with {point} OR the code designator assigned to

{route} including where appropriate the coded

designator assigned to the standard {arrival}
route is associated with {point} OR the code
designator assigned to {route} including where
appropriate the coded designator assigned to the
standard {departure} route is associated with

{point}

24. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR IFR to VFR OR NOT VFR
    to IFR OR the letters IFR are associated with

{point}

25. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A significant point code
    designator has been assigned to {point} ) OR
    the 2 to 5 characters of the assigned coded
    designator is associated with {point}
26. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 0.01 Mach

or more} is planned at {point} )

--Test Frame 1.19: (continued)
 ROIDs: I15C
 Stimuli Response
  27. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR insert

{Item 15 C} - {DCT between {point} and {point B} } OR NOT ( {point B} is defined by {goegraphical

co-ordinates} ) OR NOT ( {point} is defined by

{goegraphical co-ordinates} )

28. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point

    B} } OR {point} is defined by {goegraphical
    co-ordinates}
29. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR NOT IFR to VFR OR the
    letters VFR are associated with {point}
30. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 5pc TAS or

    more} is planned at {point} )
31. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point B} } OR {point B} is defined by {goegraphical

    co-ordinates}
32. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point}
    is defined by {bearing and distance} OR insert

{Item 15 C} - { {point} followed by {point B} }

33. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point
    B} is defined by {bearing and distance} OR
    insert {Item 15 C} - { {point} followed by

{point B} }

--Test Frame 1.20:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. NOT ATS flight track points are required by the
      appropriate ATS authority
   3. NOT (insert {Item 15 C} - { {point} details} )
   4. NOT ( {point} and {next {point} } are normally
      more than {30 minutes flying time} apart)
   5. A change of {track} is planned at {point}
   6. • Aircraft Identification is correct
   7. • FlightRules and Type of Flight is correct
   8. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   9. • Equipment is correct
  10. • Departure Aerodrome and time are correct
  11. • Mach number is prescribed by the appropriate
      ATS authority
  12. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
  13. • Flight is uncontrolled VFR
  14. • insert {Item 15 B} - {VFR}
  15. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  16. • Other Information is correct
  17. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.20: (continued)
 ROIDs: I15C
 Stimuli Response
  18. • forall point. NOT ( {point} is listed in Item
      15 C) OR A significant point code designator
      has been assigned to {point} OR 2 figures
      describing latitude in degrees followed by

{S} followed by 3 figures describing longitude

in degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {S} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 2 figures

describing latitude in degrees followed by {N}
followed by 3 figures describing longitude in
degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {N} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 4 figures

describing latitude in degrees and tens of units
of minutes followed by {S} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{S} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR 4 figures
describing latitude in degrees and tens of units
of minutes followed by {N} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{N} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR the 2 or 3
character identification of the navigation aid
followed by the 3 figure bearing from the aid in
degrees magnetic followed by the distance from
the aid in 3 figures expressing nautical miles
is associated with {point}

--Test Frame 1.20: (continued)
 ROIDs: I15C
 Stimuli Response
  19. • forall point. A change of {flight rules} is
      planned at {point} OR A change of {level} is
      planned at {point} OR A change of {speed} is
      planned at {point} OR ATS flight track points
      are required by the appropriate ATS authority OR
      NOT (insert {Item 15 C} - { {point} details} )
      OR A change of {track} is planned at {point}
  20. • forall point. NOT ( {point} is listed in Item
      15 C) OR the code designator assigned to {route
      segment} including where appropriate the coded
      designator assigned to the standard {arrival}
      route is associated with {point} OR the code
      designator assigned to {route segment} including
      where appropriate the coded designator assigned
      to the standard {departure} route is associated
      with {point} OR the code designator assigned to

{route} including where appropriate the coded

designator assigned to the standard {arrival}
route is associated with {point} OR the code
designator assigned to {route} including where
appropriate the coded designator assigned to the
standard {departure} route is associated with

{point}

21. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR IFR to VFR OR NOT VFR
    to IFR OR the letters IFR are associated with

{point}

22. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A change of {level - climb}
    is planned at {point} ) OR an oblique stroke
    followed by the speed to be maintained during
    cruise climb followed by {the level above
    which cruise climb is planned followed by
    PLUS} is associated with {point} OR an oblique
    stroke followed by the speed to be maintained
    during cruise climb followed by {the two levels
    defining the layer to be occupied during cruide
    climb} is associated with {point}
23. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A significant point code
    designator has been assigned to {point} ) OR
    the 2 to 5 characters of the assigned coded
    designator is associated with {point}

--Test Frame 1.20: (continued)
 ROIDs: I15C
 Stimuli Response
  24. • forall point. NOT ( {point} is listed in Item
      15 C) OR an oblique stroke and both the cruising
      speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 0.01 Mach

    or more} is planned at {point} )

25. • forall point. NOT (insert {Item 15 C} -

{ {point} details} ) OR NOT ( {point} and {next {point} } are normally more than {370km}

    apart) OR NOT ( {point} and {next {point} } are
    normally more than {30 minutes flying time}
    apart)
26. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR NOT IFR to VFR OR the
    letters VFR are associated with {point}
27. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 5pc TAS or

    more} is planned at {point} )
28. • forall point. insert {Item 15 C} - { {point}
    details} OR {point} and {next {point} } are
    normally more than {370km} apart OR NOT (A
    change of {track} is planned at {point} )

--Test Frame 1.21:
 ROIDs: I15B
 Stimuli Response
   1. Flight is uncontrolled VFR

   2. NOT (insert {Item 15 B} - {VFR} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct

   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct

   7. • Departure Aerodrome and time are correct
   8. • Mach number is prescribed by the appropriate
      ATS authority
   9. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
  10. • The flight is along a designated ATS route
  11. • The departure aerodrome is {connected to} the
      ATS route
  12. • insert {Item 15 C} - {the designator of the
      first ATS route}
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct

  16. • forall point. NOT (A change of {ATS route
      other than same direction lower/upper} is
      planned at {point} ) OR NOT ( {next {point} }
      is defined by geological co-ordinates) OR NOT (

{point} is defined by geological co-ordinates)

    OR insert {Item 15 C} - { {point} followed by
    the designator of the next ATS route segment}
17. • forall point. NOT (A change of {speed} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

    route) OR {point} is defined by geological
    co-ordinates OR insert {Item 15 C} - { {point}
    followed by DCT}

18. • forall point. NOT (A change of {level} is
    planned at {point} ) OR The flight to the {next

{point} } will be outside a designated route OR

    insert {Item 15 C} - { {point} followed by the
    designator of the next ATS route segment}
19. • forall point. NOT (A change of {ATS route
    other than same direction lower/upper} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {next {point} } is defined by
geological co-ordinates OR insert {Item 15 C}
- { {point} followed by DCT}

                                                    1. report
                                                       error

--Test Frame 1.22:
 ROIDs: I15A
 Stimuli Response
   1. Mach number is prescribed by the appropriate ATS
      authority
   2. NOT (insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} } )

   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct

   8. • Flight is uncontrolled VFR
   9. • insert {Item 15 B} - {VFR}
  10. • The flight is along a designated ATS route
  11. • The departure aerodrome is {connected to} the
      ATS route
  12. • insert {Item 15 C} - {the designator of the
      first ATS route}
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct

  16. • forall point. NOT (A change of {ATS route
      other than same direction lower/upper} is
      planned at {point} ) OR NOT ( {next {point} }
      is defined by geological co-ordinates) OR NOT (

{point} is defined by geological co-ordinates)

    OR insert {Item 15 C} - { {point} followed by
    the designator of the next ATS route segment}
17. • forall point. NOT (A change of {speed} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

    route) OR {point} is defined by geological
    co-ordinates OR insert {Item 15 C} - { {point}
    followed by DCT}

18. • forall point. NOT (A change of {level} is
    planned at {point} ) OR The flight to the {next

{point} } will be outside a designated route OR

    insert {Item 15 C} - { {point} followed by the
    designator of the next ATS route segment}
19. • forall point. NOT (A change of {ATS route
    other than same direction lower/upper} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {next {point} } is defined by
geological co-ordinates OR insert {Item 15 C}
- { {point} followed by DCT}

                                                    1. report
                                                       error

--Test Frame 1.23:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS route

   2. The departure aerodrome is {connected to} the
      ATS route

   3. NOT (insert {Item 15 C} - {the designator of the
      first ATS route} )

   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • Equipment is correct
   8. • Departure Aerodrome and time are correct

   9. • Mach number is prescribed by the appropriate
      ATS authority
  10. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }

  11. • Flight is uncontrolled VFR
  12. • insert {Item 15 B} - {VFR}
  13. • NOT (The departure aerodrome is {located on}
      the ATS route)
  14. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  15. • Other Information is correct
  16. • Supplementary Information is correct

  17. • forall point. NOT (A change of {ATS route
      other than same direction lower/upper} is
      planned at {point} ) OR NOT ( {next {point} }
      is defined by geological co-ordinates) OR NOT (

{point} is defined by geological co-ordinates)

    OR insert {Item 15 C} - { {point} followed by
    the designator of the next ATS route segment}
18. • forall point. NOT (A change of {speed} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

    route) OR {point} is defined by geological
    co-ordinates OR insert {Item 15 C} - { {point}
    followed by DCT}
19. • forall point. NOT (A change of {level} is
    planned at {point} ) OR The flight to the {next

{point} } will be outside a designated route OR

    insert {Item 15 C} - { {point} followed by the
    designator of the next ATS route segment}
20. • forall point. NOT (A change of {ATS route
    other than same direction lower/upper} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {next {point} } is defined by
geological co-ordinates OR insert {Item 15 C}
- { {point} followed by DCT}

                                                    1. report
                                                       error

--Test Frame 1.24:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. {point} is listed in Item 15 C
   3. A significant point code designator has been
      assigned to {point}
   4. NOT (the 2 to 5 characters of the assigned coded
      designator is associated with {point} )
   5. • Aircraft Identification is correct
   6. • FlightRules and Type of Flight is correct
   7. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   8. • Equipment is correct
   9. • Departure Aerodrome and time are correct
  10. • Mach number is prescribed by the appropriate
      ATS authority
  11. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
  12. • Flight is uncontrolled VFR
  13. • insert {Item 15 B} - {VFR}
  14. • ATS flight track points are required by the
      appropriate ATS authority
  15. • Use ATS style track points
  16. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  17. • Other Information is correct
  18. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.24: (continued)
 ROIDs: I15C
 Stimuli Response
  19. • forall point. NOT ( {point} is listed in Item
      15 C) OR A significant point code designator
      has been assigned to {point} OR 2 figures
      describing latitude in degrees followed by

{S} followed by 3 figures describing longitude

in degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {S} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 2 figures

describing latitude in degrees followed by {N}
followed by 3 figures describing longitude in
degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {N} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 4 figures

describing latitude in degrees and tens of units
of minutes followed by {S} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{S} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR 4 figures
describing latitude in degrees and tens of units
of minutes followed by {N} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{N} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR the 2 or 3
character identification of the navigation aid
followed by the 3 figure bearing from the aid in
degrees magnetic followed by the distance from
the aid in 3 figures expressing nautical miles
is associated with {point}

--Test Frame 1.24: (continued)
 ROIDs: I15C
 Stimuli Response
  20. • forall point. A change of {flight rules} is
      planned at {point} OR A change of {level} is
      planned at {point} OR A change of {speed} is
      planned at {point} OR ATS flight track points
      are required by the appropriate ATS authority OR
      NOT (insert {Item 15 C} - { {point} details} )
      OR A change of {track} is planned at {point}
  21. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR NOT (

{point B} is defined by {bearing and distance}

) OR NOT ( {point} is defined by {bearing and
distance} ) OR insert {Item 15 C} - {DCT between

{point} and {point B} }

22. • forall point. NOT ( {point} is listed in Item
    15 C) OR the code designator assigned to {route
    segment} including where appropriate the coded
    designator assigned to the standard {arrival}
    route is associated with {point} OR the code
    designator assigned to {route segment} including
    where appropriate the coded designator assigned
    to the standard {departure} route is associated
    with {point} OR the code designator assigned to

{route} including where appropriate the coded

designator assigned to the standard {arrival}
route is associated with {point} OR the code
designator assigned to {route} including where
appropriate the coded designator assigned to the
standard {departure} route is associated with

{point}

23. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR IFR to VFR OR NOT VFR
    to IFR OR the letters IFR are associated with

{point}

24. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A change of {level - climb}
    is planned at {point} ) OR an oblique stroke
    followed by the speed to be maintained during
    cruise climb followed by {the level above
    which cruise climb is planned followed by
    PLUS} is associated with {point} OR an oblique
    stroke followed by the speed to be maintained
    during cruise climb followed by {the two levels
    defining the layer to be occupied during cruide
    climb} is associated with {point}

--Test Frame 1.24: (continued)
 ROIDs: I15C
 Stimuli Response
  25. • forall point. NOT ( {point} is listed in Item
      15 C) OR an oblique stroke and both the cruising
      speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 0.01 Mach

    or more} is planned at {point} )

26. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - {DCT between {point} and {point B} } OR NOT ( {point B} is defined by {goegraphical

co-ordinates} ) OR NOT ( {point} is defined by

{goegraphical co-ordinates} )

27. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point

    B} } OR {point} is defined by {goegraphical
    co-ordinates}
28. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR NOT IFR to VFR OR the
    letters VFR are associated with {point}
29. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 5pc TAS or

    more} is planned at {point} )
30. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point B} } OR {point B} is defined by {goegraphical

    co-ordinates}
31. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point}
    is defined by {bearing and distance} OR insert

{Item 15 C} - { {point} followed by {point B} }

32. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point
    B} is defined by {bearing and distance} OR
    insert {Item 15 C} - { {point} followed by

{point B} }

--Test Frame 1.25:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS route

   2. A change of {level} is planned at {point}
   3. NOT (The flight to the {next {point} } will be
      outside a designated route)
   4. NOT (insert {Item 15 C} - { {point} followed by
      the designator of the next ATS route segment} )
   5. • Aircraft Identification is correct
   6. • FlightRules and Type of Flight is correct
   7. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   8. • Equipment is correct

   9. • Departure Aerodrome and time are correct
  10. • Mach number is prescribed by the appropriate
      ATS authority

  11. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
  12. • Flight is uncontrolled VFR
  13. • insert {Item 15 B} - {VFR}

  14. • The departure aerodrome is {connected to} the
      ATS route
  15. • insert {Item 15 C} - {the designator of the
      first ATS route}
  16. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  17. • Other Information is correct

  18. • Supplementary Information is correct
  19. • forall point. NOT (A change of {ATS route
      other than same direction lower/upper} is
      planned at {point} ) OR NOT ( {next {point} }
      is defined by geological co-ordinates) OR NOT (

{point} is defined by geological co-ordinates)

    OR insert {Item 15 C} - { {point} followed by
    the designator of the next ATS route segment}
20. • forall point. NOT (A change of {speed} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

    route) OR {point} is defined by geological
    co-ordinates OR insert {Item 15 C} - { {point}
    followed by DCT}

21. • forall point. NOT (A change of {ATS route
    other than same direction lower/upper} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {next {point} } is defined by
geological co-ordinates OR insert {Item 15 C}
- { {point} followed by DCT}

                                                    1. report
                                                       error

--Test Frame 1.26:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. {point} is listed in Item 15 C
   3. NOT (an oblique stroke and both the cruising
      speed and the cruising level is associated with

{point} )

 4. A change of {speed - 0.01 Mach or more} is
    planned at {point}
 5. • Aircraft Identification is correct
 6. • FlightRules and Type of Flight is correct
 7. • Number and Type of Aircraft and Wake
    Turbulence Category is correct
 8. • Equipment is correct
 9. • Departure Aerodrome and time are correct
10. • Mach number is prescribed by the appropriate
    ATS authority
11. • insert {Item 15 A} - {the true airspeed for
    the first or the whole cruising portion of the
    flight expressed as {M followed by 3 digits of
    Mach hundredths} }
12. • Flight is uncontrolled VFR
13. • insert {Item 15 B} - {VFR}
14. • ATS flight track points are required by the
    appropriate ATS authority
15. • Use ATS style track points
16. • Destination Aerodrome and Total Estimated
    Elapsed Time is correct
17. • Other Information is correct
18. • Supplementary Information is correct

                                                        1. report
                                                           error

--Test Frame 1.26: (continued)
 ROIDs: I15C
 Stimuli Response
  19. • forall point. NOT ( {point} is listed in Item
      15 C) OR A significant point code designator
      has been assigned to {point} OR 2 figures
      describing latitude in degrees followed by

{S} followed by 3 figures describing longitude

in degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {S} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 2 figures

describing latitude in degrees followed by {N}
followed by 3 figures describing longitude in
degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {N} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 4 figures

describing latitude in degrees and tens of units
of minutes followed by {S} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{S} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR 4 figures
describing latitude in degrees and tens of units
of minutes followed by {N} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{N} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR the 2 or 3
character identification of the navigation aid
followed by the 3 figure bearing from the aid in
degrees magnetic followed by the distance from
the aid in 3 figures expressing nautical miles
is associated with {point}

--Test Frame 1.26: (continued)
 ROIDs: I15C
 Stimuli Response
  20. • forall point. A change of {flight rules} is
      planned at {point} OR A change of {level} is
      planned at {point} OR A change of {speed} is
      planned at {point} OR ATS flight track points
      are required by the appropriate ATS authority OR
      NOT (insert {Item 15 C} - { {point} details} )
      OR A change of {track} is planned at {point}
  21. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR NOT (

{point B} is defined by {bearing and distance}

) OR NOT ( {point} is defined by {bearing and
distance} ) OR insert {Item 15 C} - {DCT between

{point} and {point B} }

22. • forall point. NOT ( {point} is listed in Item
    15 C) OR the code designator assigned to {route
    segment} including where appropriate the coded
    designator assigned to the standard {arrival}
    route is associated with {point} OR the code
    designator assigned to {route segment} including
    where appropriate the coded designator assigned
    to the standard {departure} route is associated
    with {point} OR the code designator assigned to

{route} including where appropriate the coded

designator assigned to the standard {arrival}
route is associated with {point} OR the code
designator assigned to {route} including where
appropriate the coded designator assigned to the
standard {departure} route is associated with

{point}

23. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR IFR to VFR OR NOT VFR
    to IFR OR the letters IFR are associated with

{point}

24. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A change of {level - climb}
    is planned at {point} ) OR an oblique stroke
    followed by the speed to be maintained during
    cruise climb followed by {the level above
    which cruise climb is planned followed by
    PLUS} is associated with {point} OR an oblique
    stroke followed by the speed to be maintained
    during cruise climb followed by {the two levels
    defining the layer to be occupied during cruide
    climb} is associated with {point}

--Test Frame 1.26: (continued)
 ROIDs: I15C
 Stimuli Response
  25. • forall point. NOT ( {point} is listed in
      Item 15 C) OR NOT (A significant point code
      designator has been assigned to {point} ) OR
      the 2 to 5 characters of the assigned coded
      designator is associated with {point}

  26. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR insert

{Item 15 C} - {DCT between {point} and {point B} } OR NOT ( {point B} is defined by {goegraphical

co-ordinates} ) OR NOT ( {point} is defined by

{goegraphical co-ordinates} )

27. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point

    B} } OR {point} is defined by {goegraphical
    co-ordinates}
28. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR NOT IFR to VFR OR the
    letters VFR are associated with {point}
29. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 5pc TAS or

    more} is planned at {point} )
30. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point B} } OR {point B} is defined by {goegraphical

    co-ordinates}
31. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point}
    is defined by {bearing and distance} OR insert

{Item 15 C} - { {point} followed by {point B} }

32. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point
    B} is defined by {bearing and distance} OR
    insert {Item 15 C} - { {point} followed by

{point B} }

--Test Frame 1.27:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. NOT ATS flight track points are required by the
      appropriate ATS authority
   3. insert {Item 15 C} - { {point} details}
   4. {point} and {next {point} } are normally more
      than {370km} apart
   5. {point} and {next {point} } are normally more
      than {30 minutes flying time} apart
   6. • Aircraft Identification is correct
   7. • FlightRules and Type of Flight is correct
   8. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   9. • Equipment is correct
  10. • Departure Aerodrome and time are correct
  11. • Mach number is prescribed by the appropriate
      ATS authority
  12. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
  13. • Flight is uncontrolled VFR
  14. • insert {Item 15 B} - {VFR}
  15. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  16. • Other Information is correct
  17. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.27: (continued)
 ROIDs: I15C
 Stimuli Response
  18. • forall point. NOT ( {point} is listed in Item
      15 C) OR A significant point code designator
      has been assigned to {point} OR 2 figures
      describing latitude in degrees followed by

{S} followed by 3 figures describing longitude

in degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {S} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 2 figures

describing latitude in degrees followed by {N}
followed by 3 figures describing longitude in
degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {N} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 4 figures

describing latitude in degrees and tens of units
of minutes followed by {S} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{S} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR 4 figures
describing latitude in degrees and tens of units
of minutes followed by {N} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{N} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR the 2 or 3
character identification of the navigation aid
followed by the 3 figure bearing from the aid in
degrees magnetic followed by the distance from
the aid in 3 figures expressing nautical miles
is associated with {point}

--Test Frame 1.27: (continued)
 ROIDs: I15C
 Stimuli Response
  19. • forall point. A change of {flight rules} is
      planned at {point} OR A change of {level} is
      planned at {point} OR A change of {speed} is
      planned at {point} OR ATS flight track points
      are required by the appropriate ATS authority OR
      NOT (insert {Item 15 C} - { {point} details} )
      OR A change of {track} is planned at {point}
  20. • forall point. NOT ( {point} is listed in Item
      15 C) OR the code designator assigned to {route
      segment} including where appropriate the coded
      designator assigned to the standard {arrival}
      route is associated with {point} OR the code
      designator assigned to {route segment} including
      where appropriate the coded designator assigned
      to the standard {departure} route is associated
      with {point} OR the code designator assigned to

{route} including where appropriate the coded

designator assigned to the standard {arrival}
route is associated with {point} OR the code
designator assigned to {route} including where
appropriate the coded designator assigned to the
standard {departure} route is associated with

{point}

21. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR IFR to VFR OR NOT VFR
    to IFR OR the letters IFR are associated with

{point}

22. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A change of {level - climb}
    is planned at {point} ) OR an oblique stroke
    followed by the speed to be maintained during
    cruise climb followed by {the level above
    which cruise climb is planned followed by
    PLUS} is associated with {point} OR an oblique
    stroke followed by the speed to be maintained
    during cruise climb followed by {the two levels
    defining the layer to be occupied during cruide
    climb} is associated with {point}

--Test Frame 1.27: (continued)
 ROIDs: I15C
 Stimuli Response
  24. • forall point. insert {Item 15 C} - { {point}
      details} OR {point} and {next {point} } are
      normally more than {30 minutes flying time}
      apart OR NOT (A change of {track} is planned at

{point} )

25. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A significant point code
    designator has been assigned to {point} ) OR
    the 2 to 5 characters of the assigned coded
    designator is associated with {point}
26. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 0.01 Mach

    or more} is planned at {point} )
27. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR NOT IFR to VFR OR the
    letters VFR are associated with {point}

28. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 5pc TAS or

    more} is planned at {point} )

29. • forall point. insert {Item 15 C} - { {point}
    details} OR {point} and {next {point} } are
    normally more than {370km} apart OR NOT (A
    change of {track} is planned at {point} )

--Test Frame 1.28:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. ATS flight track points are required by the
      appropriate ATS authority
   3. {point} and {point B} are successive points
   4. NOT (insert {Item 15 C} - {DCT between {point}
      and {point B} } )
   5. {point B} is defined by {goegraphical
      co-ordinates}
   6. {point} is defined by {goegraphical
      co-ordinates}
   7. • Aircraft Identification is correct
   8. • FlightRules and Type of Flight is correct
   9. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
  10. • Equipment is correct
  11. • Departure Aerodrome and time are correct
  12. • Mach number is prescribed by the appropriate
      ATS authority
  13. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
  14. • Flight is uncontrolled VFR
  15. • insert {Item 15 B} - {VFR}
  16. • Use ATS style track points
  17. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  18. • Other Information is correct
  19. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.28: (continued)
 ROIDs: I15C
 Stimuli Response
  20. • forall point. NOT ( {point} is listed in Item
      15 C) OR A significant point code designator
      has been assigned to {point} OR 2 figures
      describing latitude in degrees followed by

{S} followed by 3 figures describing longitude

in degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {S} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 2 figures

describing latitude in degrees followed by {N}
followed by 3 figures describing longitude in
degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {N} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 4 figures

describing latitude in degrees and tens of units
of minutes followed by {S} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{S} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR 4 figures
describing latitude in degrees and tens of units
of minutes followed by {N} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{N} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR the 2 or 3
character identification of the navigation aid
followed by the 3 figure bearing from the aid in
degrees magnetic followed by the distance from
the aid in 3 figures expressing nautical miles
is associated with {point}

--Test Frame 1.28: (continued)
 ROIDs: I15C
 Stimuli Response
  21. • forall point. A change of {flight rules} is
      planned at {point} OR A change of {level} is
      planned at {point} OR A change of {speed} is
      planned at {point} OR ATS flight track points
      are required by the appropriate ATS authority OR
      NOT (insert {Item 15 C} - { {point} details} )
      OR A change of {track} is planned at {point}
  22. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR NOT (

{point B} is defined by {bearing and distance}

) OR NOT ( {point} is defined by {bearing and
distance} ) OR insert {Item 15 C} - {DCT between

{point} and {point B} }

23. • forall point. NOT ( {point} is listed in Item
    15 C) OR the code designator assigned to {route
    segment} including where appropriate the coded
    designator assigned to the standard {arrival}
    route is associated with {point} OR the code
    designator assigned to {route segment} including
    where appropriate the coded designator assigned
    to the standard {departure} route is associated
    with {point} OR the code designator assigned to

{route} including where appropriate the coded

designator assigned to the standard {arrival}
route is associated with {point} OR the code
designator assigned to {route} including where
appropriate the coded designator assigned to the
standard {departure} route is associated with

{point}

24. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR IFR to VFR OR NOT VFR
    to IFR OR the letters IFR are associated with

{point}

25. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A change of {level - climb}
    is planned at {point} ) OR an oblique stroke
    followed by the speed to be maintained during
    cruise climb followed by {the level above
    which cruise climb is planned followed by
    PLUS} is associated with {point} OR an oblique
    stroke followed by the speed to be maintained
    during cruise climb followed by {the two levels
    defining the layer to be occupied during cruide
    climb} is associated with {point}

--Test Frame 1.28: (continued)
 ROIDs: I15C
 Stimuli Response
  26. • forall point. NOT ( {point} is listed in
      Item 15 C) OR NOT (A significant point code
      designator has been assigned to {point} ) OR
      the 2 to 5 characters of the assigned coded
      designator is associated with {point}

  27. • forall point. NOT ( {point} is listed in Item
      15 C) OR an oblique stroke and both the cruising
      speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 0.01 Mach

    or more} is planned at {point} )
28. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point

    B} } OR {point} is defined by {goegraphical
    co-ordinates}
29. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR NOT IFR to VFR OR the
    letters VFR are associated with {point}

30. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 5pc TAS or

    more} is planned at {point} )

31. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point B} } OR {point B} is defined by {goegraphical

    co-ordinates}
32. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point}
    is defined by {bearing and distance} OR insert

{Item 15 C} - { {point} followed by {point B} }

33. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point
    B} is defined by {bearing and distance} OR
    insert {Item 15 C} - { {point} followed by

{point B} }

--Test Frame 1.29:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. ATS flight track points are required by the
      appropriate ATS authority
   3. {point} and {point B} are successive points
   4. NOT (insert {Item 15 C} - { {point} followed by

{point B} } )

 5. NOT ( {point} is defined by {goegraphical
    co-ordinates} )
 6. • Aircraft Identification is correct
 7. • FlightRules and Type of Flight is correct
 8. • Number and Type of Aircraft and Wake
    Turbulence Category is correct
 9. • Equipment is correct
10. • Departure Aerodrome and time are correct
11. • Mach number is prescribed by the appropriate
    ATS authority
12. • insert {Item 15 A} - {the true airspeed for
    the first or the whole cruising portion of the
    flight expressed as {M followed by 3 digits of
    Mach hundredths} }
13. • Flight is uncontrolled VFR
14. • insert {Item 15 B} - {VFR}
15. • Use ATS style track points
16. • Destination Aerodrome and Total Estimated
    Elapsed Time is correct
17. • Other Information is correct
18. • Supplementary Information is correct

                                                        1. report
                                                           error

--Test Frame 1.29: (continued)
 ROIDs: I15C
 Stimuli Response
  19. • forall point. NOT ( {point} is listed in Item
      15 C) OR A significant point code designator
      has been assigned to {point} OR 2 figures
      describing latitude in degrees followed by

{S} followed by 3 figures describing longitude

in degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {S} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 2 figures

describing latitude in degrees followed by {N}
followed by 3 figures describing longitude in
degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {N} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 4 figures

describing latitude in degrees and tens of units
of minutes followed by {S} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{S} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR 4 figures
describing latitude in degrees and tens of units
of minutes followed by {N} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{N} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR the 2 or 3
character identification of the navigation aid
followed by the 3 figure bearing from the aid in
degrees magnetic followed by the distance from
the aid in 3 figures expressing nautical miles
is associated with {point}

--Test Frame 1.29: (continued)
 ROIDs: I15C
 Stimuli Response
  20. • forall point. A change of {flight rules} is
      planned at {point} OR A change of {level} is
      planned at {point} OR A change of {speed} is
      planned at {point} OR ATS flight track points
      are required by the appropriate ATS authority OR
      NOT (insert {Item 15 C} - { {point} details} )
      OR A change of {track} is planned at {point}
  21. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR NOT (

{point B} is defined by {bearing and distance}

) OR NOT ( {point} is defined by {bearing and
distance} ) OR insert {Item 15 C} - {DCT between

{point} and {point B} }

22. • forall point. NOT ( {point} is listed in Item
    15 C) OR the code designator assigned to {route
    segment} including where appropriate the coded
    designator assigned to the standard {arrival}
    route is associated with {point} OR the code
    designator assigned to {route segment} including
    where appropriate the coded designator assigned
    to the standard {departure} route is associated
    with {point} OR the code designator assigned to

{route} including where appropriate the coded

designator assigned to the standard {arrival}
route is associated with {point} OR the code
designator assigned to {route} including where
appropriate the coded designator assigned to the
standard {departure} route is associated with

{point}

23. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR IFR to VFR OR NOT VFR
    to IFR OR the letters IFR are associated with

{point}

24. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A change of {level - climb}
    is planned at {point} ) OR an oblique stroke
    followed by the speed to be maintained during
    cruise climb followed by {the level above
    which cruise climb is planned followed by
    PLUS} is associated with {point} OR an oblique
    stroke followed by the speed to be maintained
    during cruise climb followed by {the two levels
    defining the layer to be occupied during cruide
    climb} is associated with {point}

--Test Frame 1.29: (continued)
 ROIDs: I15C
 Stimuli Response
  25. • forall point. NOT ( {point} is listed in
      Item 15 C) OR NOT (A significant point code
      designator has been assigned to {point} ) OR
      the 2 to 5 characters of the assigned coded
      designator is associated with {point}

  26. • forall point. NOT ( {point} is listed in Item
      15 C) OR an oblique stroke and both the cruising
      speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 0.01 Mach

    or more} is planned at {point} )
27. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - {DCT between {point} and {point B} } OR NOT ( {point B} is defined by {goegraphical

co-ordinates} ) OR NOT ( {point} is defined by

{goegraphical co-ordinates} )

28. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR NOT IFR to VFR OR the
    letters VFR are associated with {point}
29. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 5pc TAS or

    more} is planned at {point} )
30. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point B} } OR {point B} is defined by {goegraphical

    co-ordinates}
31. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point}
    is defined by {bearing and distance} OR insert

{Item 15 C} - { {point} followed by {point B} }

32. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point
    B} is defined by {bearing and distance} OR
    insert {Item 15 C} - { {point} followed by

{point B} }

--Test Frame 1.30:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. A change of {flight rules} is planned at {point}
   3. {point} is listed in Item 15 C
   4. IFR to VFR
   5. NOT (the letters VFR are associated with {point}
      )
   6. • Aircraft Identification is correct
   7. • FlightRules and Type of Flight is correct
   8. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   9. • Equipment is correct
  10. • Departure Aerodrome and time are correct
  11. • Mach number is prescribed by the appropriate
      ATS authority
  12. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
  13. • Flight is uncontrolled VFR
  14. • insert {Item 15 B} - {VFR}
  15. • ATS flight track points are required by the
      appropriate ATS authority
  16. • Use ATS style track points
  17. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  18. • Other Information is correct
  19. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.30: (continued)
 ROIDs: I15C
 Stimuli Response
  20. • forall point. NOT ( {point} is listed in Item
      15 C) OR A significant point code designator
      has been assigned to {point} OR 2 figures
      describing latitude in degrees followed by

{S} followed by 3 figures describing longitude

in degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {S} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 2 figures

describing latitude in degrees followed by {N}
followed by 3 figures describing longitude in
degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {N} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 4 figures

describing latitude in degrees and tens of units
of minutes followed by {S} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{S} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR 4 figures
describing latitude in degrees and tens of units
of minutes followed by {N} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{N} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR the 2 or 3
character identification of the navigation aid
followed by the 3 figure bearing from the aid in
degrees magnetic followed by the distance from
the aid in 3 figures expressing nautical miles
is associated with {point}

--Test Frame 1.30: (continued)
 ROIDs: I15C
 Stimuli Response
  21. • forall point. A change of {flight rules} is
      planned at {point} OR A change of {level} is
      planned at {point} OR A change of {speed} is
      planned at {point} OR ATS flight track points
      are required by the appropriate ATS authority OR
      NOT (insert {Item 15 C} - { {point} details} )
      OR A change of {track} is planned at {point}
  22. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR NOT (

{point B} is defined by {bearing and distance}

) OR NOT ( {point} is defined by {bearing and
distance} ) OR insert {Item 15 C} - {DCT between

{point} and {point B} }

23. • forall point. NOT ( {point} is listed in Item
    15 C) OR the code designator assigned to {route
    segment} including where appropriate the coded
    designator assigned to the standard {arrival}
    route is associated with {point} OR the code
    designator assigned to {route segment} including
    where appropriate the coded designator assigned
    to the standard {departure} route is associated
    with {point} OR the code designator assigned to

{route} including where appropriate the coded

designator assigned to the standard {arrival}
route is associated with {point} OR the code
designator assigned to {route} including where
appropriate the coded designator assigned to the
standard {departure} route is associated with

{point}

24. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR IFR to VFR OR NOT VFR
    to IFR OR the letters IFR are associated with

{point}

25. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A change of {level - climb}
    is planned at {point} ) OR an oblique stroke
    followed by the speed to be maintained during
    cruise climb followed by {the level above
    which cruise climb is planned followed by
    PLUS} is associated with {point} OR an oblique
    stroke followed by the speed to be maintained
    during cruise climb followed by {the two levels
    defining the layer to be occupied during cruide
    climb} is associated with {point}

--Test Frame 1.30: (continued)
 ROIDs: I15C
 Stimuli Response
  26. • forall point. NOT ( {point} is listed in
      Item 15 C) OR NOT (A significant point code
      designator has been assigned to {point} ) OR
      the 2 to 5 characters of the assigned coded
      designator is associated with {point}

  27. • forall point. NOT ( {point} is listed in Item
      15 C) OR an oblique stroke and both the cruising
      speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 0.01 Mach

    or more} is planned at {point} )
28. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - {DCT between {point} and {point B} } OR NOT ( {point B} is defined by {goegraphical

co-ordinates} ) OR NOT ( {point} is defined by

{goegraphical co-ordinates} )

29. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point

    B} } OR {point} is defined by {goegraphical
    co-ordinates}
30. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 5pc TAS or

    more} is planned at {point} )
31. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point B} } OR {point B} is defined by {goegraphical

    co-ordinates}
32. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point}
    is defined by {bearing and distance} OR insert

{Item 15 C} - { {point} followed by {point B} }

33. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point
    B} is defined by {bearing and distance} OR
    insert {Item 15 C} - { {point} followed by

{point B} }

1. report
   error

--Test Frame 1.31:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS route

   2. The departure aerodrome is {located on} the ATS
      route

   3. NOT (insert {Item 15 C} - {the designator of the
      first ATS route} )

   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • Equipment is correct
   8. • Departure Aerodrome and time are correct

   9. • Mach number is prescribed by the appropriate
      ATS authority
  10. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }

  11. • Flight is uncontrolled VFR
  12. • insert {Item 15 B} - {VFR}
  13. • NOT (The departure aerodrome is {connected to}
      the ATS route)
  14. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  15. • Other Information is correct
  16. • Supplementary Information is correct

  17. • forall point. NOT (A change of {ATS route
      other than same direction lower/upper} is
      planned at {point} ) OR NOT ( {next {point} }
      is defined by geological co-ordinates) OR NOT (

{point} is defined by geological co-ordinates)

    OR insert {Item 15 C} - { {point} followed by
    the designator of the next ATS route segment}
18. • forall point. NOT (A change of {speed} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

    route) OR {point} is defined by geological
    co-ordinates OR insert {Item 15 C} - { {point}
    followed by DCT}
19. • forall point. NOT (A change of {level} is
    planned at {point} ) OR The flight to the {next

{point} } will be outside a designated route OR

    insert {Item 15 C} - { {point} followed by the
    designator of the next ATS route segment}
20. • forall point. NOT (A change of {ATS route
    other than same direction lower/upper} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

route) OR {next {point} } is defined by
geological co-ordinates OR insert {Item 15 C}
- { {point} followed by DCT}

                                                    1. report
                                                       error

--Test Frame 1.32:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. ATS flight track points are required by the
      appropriate ATS authority
   3. NOT Use ATS style track points
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • Equipment is correct
   8. • Departure Aerodrome and time are correct
   9. • Mach number is prescribed by the appropriate
      ATS authority
  10. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
  11. • Flight is uncontrolled VFR
  12. • insert {Item 15 B} - {VFR}
  13. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  14. • Other Information is correct
  15. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.32: (continued)
 ROIDs: I15C
 Stimuli Response
  16. • forall point. NOT ( {point} is listed in Item
      15 C) OR A significant point code designator
      has been assigned to {point} OR 2 figures
      describing latitude in degrees followed by

{S} followed by 3 figures describing longitude

in degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {S} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 2 figures

describing latitude in degrees followed by {N}
followed by 3 figures describing longitude in
degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {N} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 4 figures

describing latitude in degrees and tens of units
of minutes followed by {S} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{S} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR 4 figures
describing latitude in degrees and tens of units
of minutes followed by {N} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{N} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR the 2 or 3
character identification of the navigation aid
followed by the 3 figure bearing from the aid in
degrees magnetic followed by the distance from
the aid in 3 figures expressing nautical miles
is associated with {point}

--Test Frame 1.32: (continued)
 ROIDs: I15C
 Stimuli Response
  17. • forall point. A change of {flight rules} is
      planned at {point} OR A change of {level} is
      planned at {point} OR A change of {speed} is
      planned at {point} OR ATS flight track points
      are required by the appropriate ATS authority OR
      NOT (insert {Item 15 C} - { {point} details} )
      OR A change of {track} is planned at {point}
  18. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR NOT (

{point B} is defined by {bearing and distance}

) OR NOT ( {point} is defined by {bearing and
distance} ) OR insert {Item 15 C} - {DCT between

{point} and {point B} }

19. • forall point. NOT ( {point} is listed in Item
    15 C) OR the code designator assigned to {route
    segment} including where appropriate the coded
    designator assigned to the standard {arrival}
    route is associated with {point} OR the code
    designator assigned to {route segment} including
    where appropriate the coded designator assigned
    to the standard {departure} route is associated
    with {point} OR the code designator assigned to

{route} including where appropriate the coded

designator assigned to the standard {arrival}
route is associated with {point} OR the code
designator assigned to {route} including where
appropriate the coded designator assigned to the
standard {departure} route is associated with

{point}

20. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR IFR to VFR OR NOT VFR
    to IFR OR the letters IFR are associated with

{point}

21. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A change of {level - climb}
    is planned at {point} ) OR an oblique stroke
    followed by the speed to be maintained during
    cruise climb followed by {the level above
    which cruise climb is planned followed by
    PLUS} is associated with {point} OR an oblique
    stroke followed by the speed to be maintained
    during cruise climb followed by {the two levels
    defining the layer to be occupied during cruide
    climb} is associated with {point}

--Test Frame 1.32: (continued)
 ROIDs: I15C
 Stimuli Response
  22. • forall point. NOT ( {point} is listed in
      Item 15 C) OR NOT (A significant point code
      designator has been assigned to {point} ) OR
      the 2 to 5 characters of the assigned coded
      designator is associated with {point}

  23. • forall point. NOT ( {point} is listed in Item
      15 C) OR an oblique stroke and both the cruising
      speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 0.01 Mach

    or more} is planned at {point} )
24. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - {DCT between {point} and {point B} } OR NOT ( {point B} is defined by {goegraphical

co-ordinates} ) OR NOT ( {point} is defined by

{goegraphical co-ordinates} )

25. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point

    B} } OR {point} is defined by {goegraphical
    co-ordinates}
26. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR NOT IFR to VFR OR the
    letters VFR are associated with {point}
27. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 5pc TAS or

    more} is planned at {point} )
28. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point B} } OR {point B} is defined by {goegraphical

    co-ordinates}
29. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point}
    is defined by {bearing and distance} OR insert

{Item 15 C} - { {point} followed by {point B} }

30. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point
    B} is defined by {bearing and distance} OR
    insert {Item 15 C} - { {point} followed by

{point B} }

--Test Frame 1.33:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. {point} is listed in Item 15 C
   3. NOT (an oblique stroke and both the cruising
      speed and the cruising level is associated with

{point} )

 4. A change of {speed - 5pc TAS or more} is planned
    at {point}
 5. • Aircraft Identification is correct
 6. • FlightRules and Type of Flight is correct
 7. • Number and Type of Aircraft and Wake
    Turbulence Category is correct
 8. • Equipment is correct
 9. • Departure Aerodrome and time are correct
10. • Mach number is prescribed by the appropriate
    ATS authority
11. • insert {Item 15 A} - {the true airspeed for
    the first or the whole cruising portion of the
    flight expressed as {M followed by 3 digits of
    Mach hundredths} }
12. • Flight is uncontrolled VFR
13. • insert {Item 15 B} - {VFR}
14. • ATS flight track points are required by the
    appropriate ATS authority
15. • Use ATS style track points
16. • Destination Aerodrome and Total Estimated
    Elapsed Time is correct
17. • Other Information is correct
18. • Supplementary Information is correct

                                                        1. report
                                                           error

--Test Frame 1.33: (continued)
 ROIDs: I15C
 Stimuli Response
  19. • forall point. NOT ( {point} is listed in Item
      15 C) OR A significant point code designator
      has been assigned to {point} OR 2 figures
      describing latitude in degrees followed by

{S} followed by 3 figures describing longitude

in degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {S} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 2 figures

describing latitude in degrees followed by {N}
followed by 3 figures describing longitude in
degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {N} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 4 figures

describing latitude in degrees and tens of units
of minutes followed by {S} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{S} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR 4 figures
describing latitude in degrees and tens of units
of minutes followed by {N} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{N} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR the 2 or 3
character identification of the navigation aid
followed by the 3 figure bearing from the aid in
degrees magnetic followed by the distance from
the aid in 3 figures expressing nautical miles
is associated with {point}

--Test Frame 1.33: (continued)
 ROIDs: I15C
 Stimuli Response
  20. • forall point. A change of {flight rules} is
      planned at {point} OR A change of {level} is
      planned at {point} OR A change of {speed} is
      planned at {point} OR ATS flight track points
      are required by the appropriate ATS authority OR
      NOT (insert {Item 15 C} - { {point} details} )
      OR A change of {track} is planned at {point}
  21. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR NOT (

{point B} is defined by {bearing and distance}

) OR NOT ( {point} is defined by {bearing and
distance} ) OR insert {Item 15 C} - {DCT between

{point} and {point B} }

22. • forall point. NOT ( {point} is listed in Item
    15 C) OR the code designator assigned to {route
    segment} including where appropriate the coded
    designator assigned to the standard {arrival}
    route is associated with {point} OR the code
    designator assigned to {route segment} including
    where appropriate the coded designator assigned
    to the standard {departure} route is associated
    with {point} OR the code designator assigned to

{route} including where appropriate the coded

designator assigned to the standard {arrival}
route is associated with {point} OR the code
designator assigned to {route} including where
appropriate the coded designator assigned to the
standard {departure} route is associated with

{point}

23. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR IFR to VFR OR NOT VFR
    to IFR OR the letters IFR are associated with

{point}

24. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A change of {level - climb}
    is planned at {point} ) OR an oblique stroke
    followed by the speed to be maintained during
    cruise climb followed by {the level above
    which cruise climb is planned followed by
    PLUS} is associated with {point} OR an oblique
    stroke followed by the speed to be maintained
    during cruise climb followed by {the two levels
    defining the layer to be occupied during cruide
    climb} is associated with {point}

--Test Frame 1.33: (continued)
 ROIDs: I15C
 Stimuli Response
  25. • forall point. NOT ( {point} is listed in
      Item 15 C) OR NOT (A significant point code
      designator has been assigned to {point} ) OR
      the 2 to 5 characters of the assigned coded
      designator is associated with {point}

  26. • forall point. NOT ( {point} is listed in Item
      15 C) OR an oblique stroke and both the cruising
      speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 0.01 Mach

    or more} is planned at {point} )
27. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - {DCT between {point} and {point B} } OR NOT ( {point B} is defined by {goegraphical

co-ordinates} ) OR NOT ( {point} is defined by

{goegraphical co-ordinates} )

28. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point

    B} } OR {point} is defined by {goegraphical
    co-ordinates}
29. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR NOT IFR to VFR OR the
    letters VFR are associated with {point}
30. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point B} } OR {point B} is defined by {goegraphical

    co-ordinates}
31. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point}
    is defined by {bearing and distance} OR insert

{Item 15 C} - { {point} followed by {point B} }

32. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point
    B} is defined by {bearing and distance} OR
    insert {Item 15 C} - { {point} followed by

{point B} }

--Test Frame 1.34:
 ROIDs: I15C
 Stimuli Response
   1. The flight is along a designated ATS route

   2. A change of {ATS route other than same direction
      lower/upper} is planned at {point}

   3. The flight to the {next {point} } will be
      outside a designated route

   4. NOT ( {next {point} } is defined by geological
      co-ordinates)

   5. NOT (insert {Item 15 C} - { {point} followed by
      DCT} )
   6. • Aircraft Identification is correct

   7. • FlightRules and Type of Flight is correct
   8. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   9. • Equipment is correct
  10. • Departure Aerodrome and time are correct
  11. • Mach number is prescribed by the appropriate
      ATS authority
  12. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }

  13. • Flight is uncontrolled VFR
  14. • insert {Item 15 B} - {VFR}
  15. • The departure aerodrome is {connected to} the
      ATS route
  16. • insert {Item 15 C} - {the designator of the
      first ATS route}
  17. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  18. • Other Information is correct
  19. • Supplementary Information is correct
  20. • forall point. NOT (A change of {ATS route
      other than same direction lower/upper} is
      planned at {point} ) OR NOT ( {next {point} }
      is defined by geological co-ordinates) OR NOT (

{point} is defined by geological co-ordinates)

    OR insert {Item 15 C} - { {point} followed by
    the designator of the next ATS route segment}

21. • forall point. NOT (A change of {speed} is
    planned at {point} ) OR NOT (The flight to the

{next {point} } will be outside a designated

    route) OR {point} is defined by geological
    co-ordinates OR insert {Item 15 C} - { {point}
    followed by DCT}
22. • forall point. NOT (A change of {level} is
    planned at {point} ) OR The flight to the {next

{point} } will be outside a designated route OR

insert {Item 15 C} - { {point} followed by the
designator of the next ATS route segment}

                                                    1. report
                                                       error

--Test Frame 1.35:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. ATS flight track points are required by the
      appropriate ATS authority
   3. {point} and {point B} are successive points
   4. NOT (insert {Item 15 C} - { {point} followed by

{point B} } )

 5. NOT ( {point B} is defined by {goegraphical
    co-ordinates} )
 6. • Aircraft Identification is correct
 7. • FlightRules and Type of Flight is correct
 8. • Number and Type of Aircraft and Wake
    Turbulence Category is correct
 9. • Equipment is correct
10. • Departure Aerodrome and time are correct
11. • Mach number is prescribed by the appropriate
    ATS authority
12. • insert {Item 15 A} - {the true airspeed for
    the first or the whole cruising portion of the
    flight expressed as {M followed by 3 digits of
    Mach hundredths} }
13. • Flight is uncontrolled VFR
14. • insert {Item 15 B} - {VFR}
15. • Use ATS style track points
16. • Destination Aerodrome and Total Estimated
    Elapsed Time is correct
17. • Other Information is correct
18. • Supplementary Information is correct

                                                        1. report
                                                           error

--Test Frame 1.35: (continued)
 ROIDs: I15C
 Stimuli Response
  19. • forall point. NOT ( {point} is listed in Item
      15 C) OR A significant point code designator
      has been assigned to {point} OR 2 figures
      describing latitude in degrees followed by

{S} followed by 3 figures describing longitude

in degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {S} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 2 figures

describing latitude in degrees followed by {N}
followed by 3 figures describing longitude in
degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {N} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 4 figures

describing latitude in degrees and tens of units
of minutes followed by {S} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{S} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR 4 figures
describing latitude in degrees and tens of units
of minutes followed by {N} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{N} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR the 2 or 3
character identification of the navigation aid
followed by the 3 figure bearing from the aid in
degrees magnetic followed by the distance from
the aid in 3 figures expressing nautical miles
is associated with {point}

--Test Frame 1.35: (continued)
 ROIDs: I15C
 Stimuli Response
  20. • forall point. A change of {flight rules} is
      planned at {point} OR A change of {level} is
      planned at {point} OR A change of {speed} is
      planned at {point} OR ATS flight track points
      are required by the appropriate ATS authority OR
      NOT (insert {Item 15 C} - { {point} details} )
      OR A change of {track} is planned at {point}
  21. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR NOT (

{point B} is defined by {bearing and distance}

) OR NOT ( {point} is defined by {bearing and
distance} ) OR insert {Item 15 C} - {DCT between

{point} and {point B} }

22. • forall point. NOT ( {point} is listed in Item
    15 C) OR the code designator assigned to {route
    segment} including where appropriate the coded
    designator assigned to the standard {arrival}
    route is associated with {point} OR the code
    designator assigned to {route segment} including
    where appropriate the coded designator assigned
    to the standard {departure} route is associated
    with {point} OR the code designator assigned to

{route} including where appropriate the coded

designator assigned to the standard {arrival}
route is associated with {point} OR the code
designator assigned to {route} including where
appropriate the coded designator assigned to the
standard {departure} route is associated with

{point}

23. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR IFR to VFR OR NOT VFR
    to IFR OR the letters IFR are associated with

{point}

24. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A change of {level - climb}
    is planned at {point} ) OR an oblique stroke
    followed by the speed to be maintained during
    cruise climb followed by {the level above
    which cruise climb is planned followed by
    PLUS} is associated with {point} OR an oblique
    stroke followed by the speed to be maintained
    during cruise climb followed by {the two levels
    defining the layer to be occupied during cruide
    climb} is associated with {point}

--Test Frame 1.35: (continued)
 ROIDs: I15C
 Stimuli Response
  25. • forall point. NOT ( {point} is listed in
      Item 15 C) OR NOT (A significant point code
      designator has been assigned to {point} ) OR
      the 2 to 5 characters of the assigned coded
      designator is associated with {point}

  26. • forall point. NOT ( {point} is listed in Item
      15 C) OR an oblique stroke and both the cruising
      speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 0.01 Mach

    or more} is planned at {point} )
27. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - {DCT between {point} and {point B} } OR NOT ( {point B} is defined by {goegraphical

co-ordinates} ) OR NOT ( {point} is defined by

{goegraphical co-ordinates} )

28. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point

    B} } OR {point} is defined by {goegraphical
    co-ordinates}
29. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR NOT IFR to VFR OR the
    letters VFR are associated with {point}
30. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 5pc TAS or

    more} is planned at {point} )
31. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point}
    is defined by {bearing and distance} OR insert

{Item 15 C} - { {point} followed by {point B} }

32. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point
    B} is defined by {bearing and distance} OR
    insert {Item 15 C} - { {point} followed by

{point B} }

--Test Frame 1.36:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. ATS flight track points are required by the
      appropriate ATS authority
   3. {point} and {point B} are successive points
   4. NOT ( {point} is defined by {bearing and
      distance} )
   5. NOT (insert {Item 15 C} - { {point} followed by

{point B} } )

 6. • Aircraft Identification is correct
 7. • FlightRules and Type of Flight is correct
 8. • Number and Type of Aircraft and Wake
    Turbulence Category is correct
 9. • Equipment is correct
10. • Departure Aerodrome and time are correct
11. • Mach number is prescribed by the appropriate
    ATS authority
12. • insert {Item 15 A} - {the true airspeed for
    the first or the whole cruising portion of the
    flight expressed as {M followed by 3 digits of
    Mach hundredths} }
13. • Flight is uncontrolled VFR
14. • insert {Item 15 B} - {VFR}
15. • Use ATS style track points
16. • Destination Aerodrome and Total Estimated
    Elapsed Time is correct
17. • Other Information is correct
18. • Supplementary Information is correct

                                                        1. report
                                                           error

--Test Frame 1.36: (continued)
 ROIDs: I15C
 Stimuli Response
  19. • forall point. NOT ( {point} is listed in Item
      15 C) OR A significant point code designator
      has been assigned to {point} OR 2 figures
      describing latitude in degrees followed by

{S} followed by 3 figures describing longitude

in degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {S} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 2 figures

describing latitude in degrees followed by {N}
followed by 3 figures describing longitude in
degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {N} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 4 figures

describing latitude in degrees and tens of units
of minutes followed by {S} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{S} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR 4 figures
describing latitude in degrees and tens of units
of minutes followed by {N} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{N} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR the 2 or 3
character identification of the navigation aid
followed by the 3 figure bearing from the aid in
degrees magnetic followed by the distance from
the aid in 3 figures expressing nautical miles
is associated with {point}

--Test Frame 1.36: (continued)
 ROIDs: I15C
 Stimuli Response
  20. • forall point. A change of {flight rules} is
      planned at {point} OR A change of {level} is
      planned at {point} OR A change of {speed} is
      planned at {point} OR ATS flight track points
      are required by the appropriate ATS authority OR
      NOT (insert {Item 15 C} - { {point} details} )
      OR A change of {track} is planned at {point}
  21. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR NOT (

{point B} is defined by {bearing and distance}

) OR NOT ( {point} is defined by {bearing and
distance} ) OR insert {Item 15 C} - {DCT between

{point} and {point B} }

22. • forall point. NOT ( {point} is listed in Item
    15 C) OR the code designator assigned to {route
    segment} including where appropriate the coded
    designator assigned to the standard {arrival}
    route is associated with {point} OR the code
    designator assigned to {route segment} including
    where appropriate the coded designator assigned
    to the standard {departure} route is associated
    with {point} OR the code designator assigned to

{route} including where appropriate the coded

designator assigned to the standard {arrival}
route is associated with {point} OR the code
designator assigned to {route} including where
appropriate the coded designator assigned to the
standard {departure} route is associated with

{point}

23. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR IFR to VFR OR NOT VFR
    to IFR OR the letters IFR are associated with

{point}

24. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A change of {level - climb}
    is planned at {point} ) OR an oblique stroke
    followed by the speed to be maintained during
    cruise climb followed by {the level above
    which cruise climb is planned followed by
    PLUS} is associated with {point} OR an oblique
    stroke followed by the speed to be maintained
    during cruise climb followed by {the two levels
    defining the layer to be occupied during cruide
    climb} is associated with {point}

--Test Frame 1.36: (continued)
 ROIDs: I15C
 Stimuli Response
  25. • forall point. NOT ( {point} is listed in
      Item 15 C) OR NOT (A significant point code
      designator has been assigned to {point} ) OR
      the 2 to 5 characters of the assigned coded
      designator is associated with {point}

  26. • forall point. NOT ( {point} is listed in Item
      15 C) OR an oblique stroke and both the cruising
      speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 0.01 Mach

    or more} is planned at {point} )
27. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - {DCT between {point} and {point B} } OR NOT ( {point B} is defined by {goegraphical

co-ordinates} ) OR NOT ( {point} is defined by

{goegraphical co-ordinates} )

28. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point

    B} } OR {point} is defined by {goegraphical
    co-ordinates}
29. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR NOT IFR to VFR OR the
    letters VFR are associated with {point}
30. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 5pc TAS or

    more} is planned at {point} )
31. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point B} } OR {point B} is defined by {goegraphical

    co-ordinates}
32. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point
    B} is defined by {bearing and distance} OR
    insert {Item 15 C} - { {point} followed by

{point B} }

--Test Frame 1.37:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. ATS flight track points are required by the
      appropriate ATS authority
   3. {point} and {point B} are successive points
   4. NOT ( {point B} is defined by {bearing and
      distance} )
   5. NOT (insert {Item 15 C} - { {point} followed by

{point B} } )

 6. • Aircraft Identification is correct
 7. • FlightRules and Type of Flight is correct
 8. • Number and Type of Aircraft and Wake
    Turbulence Category is correct
 9. • Equipment is correct
10. • Departure Aerodrome and time are correct
11. • Mach number is prescribed by the appropriate
    ATS authority
12. • insert {Item 15 A} - {the true airspeed for
    the first or the whole cruising portion of the
    flight expressed as {M followed by 3 digits of
    Mach hundredths} }
13. • Flight is uncontrolled VFR
14. • insert {Item 15 B} - {VFR}
15. • Use ATS style track points
16. • Destination Aerodrome and Total Estimated
    Elapsed Time is correct
17. • Other Information is correct
18. • Supplementary Information is correct

                                                        1. report
                                                           error

--Test Frame 1.37: (continued)
 ROIDs: I15C
 Stimuli Response
  19. • forall point. NOT ( {point} is listed in Item
      15 C) OR A significant point code designator
      has been assigned to {point} OR 2 figures
      describing latitude in degrees followed by

{S} followed by 3 figures describing longitude

in degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {S} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 2 figures

describing latitude in degrees followed by {N}
followed by 3 figures describing longitude in
degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {N} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 4 figures

describing latitude in degrees and tens of units
of minutes followed by {S} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{S} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR 4 figures
describing latitude in degrees and tens of units
of minutes followed by {N} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{N} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR the 2 or 3
character identification of the navigation aid
followed by the 3 figure bearing from the aid in
degrees magnetic followed by the distance from
the aid in 3 figures expressing nautical miles
is associated with {point}

--Test Frame 1.37: (continued)
 ROIDs: I15C
 Stimuli Response
  20. • forall point. A change of {flight rules} is
      planned at {point} OR A change of {level} is
      planned at {point} OR A change of {speed} is
      planned at {point} OR ATS flight track points
      are required by the appropriate ATS authority OR
      NOT (insert {Item 15 C} - { {point} details} )
      OR A change of {track} is planned at {point}
  21. • forall point. forall point B. NOT ( {point}
      and {point B} are successive points) OR NOT (

{point B} is defined by {bearing and distance}

) OR NOT ( {point} is defined by {bearing and
distance} ) OR insert {Item 15 C} - {DCT between

{point} and {point B} }

22. • forall point. NOT ( {point} is listed in Item
    15 C) OR the code designator assigned to {route
    segment} including where appropriate the coded
    designator assigned to the standard {arrival}
    route is associated with {point} OR the code
    designator assigned to {route segment} including
    where appropriate the coded designator assigned
    to the standard {departure} route is associated
    with {point} OR the code designator assigned to

{route} including where appropriate the coded

designator assigned to the standard {arrival}
route is associated with {point} OR the code
designator assigned to {route} including where
appropriate the coded designator assigned to the
standard {departure} route is associated with

{point}

23. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR IFR to VFR OR NOT VFR
    to IFR OR the letters IFR are associated with

{point}

24. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A change of {level - climb}
    is planned at {point} ) OR an oblique stroke
    followed by the speed to be maintained during
    cruise climb followed by {the level above
    which cruise climb is planned followed by
    PLUS} is associated with {point} OR an oblique
    stroke followed by the speed to be maintained
    during cruise climb followed by {the two levels
    defining the layer to be occupied during cruide
    climb} is associated with {point}

--Test Frame 1.37: (continued)
 ROIDs: I15C
 Stimuli Response
  25. • forall point. NOT ( {point} is listed in
      Item 15 C) OR NOT (A significant point code
      designator has been assigned to {point} ) OR
      the 2 to 5 characters of the assigned coded
      designator is associated with {point}

  26. • forall point. NOT ( {point} is listed in Item
      15 C) OR an oblique stroke and both the cruising
      speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 0.01 Mach

    or more} is planned at {point} )
27. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - {DCT between {point} and {point B} } OR NOT ( {point B} is defined by {goegraphical

co-ordinates} ) OR NOT ( {point} is defined by

{goegraphical co-ordinates} )

28. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point

    B} } OR {point} is defined by {goegraphical
    co-ordinates}
29. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR NOT IFR to VFR OR the
    letters VFR are associated with {point}
30. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 5pc TAS or

    more} is planned at {point} )
31. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR insert

{Item 15 C} - { {point} followed by {point B} } OR {point B} is defined by {goegraphical

    co-ordinates}
32. • forall point. forall point B. NOT ( {point}
    and {point B} are successive points) OR {point}
    is defined by {bearing and distance} OR insert

{Item 15 C} - { {point} followed by {point B} }

1. report
   error

--Test Frame 1.38:
 ROIDs: I15C
 Stimuli Response
   1. NOT The flight is along a designated ATS route
   2. NOT ATS flight track points are required by the
      appropriate ATS authority
   3. NOT (insert {Item 15 C} - { {point} details} )
   4. NOT ( {point} and {next {point} } are normally
      more than {370km} apart)
   5. A change of {track} is planned at {point}
   6. • Aircraft Identification is correct
   7. • FlightRules and Type of Flight is correct
   8. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   9. • Equipment is correct
  10. • Departure Aerodrome and time are correct
  11. • Mach number is prescribed by the appropriate
      ATS authority
  12. • insert {Item 15 A} - {the true airspeed for
      the first or the whole cruising portion of the
      flight expressed as {M followed by 3 digits of
      Mach hundredths} }
  13. • Flight is uncontrolled VFR
  14. • insert {Item 15 B} - {VFR}
  15. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  16. • Other Information is correct
  17. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.38: (continued)
 ROIDs: I15C
 Stimuli Response
  18. • forall point. NOT ( {point} is listed in Item
      15 C) OR A significant point code designator
      has been assigned to {point} OR 2 figures
      describing latitude in degrees followed by

{S} followed by 3 figures describing longitude

in degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {S} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 2 figures

describing latitude in degrees followed by {N}
followed by 3 figures describing longitude in
degrees followed by {W} is associated with

{point} OR 2 figures describing latitude in

degrees followed by {N} followed by 3 figures
describing longitude in degrees followed by

{E} is associated with {point} OR 4 figures

describing latitude in degrees and tens of units
of minutes followed by {S} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{S} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR 4 figures
describing latitude in degrees and tens of units
of minutes followed by {N} followed by 5 figures
describing longitude in degrees and tens of
units of minutes followed by {W} is associated
with {point} OR 4 figures describing latitude in
degrees and tens of units of minutes followed by

{N} followed by 5 figures describing longitude

in degrees and tens of units of minutes followed
by {E} is associated with {point} OR the 2 or 3
character identification of the navigation aid
followed by the 3 figure bearing from the aid in
degrees magnetic followed by the distance from
the aid in 3 figures expressing nautical miles
is associated with {point}

--Test Frame 1.38: (continued)
 ROIDs: I15C
 Stimuli Response
  19. • forall point. A change of {flight rules} is
      planned at {point} OR A change of {level} is
      planned at {point} OR A change of {speed} is
      planned at {point} OR ATS flight track points
      are required by the appropriate ATS authority OR
      NOT (insert {Item 15 C} - { {point} details} )
      OR A change of {track} is planned at {point}
  20. • forall point. NOT ( {point} is listed in Item
      15 C) OR the code designator assigned to {route
      segment} including where appropriate the coded
      designator assigned to the standard {arrival}
      route is associated with {point} OR the code
      designator assigned to {route segment} including
      where appropriate the coded designator assigned
      to the standard {departure} route is associated
      with {point} OR the code designator assigned to

{route} including where appropriate the coded

designator assigned to the standard {arrival}
route is associated with {point} OR the code
designator assigned to {route} including where
appropriate the coded designator assigned to the
standard {departure} route is associated with

{point}

21. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR IFR to VFR OR NOT VFR
    to IFR OR the letters IFR are associated with

{point}

22. • forall point. NOT ( {point} is listed in
    Item 15 C) OR NOT (A change of {level - climb}
    is planned at {point} ) OR an oblique stroke
    followed by the speed to be maintained during
    cruise climb followed by {the level above
    which cruise climb is planned followed by
    PLUS} is associated with {point} OR an oblique
    stroke followed by the speed to be maintained
    during cruise climb followed by {the two levels
    defining the layer to be occupied during cruide
    climb} is associated with {point}
23. • forall point. insert {Item 15 C} - { {point}
    details} OR {point} and {next {point} } are
    normally more than {30 minutes flying time}
    apart OR NOT (A change of {track} is planned at

{point} )

--Test Frame 1.38: (continued)
 ROIDs: I15C
 Stimuli Response
  24. • forall point. NOT ( {point} is listed in
      Item 15 C) OR NOT (A significant point code
      designator has been assigned to {point} ) OR
      the 2 to 5 characters of the assigned coded
      designator is associated with {point}

  25. • forall point. NOT ( {point} is listed in Item
      15 C) OR an oblique stroke and both the cruising
      speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 0.01 Mach

    or more} is planned at {point} )
26. • forall point. NOT (insert {Item 15 C} -

{ {point} details} ) OR NOT ( {point} and {next {point} } are normally more than {370km}

    apart) OR NOT ( {point} and {next {point} } are
    normally more than {30 minutes flying time}
    apart)
27. • forall point. NOT (A change of {flight rules}
    is planned at {point} ) OR NOT ( {point} is
    listed in Item 15 C) OR NOT IFR to VFR OR the
    letters VFR are associated with {point}
28. • forall point. NOT ( {point} is listed in Item
    15 C) OR an oblique stroke and both the cruising
    speed and the cruising level is associated with

{point} OR NOT (A change of {speed - 5pc TAS or

more} is planned at {point} )

E.3.7 Destination Aerodrome and Total Estimated Elapsed Time

--Test Frame 1.1:
 Stimuli Response
   1. NOT Supplementary Information is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Route is correct
   8. • Location indicator has been assigned
   9. • insert {Item 16 Dest} - {the ICAO four letter
      location indicator of the destination aerodrome
      followed by the total estimated elapsed time}
  10. • Location indicator has been assigned to the
      alternate aerodrome
  11. • Other Information is correct

                                                          1. report
                                                             error

--Test Frame 1.2:
 Stimuli Response
   1. NOT Other Information is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Route is correct
   8. • Location indicator has been assigned
   9. • insert {Item 16 Dest} - {the ICAO four letter
      location indicator of the destination aerodrome
      followed by the total estimated elapsed time}
  10. • Location indicator has been assigned to the
      alternate aerodrome
  11. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.3:
 Stimuli Response
   1. NOT Route is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Location indicator has been assigned
   8. • insert {Item 16 Dest} - {the ICAO four letter
      location indicator of the destination aerodrome
      followed by the total estimated elapsed time}
   9. • Location indicator has been assigned to the
      alternate aerodrome
  10. • Other Information is correct
  11. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.4:
 Stimuli Response
   1. NOT Departure Aerodrome and time are correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Route is correct
   7. • Location indicator has been assigned
   8. • insert {Item 16 Dest} - {the ICAO four letter
      location indicator of the destination aerodrome
      followed by the total estimated elapsed time}
   9. • Location indicator has been assigned to the
      alternate aerodrome
  10. • Other Information is correct
  11. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.5:
 Stimuli Response
   1. NOT Equipment is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Departure Aerodrome and time are correct
   6. • Route is correct
   7. • Location indicator has been assigned
   8. • insert {Item 16 Dest} - {the ICAO four letter
      location indicator of the destination aerodrome
      followed by the total estimated elapsed time}
   9. • Location indicator has been assigned to the
      alternate aerodrome
  10. • Other Information is correct
  11. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.6:
 Stimuli Response
   1. NOT Number and Type of Aircraft and Wake
      Turbulence Category is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Equipment is correct
   5. • Departure Aerodrome and time are correct
   6. • Route is correct
   7. • Location indicator has been assigned
   8. • insert {Item 16 Dest} - {the ICAO four letter
      location indicator of the destination aerodrome
      followed by the total estimated elapsed time}
   9. • Location indicator has been assigned to the
      alternate aerodrome
  10. • Other Information is correct
  11. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.7:
 Stimuli Response
   1. NOT FlightRules and Type of Flight is correct
   2. • Aircraft Identification is correct
   3. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   4. • Equipment is correct
   5. • Departure Aerodrome and time are correct
   6. • Route is correct
   7. • Location indicator has been assigned
   8. • insert {Item 16 Dest} - {the ICAO four letter
      location indicator of the destination aerodrome
      followed by the total estimated elapsed time}
   9. • Location indicator has been assigned to the
      alternate aerodrome
  10. • Other Information is correct
  11. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.8:
 Stimuli Response
   1. NOT Aircraft Identification is correct
   2. • FlightRules and Type of Flight is correct
   3. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   4. • Equipment is correct
   5. • Departure Aerodrome and time are correct
   6. • Route is correct
   7. • Location indicator has been assigned
   8. • insert {Item 16 Dest} - {the ICAO four letter
      location indicator of the destination aerodrome
      followed by the total estimated elapsed time}
   9. • Location indicator has been assigned to the
      alternate aerodrome
  10. • Other Information is correct
  11. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.9:
 ROIDs: I16-1
 Stimuli Response
   1. Location indicator has been assigned
   2. NOT (insert {Item 16 Dest} - {the ICAO four
      letter location indicator of the destination
      aerodrome followed by the total estimated
      elapsed time} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Location indicator has been assigned to the
      alternate aerodrome
  10. • Other Information is correct
  11. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.10:
 ROIDs: I16-2
 Stimuli Response
   1. NOT Location indicator has been assigned to the
      alternate aerodrome
   2. NOT (insert {Item 18} - {ALTN/ the name of the
      alternate aerodrome} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Location indicator has been assigned
  10. • insert {Item 16 Dest} - {the ICAO four letter
      location indicator of the destination aerodrome
      followed by the total estimated elapsed time}
  11. • insert {Item 16 Alt} - {ZZZZ}
  12. • Other Information is correct
  13. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.11:
 ROIDs: I16-1
 Stimuli Response
   1. NOT Location indicator has been assigned
   2. NOT (insert {Item 18} - {DEST/ the name of the
      aerodrome} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • insert {Item 16 Dest} - {ZZZZ followed by the
      total estimated elapsed time}
  10. • Location indicator has been assigned to the
      alternate aerodrome
  11. • Other Information is correct
  12. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.12:
 ROIDs: I16-2
 Stimuli Response
   1. NOT Location indicator has been assigned to the
      alternate aerodrome
   2. NOT (insert {Item 16 Alt} - {ZZZZ} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Location indicator has been assigned
  10. • insert {Item 16 Dest} - {the ICAO four letter
      location indicator of the destination aerodrome
      followed by the total estimated elapsed time}
  11. • insert {Item 18} - {ALTN/ the name of the
      alternate aerodrome}
  12. • Other Information is correct
  13. • Supplementary Information is correct

                                                          1. report
                                                             error

--Test Frame 1.13:
 ROIDs: I16-1
 Stimuli Response
   1. NOT Location indicator has been assigned
   2. NOT (insert {Item 16 Dest} - {ZZZZ followed by
      the total estimated elapsed time} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • insert {Item 18} - {DEST/ the name of the
      aerodrome}
  10. • Location indicator has been assigned to the
      alternate aerodrome
  11. • Other Information is correct
  12. • Supplementary Information is correct

                                                          1. report
                                                             error

E.3.8 Other Information

--Test Frame 1.1:
 Stimuli Response
   1. NOT Supplementary Information is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct

   6. • Departure Aerodrome and time are correct
   7. • Route is correct
   8. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   9. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}
  10. • insert {Item 18} - {REG/registration markings
      of the aircraft}
  11. • insert {Item 18} - {SEL/SELCAL Code}

  12. • The name of the operator is obvious from the
      aircraft identification in Item 7
  13. • insert {Item 18} - {STS/reason for special
      handling}
  14. • insert {Item 18} - {PER/Aircraft performance
      data}
  15. • insert {Item 18} - {RMK/any other remarks}

  16. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }
  17. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

18. • forall point. NOT ( {point} is a {FIR
    boundary} prescribed {on the basis of regional
    air navigation agreements} ) OR insert {Item 18}
    - {EET/ {point} }

19. • forall point. NOT ( {point} is a {significant
    point} prescribed {by the approapriate ATS
    authority} ) OR insert {Item 18} - {EET/ {point}

}

20. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.2:
 Stimuli Response
   1. NOT Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct

   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct

   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Route is correct
   8. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}

   9. • insert {Item 18} - {REG/registration markings
      of the aircraft}
  10. • insert {Item 18} - {SEL/SELCAL Code}

  11. • The name of the operator is obvious from the
      aircraft identification in Item 7

  12. • insert {Item 18} - {STS/reason for special
      handling}

  13. • insert {Item 18} - {PER/Aircraft performance
      data}

  14. • insert {Item 18} - {RMK/any other remarks}
  15. • Supplementary Information is correct
  16. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }

  17. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

18. • forall point. NOT ( {point} is a {FIR
    boundary} prescribed {on the basis of regional
    air navigation agreements} ) OR insert {Item 18}
    - {EET/ {point} }
19. • forall point. NOT ( {point} is a {significant
    point} prescribed {by the approapriate ATS
    authority} ) OR insert {Item 18} - {EET/ {point}

}

20. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.3:
 Stimuli Response
   1. NOT Route is correct
   2. • Aircraft Identification is correct

   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   8. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}

   9. • insert {Item 18} - {REG/registration markings
      of the aircraft}
  10. • insert {Item 18} - {SEL/SELCAL Code}

  11. • The name of the operator is obvious from the
      aircraft identification in Item 7

  12. • insert {Item 18} - {STS/reason for special
      handling}

  13. • insert {Item 18} - {PER/Aircraft performance
      data}

  14. • insert {Item 18} - {RMK/any other remarks}
  15. • Supplementary Information is correct
  16. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }

  17. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

18. • forall point. NOT ( {point} is a {FIR
    boundary} prescribed {on the basis of regional
    air navigation agreements} ) OR insert {Item 18}
    - {EET/ {point} }
19. • forall point. NOT ( {point} is a {significant
    point} prescribed {by the approapriate ATS
    authority} ) OR insert {Item 18} - {EET/ {point}

}

20. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.4:
 Stimuli Response
   1. NOT Departure Aerodrome and time are correct
   2. • Aircraft Identification is correct

   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Route is correct
   7. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   8. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}

   9. • insert {Item 18} - {REG/registration markings
      of the aircraft}
  10. • insert {Item 18} - {SEL/SELCAL Code}

  11. • The name of the operator is obvious from the
      aircraft identification in Item 7

  12. • insert {Item 18} - {STS/reason for special
      handling}

  13. • insert {Item 18} - {PER/Aircraft performance
      data}

  14. • insert {Item 18} - {RMK/any other remarks}
  15. • Supplementary Information is correct
  16. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }

  17. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

18. • forall point. NOT ( {point} is a {FIR
    boundary} prescribed {on the basis of regional
    air navigation agreements} ) OR insert {Item 18}
    - {EET/ {point} }
19. • forall point. NOT ( {point} is a {significant
    point} prescribed {by the approapriate ATS
    authority} ) OR insert {Item 18} - {EET/ {point}

}

20. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.5:
 Stimuli Response
   1. NOT Equipment is correct
   2. • Aircraft Identification is correct

   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Departure Aerodrome and time are correct
   6. • Route is correct
   7. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   8. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}

   9. • insert {Item 18} - {REG/registration markings
      of the aircraft}
  10. • insert {Item 18} - {SEL/SELCAL Code}

  11. • The name of the operator is obvious from the
      aircraft identification in Item 7

  12. • insert {Item 18} - {STS/reason for special
      handling}

  13. • insert {Item 18} - {PER/Aircraft performance
      data}

  14. • insert {Item 18} - {RMK/any other remarks}
  15. • Supplementary Information is correct
  16. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }

  17. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

18. • forall point. NOT ( {point} is a {FIR
    boundary} prescribed {on the basis of regional
    air navigation agreements} ) OR insert {Item 18}
    - {EET/ {point} }
19. • forall point. NOT ( {point} is a {significant
    point} prescribed {by the approapriate ATS
    authority} ) OR insert {Item 18} - {EET/ {point}

}

20. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.6:
 Stimuli Response
   1. NOT Number and Type of Aircraft and Wake
      Turbulence Category is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct

   4. • Equipment is correct
   5. • Departure Aerodrome and time are correct
   6. • Route is correct
   7. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   8. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}

   9. • insert {Item 18} - {REG/registration markings
      of the aircraft}
  10. • insert {Item 18} - {SEL/SELCAL Code}

  11. • The name of the operator is obvious from the
      aircraft identification in Item 7

  12. • insert {Item 18} - {STS/reason for special
      handling}

  13. • insert {Item 18} - {PER/Aircraft performance
      data}

  14. • insert {Item 18} - {RMK/any other remarks}
  15. • Supplementary Information is correct
  16. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }

  17. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

18. • forall point. NOT ( {point} is a {FIR
    boundary} prescribed {on the basis of regional
    air navigation agreements} ) OR insert {Item 18}
    - {EET/ {point} }
19. • forall point. NOT ( {point} is a {significant
    point} prescribed {by the approapriate ATS
    authority} ) OR insert {Item 18} - {EET/ {point}

}

20. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.7:
 Stimuli Response
   1. NOT FlightRules and Type of Flight is correct
   2. • Aircraft Identification is correct

   3. • Number and Type of Aircraft and Wake
      Turbulence Category is correct

   4. • Equipment is correct
   5. • Departure Aerodrome and time are correct
   6. • Route is correct
   7. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   8. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}

   9. • insert {Item 18} - {REG/registration markings
      of the aircraft}
  10. • insert {Item 18} - {SEL/SELCAL Code}

  11. • The name of the operator is obvious from the
      aircraft identification in Item 7

  12. • insert {Item 18} - {STS/reason for special
      handling}

  13. • insert {Item 18} - {PER/Aircraft performance
      data}

  14. • insert {Item 18} - {RMK/any other remarks}
  15. • Supplementary Information is correct
  16. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }

  17. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

18. • forall point. NOT ( {point} is a {FIR
    boundary} prescribed {on the basis of regional
    air navigation agreements} ) OR insert {Item 18}
    - {EET/ {point} }
19. • forall point. NOT ( {point} is a {significant
    point} prescribed {by the approapriate ATS
    authority} ) OR insert {Item 18} - {EET/ {point}

}

20. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.8:
 Stimuli Response
   1. NOT Aircraft Identification is correct
   2. • FlightRules and Type of Flight is correct

   3. • Number and Type of Aircraft and Wake
      Turbulence Category is correct

   4. • Equipment is correct
   5. • Departure Aerodrome and time are correct
   6. • Route is correct
   7. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   8. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}

   9. • insert {Item 18} - {REG/registration markings
      of the aircraft}
  10. • insert {Item 18} - {SEL/SELCAL Code}

  11. • The name of the operator is obvious from the
      aircraft identification in Item 7

  12. • insert {Item 18} - {STS/reason for special
      handling}

  13. • insert {Item 18} - {PER/Aircraft performance
      data}

  14. • insert {Item 18} - {RMK/any other remarks}
  15. • Supplementary Information is correct
  16. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }

  17. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

18. • forall point. NOT ( {point} is a {FIR
    boundary} prescribed {on the basis of regional
    air navigation agreements} ) OR insert {Item 18}
    - {EET/ {point} }
19. • forall point. NOT ( {point} is a {significant
    point} prescribed {by the approapriate ATS
    authority} ) OR insert {Item 18} - {EET/ {point}

}

20. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.9:
 ROIDs: I18-9
 Stimuli Response
   1. Any other plain lanugage remarks are necessary

   2. NOT (insert {Item 18} - {RMK/any other remarks}
      )

   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct

   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}
  11. • insert {Item 18} - {REG/registration markings
      of the aircraft}
  12. • insert {Item 18} - {SEL/SELCAL Code}
  13. • The name of the operator is obvious from the
      aircraft identification in Item 7
  14. • insert {Item 18} - {STS/reason for special
      handling}
  15. • insert {Item 18} - {PER/Aircraft performance
      data}
  16. • Supplementary Information is correct
  17. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }
  18. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

19. • forall point. NOT ( {point} is a {FIR
    boundary} prescribed {on the basis of regional
    air navigation agreements} ) OR insert {Item 18}
    - {EET/ {point} }
20. • forall point. NOT ( {point} is a {significant
    point} prescribed {by the approapriate ATS
    authority} ) OR insert {Item 18} - {EET/ {point}

}

21. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.10:
 ROIDs: I18-8
 Stimuli Response
   1. {aerodrome} is an en-route alternate aerodrome
   2. NOT (insert {Item 18} - {RALT/ {aerodrome} } )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}
  11. • insert {Item 18} - {REG/registration markings
      of the aircraft}
  12. • insert {Item 18} - {SEL/SELCAL Code}
  13. • The name of the operator is obvious from the
      aircraft identification in Item 7
  14. • insert {Item 18} - {STS/reason for special
      handling}
  15. • insert {Item 18} - {PER/Aircraft performance
      data}
  16. • insert {Item 18} - {RMK/any other remarks}
  17. • Supplementary Information is correct
  18. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

19. • forall point. NOT ( {point} is a {FIR
    boundary} prescribed {on the basis of regional
    air navigation agreements} ) OR insert {Item 18}
    - {EET/ {point} }
20. • forall point. NOT ( {point} is a {significant
    point} prescribed {by the approapriate ATS
    authority} ) OR insert {Item 18} - {EET/ {point}

}

21. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.11:
 ROIDs: I18-7
 Stimuli Response
   1. Aircraft performance data is prescribed by the
      appropriate ATS authority
   2. NOT (insert {Item 18} - {PER/Aircraft
      performance data} )
   3. • Aircraft Identification is correct

   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct

   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}

  11. • insert {Item 18} - {REG/registration markings
      of the aircraft}

  12. • insert {Item 18} - {SEL/SELCAL Code}
  13. • The name of the operator is obvious from the
      aircraft identification in Item 7
  14. • insert {Item 18} - {STS/reason for special
      handling}
  15. • insert {Item 18} - {RMK/any other remarks}
  16. • Supplementary Information is correct
  17. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }
  18. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

19. • forall point. NOT ( {point} is a {FIR
    boundary} prescribed {on the basis of regional
    air navigation agreements} ) OR insert {Item 18}
    - {EET/ {point} }
20. • forall point. NOT ( {point} is a {significant
    point} prescribed {by the approapriate ATS
    authority} ) OR insert {Item 18} - {EET/ {point}

}

21. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.12:
 ROIDs: I18-6
 Stimuli Response
   1. There is a reason for special handling

   2. NOT (insert {Item 18} - {STS/reason for special
      handling} )

   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct

   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}
  11. • insert {Item 18} - {REG/registration markings
      of the aircraft}
  12. • insert {Item 18} - {SEL/SELCAL Code}
  13. • The name of the operator is obvious from the
      aircraft identification in Item 7
  14. • insert {Item 18} - {PER/Aircraft performance
      data}
  15. • insert {Item 18} - {RMK/any other remarks}
  16. • Supplementary Information is correct

  17. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }
  18. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

19. • forall point. NOT ( {point} is a {FIR
    boundary} prescribed {on the basis of regional
    air navigation agreements} ) OR insert {Item 18}
    - {EET/ {point} }
20. • forall point. NOT ( {point} is a {significant
    point} prescribed {by the approapriate ATS
    authority} ) OR insert {Item 18} - {EET/ {point}

}

21. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.13:
 ROIDs: I18-5
 Stimuli Response
   1. NOT The name of the operator is obvious from the
      aircraft identification in Item 7
   2. NOT (insert {Item 18} - {OPR/operator name} )

   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct

   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}
  11. • insert {Item 18} - {REG/registration markings
      of the aircraft}
  12. • insert {Item 18} - {SEL/SELCAL Code}
  13. • insert {Item 18} - {STS/reason for special
      handling}
  14. • insert {Item 18} - {PER/Aircraft performance
      data}
  15. • insert {Item 18} - {RMK/any other remarks}
  16. • Supplementary Information is correct

  17. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }
  18. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

19. • forall point. NOT ( {point} is a {FIR
    boundary} prescribed {on the basis of regional
    air navigation agreements} ) OR insert {Item 18}
    - {EET/ {point} }
20. • forall point. NOT ( {point} is a {significant
    point} prescribed {by the approapriate ATS
    authority} ) OR insert {Item 18} - {EET/ {point}

}

21. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.14:
 ROIDs: I18-4
 Stimuli Response
   1. A SELCAL Code is prescribed by the appropriate
      ATS authority
   2. NOT (insert {Item 18} - {SEL/SELCAL Code} )

   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct

   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}
  11. • insert {Item 18} - {REG/registration markings
      of the aircraft}
  12. • The name of the operator is obvious from the
      aircraft identification in Item 7
  13. • insert {Item 18} - {STS/reason for special
      handling}
  14. • insert {Item 18} - {PER/Aircraft performance
      data}
  15. • insert {Item 18} - {RMK/any other remarks}
  16. • Supplementary Information is correct
  17. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }
  18. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

19. • forall point. NOT ( {point} is a {FIR
    boundary} prescribed {on the basis of regional
    air navigation agreements} ) OR insert {Item 18}
    - {EET/ {point} }
20. • forall point. NOT ( {point} is a {significant
    point} prescribed {by the approapriate ATS
    authority} ) OR insert {Item 18} - {EET/ {point}

}

21. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.15:
 ROIDs: I18-3
 Stimuli Response
   1. The registration markings of the aircraft are
      different from the aircraft identification in
      Item 7
   2. NOT (insert {Item 18} - {REG/registration
      markings of the aircraft} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct

   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct

   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}
  11. • insert {Item 18} - {SEL/SELCAL Code}

  12. • The name of the operator is obvious from the
      aircraft identification in Item 7

  13. • insert {Item 18} - {STS/reason for special
      handling}

  14. • insert {Item 18} - {PER/Aircraft performance
      data}
  15. • insert {Item 18} - {RMK/any other remarks}

  16. • Supplementary Information is correct
  17. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }

  18. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

19. • forall point. NOT ( {point} is a {FIR
    boundary} prescribed {on the basis of regional
    air navigation agreements} ) OR insert {Item 18}
    - {EET/ {point} }
20. • forall point. NOT ( {point} is a {significant
    point} prescribed {by the approapriate ATS
    authority} ) OR insert {Item 18} - {EET/ {point}

}

21. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.16:
 ROIDs: I18-2
 Stimuli Response
   1. The route is revised

   2. NOT (insert {Item 18} - {RIF/route details to
      the revised destination aerodrome followed by
      the ICAO four letter location indicator of the
      aerodrome} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct

   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct

   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • insert {Item 18} - {REG/registration markings
      of the aircraft}
  11. • insert {Item 18} - {SEL/SELCAL Code}
  12. • The name of the operator is obvious from the
      aircraft identification in Item 7
  13. • insert {Item 18} - {STS/reason for special
      handling}
  14. • insert {Item 18} - {PER/Aircraft performance
      data}
  15. • insert {Item 18} - {RMK/any other remarks}
  16. • Supplementary Information is correct

  17. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }
  18. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

19. • forall point. NOT ( {point} is a {FIR
    boundary} prescribed {on the basis of regional
    air navigation agreements} ) OR insert {Item 18}
    - {EET/ {point} }
20. • forall point. NOT ( {point} is a {significant
    point} prescribed {by the approapriate ATS
    authority} ) OR insert {Item 18} - {EET/ {point}

}

21. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.17:
 ROIDs: I18-1
 Stimuli Response
   1. {point’} is a {FIR boundary} prescribed {by the
      approapriate ATS authority}
   2. NOT (insert {Item 18} - {EET/ {point’} } )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}
  11. • insert {Item 18} - {REG/registration markings
      of the aircraft}
  12. • insert {Item 18} - {SEL/SELCAL Code}
  13. • The name of the operator is obvious from the
      aircraft identification in Item 7
  14. • insert {Item 18} - {STS/reason for special
      handling}
  15. • insert {Item 18} - {PER/Aircraft performance
      data}
  16. • insert {Item 18} - {RMK/any other remarks}
  17. • Supplementary Information is correct
  18. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }
  19. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {on the basis of regional
      air navigation agreements} ) OR insert {Item 18}
      - {EET/ {point} }
  20. • forall point. NOT ( {point} is a {significant
      point} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

21. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.18:
 ROIDs: I18-1
 Stimuli Response
   1. {point’} is a {FIR boundary} prescribed {on the
      basis of regional air navigation agreements}
   2. NOT (insert {Item 18} - {EET/ {point’} } )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}
  11. • insert {Item 18} - {REG/registration markings
      of the aircraft}
  12. • insert {Item 18} - {SEL/SELCAL Code}
  13. • The name of the operator is obvious from the
      aircraft identification in Item 7
  14. • insert {Item 18} - {STS/reason for special
      handling}
  15. • insert {Item 18} - {PER/Aircraft performance
      data}
  16. • insert {Item 18} - {RMK/any other remarks}
  17. • Supplementary Information is correct
  18. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }
  19. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

20. • forall point. NOT ( {point} is a {significant
    point} prescribed {by the approapriate ATS
    authority} ) OR insert {Item 18} - {EET/ {point}

}

21. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.19:
 ROIDs: I18-1
 Stimuli Response
   1. {point’} is a {significant point} prescribed {by
      the approapriate ATS authority}
   2. NOT (insert {Item 18} - {EET/ {point’} } )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}
  11. • insert {Item 18} - {REG/registration markings
      of the aircraft}
  12. • insert {Item 18} - {SEL/SELCAL Code}
  13. • The name of the operator is obvious from the
      aircraft identification in Item 7
  14. • insert {Item 18} - {STS/reason for special
      handling}
  15. • insert {Item 18} - {PER/Aircraft performance
      data}
  16. • insert {Item 18} - {RMK/any other remarks}
  17. • Supplementary Information is correct
  18. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }
  19. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

20. • forall point. NOT ( {point} is a {FIR
    boundary} prescribed {on the basis of regional
    air navigation agreements} ) OR insert {Item 18}
    - {EET/ {point} }
21. • forall point. NOT ( {point} is a {significant
    point} prescribed {on the basis of regional air
    navigation agreements} ) OR insert {Item 18} -

{EET/ {point} }

1. report
   error

--Test Frame 1.20:
 ROIDs: I18-1
 Stimuli Response
   1. {point’} is a {significant point} prescribed {on
      the basis of regional air navigation agreements}
   2. NOT (insert {Item 18} - {EET/ {point’} } )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • insert {Item 18} - {RIF/route details to the
      revised destination aerodrome followed by the
      ICAO four letter location indicator of the
      aerodrome}
  11. • insert {Item 18} - {REG/registration markings
      of the aircraft}
  12. • insert {Item 18} - {SEL/SELCAL Code}
  13. • The name of the operator is obvious from the
      aircraft identification in Item 7
  14. • insert {Item 18} - {STS/reason for special
      handling}
  15. • insert {Item 18} - {PER/Aircraft performance
      data}
  16. • insert {Item 18} - {RMK/any other remarks}
  17. • Supplementary Information is correct
  18. • forall aerodrome. NOT ( {aerodrome} is an
      en-route alternate aerodrome) OR insert {Item
      18} - {RALT/ {aerodrome} }
  19. • forall point. NOT ( {point} is a {FIR
      boundary} prescribed {by the approapriate ATS
      authority} ) OR insert {Item 18} - {EET/ {point}

}

20. • forall point. NOT ( {point} is a {FIR
    boundary} prescribed {on the basis of regional
    air navigation agreements} ) OR insert {Item 18}
    - {EET/ {point} }
21. • forall point. NOT ( {point} is a {significant
    point} prescribed {by the approapriate ATS
    authority} ) OR insert {Item 18} - {EET/ {point}

}

1. report
   error

E.3.9 Supplementary Information

--Test Frame 1.1:
 Stimuli Response
   1. NOT Supplementary Information [Part 2] is
      correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Route is correct
   8. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   9. • Other Information is correct
  10. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  11. • The total number of persons is known
  12. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  13. • cross out {Item 19 R} - {U}
  14. • cross out {Item 19 R} - {V}
  15. • Emergency location beacon is available
  16. • Polar equipment is carried
  17. • Desert equipment is carried
  18. • Maritime equipment is carried
  19. • Jungle equipment is carried
  20. • cross out {Item 19 J} - {V}
  21. • cross out {Item 19 J} - {U}
  22. • cross out {Item 19 J} - {F }
  23. • cross out {Item 19 J} - {L}

                                                          1. report
                                                             error

--Test Frame 1.2:
 Stimuli Response
   1. NOT Other Information is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Route is correct
   8. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   9. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  10. • The total number of persons is known
  11. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  12. • cross out {Item 19 R} - {U}
  13. • cross out {Item 19 R} - {V}
  14. • Emergency location beacon is available
  15. • Polar equipment is carried
  16. • Desert equipment is carried
  17. • Maritime equipment is carried
  18. • Jungle equipment is carried
  19. • cross out {Item 19 J} - {V}
  20. • cross out {Item 19 J} - {U}
  21. • cross out {Item 19 J} - {F }
  22. • cross out {Item 19 J} - {L}
  23. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.3:
 Stimuli Response
   1. NOT Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Route is correct
   8. • Other Information is correct
   9. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  10. • The total number of persons is known
  11. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  12. • cross out {Item 19 R} - {U}
  13. • cross out {Item 19 R} - {V}
  14. • Emergency location beacon is available
  15. • Polar equipment is carried
  16. • Desert equipment is carried
  17. • Maritime equipment is carried
  18. • Jungle equipment is carried
  19. • cross out {Item 19 J} - {V}
  20. • cross out {Item 19 J} - {U}
  21. • cross out {Item 19 J} - {F }
  22. • cross out {Item 19 J} - {L}
  23. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.4:
 Stimuli Response
   1. NOT Route is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   8. • Other Information is correct
   9. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  10. • The total number of persons is known
  11. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  12. • cross out {Item 19 R} - {U}
  13. • cross out {Item 19 R} - {V}
  14. • Emergency location beacon is available
  15. • Polar equipment is carried
  16. • Desert equipment is carried
  17. • Maritime equipment is carried
  18. • Jungle equipment is carried
  19. • cross out {Item 19 J} - {V}
  20. • cross out {Item 19 J} - {U}
  21. • cross out {Item 19 J} - {F }
  22. • cross out {Item 19 J} - {L}
  23. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.5:
 Stimuli Response
   1. NOT Departure Aerodrome and time are correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Route is correct
   7. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   8. • Other Information is correct
   9. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  10. • The total number of persons is known
  11. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  12. • cross out {Item 19 R} - {U}
  13. • cross out {Item 19 R} - {V}
  14. • Emergency location beacon is available
  15. • Polar equipment is carried
  16. • Desert equipment is carried
  17. • Maritime equipment is carried
  18. • Jungle equipment is carried
  19. • cross out {Item 19 J} - {V}
  20. • cross out {Item 19 J} - {U}
  21. • cross out {Item 19 J} - {F }
  22. • cross out {Item 19 J} - {L}
  23. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.6:
 Stimuli Response
   1. NOT Equipment is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Departure Aerodrome and time are correct
   6. • Route is correct
   7. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   8. • Other Information is correct
   9. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  10. • The total number of persons is known
  11. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  12. • cross out {Item 19 R} - {U}
  13. • cross out {Item 19 R} - {V}
  14. • Emergency location beacon is available
  15. • Polar equipment is carried
  16. • Desert equipment is carried
  17. • Maritime equipment is carried
  18. • Jungle equipment is carried
  19. • cross out {Item 19 J} - {V}
  20. • cross out {Item 19 J} - {U}
  21. • cross out {Item 19 J} - {F }
  22. • cross out {Item 19 J} - {L}
  23. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.7:
 Stimuli Response
   1. NOT Number and Type of Aircraft and Wake
      Turbulence Category is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Equipment is correct
   5. • Departure Aerodrome and time are correct
   6. • Route is correct
   7. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   8. • Other Information is correct
   9. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  10. • The total number of persons is known
  11. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  12. • cross out {Item 19 R} - {U}
  13. • cross out {Item 19 R} - {V}
  14. • Emergency location beacon is available
  15. • Polar equipment is carried
  16. • Desert equipment is carried
  17. • Maritime equipment is carried
  18. • Jungle equipment is carried
  19. • cross out {Item 19 J} - {V}
  20. • cross out {Item 19 J} - {U}
  21. • cross out {Item 19 J} - {F }
  22. • cross out {Item 19 J} - {L}
  23. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.8:
 Stimuli Response
   1. NOT FlightRules and Type of Flight is correct
   2. • Aircraft Identification is correct
   3. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   4. • Equipment is correct
   5. • Departure Aerodrome and time are correct
   6. • Route is correct
   7. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   8. • Other Information is correct
   9. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  10. • The total number of persons is known
  11. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  12. • cross out {Item 19 R} - {U}
  13. • cross out {Item 19 R} - {V}
  14. • Emergency location beacon is available
  15. • Polar equipment is carried
  16. • Desert equipment is carried
  17. • Maritime equipment is carried
  18. • Jungle equipment is carried
  19. • cross out {Item 19 J} - {V}
  20. • cross out {Item 19 J} - {U}
  21. • cross out {Item 19 J} - {F }
  22. • cross out {Item 19 J} - {L}
  23. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.9:
 Stimuli Response
   1. NOT Aircraft Identification is correct
   2. • FlightRules and Type of Flight is correct
   3. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   4. • Equipment is correct
   5. • Departure Aerodrome and time are correct
   6. • Route is correct
   7. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   8. • Other Information is correct
   9. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  10. • The total number of persons is known
  11. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  12. • cross out {Item 19 R} - {U}
  13. • cross out {Item 19 R} - {V}
  14. • Emergency location beacon is available
  15. • Polar equipment is carried
  16. • Desert equipment is carried
  17. • Maritime equipment is carried
  18. • Jungle equipment is carried
  19. • cross out {Item 19 J} - {V}
  20. • cross out {Item 19 J} - {U}
  21. • cross out {Item 19 J} - {F }
  22. • cross out {Item 19 J} - {L}
  23. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.10:
 ROIDs: I19P
 Stimuli Response
   1. Number of persons is required by the ATS
      authority
   2. The total number of persons is known
   3. NOT (insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • Equipment is correct
   8. • Departure Aerodrome and time are correct
   9. • Route is correct
  10. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  11. • Other Information is correct
  12. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  13. • cross out {Item 19 R} - {U}
  14. • cross out {Item 19 R} - {V}
  15. • Emergency location beacon is available
  16. • Polar equipment is carried
  17. • Desert equipment is carried
  18. • Maritime equipment is carried
  19. • Jungle equipment is carried
  20. • cross out {Item 19 J} - {V}
  21. • cross out {Item 19 J} - {U}
  22. • cross out {Item 19 J} - {F }
  23. • cross out {Item 19 J} - {L}
  24. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.11:
 ROIDs: I19ES3
 Stimuli Response
   1. NOT (cross out {Item 19 R} - {V} )
   2. Life jackets are carried
   3. cross out {Item 19 J} - {V}
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • Equipment is correct
   8. • Departure Aerodrome and time are correct
   9. • Route is correct
  10. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  11. • Other Information is correct
  12. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  13. • The total number of persons is known
  14. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  15. • cross out {Item 19 R} - {U}
  16. • VHF on frequency 121.5 MHz is available
  17. • Emergency location beacon is available
  18. • Polar equipment is carried
  19. • Desert equipment is carried
  20. • Maritime equipment is carried
  21. • Jungle equipment is carried
  22. • cross out {Item 19 J} - {U}
  23. • cross out {Item 19 J} - {F }
  24. • cross out {Item 19 J} - {L}
  25. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.12:
 ROIDs: I19ES2
 Stimuli Response
   1. NOT Jungle equipment is carried
   2. NOT (cross out {Item 19 S} - {J} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  12. • The total number of persons is known
  13. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  14. • cross out {Item 19 R} - {U}
  15. • cross out {Item 19 R} - {V}
  16. • Emergency location beacon is available
  17. • Polar equipment is carried
  18. • Desert equipment is carried
  19. • Maritime equipment is carried
  20. • cross out {Item 19 J} - {V}
  21. • cross out {Item 19 J} - {U}
  22. • cross out {Item 19 J} - {F }
  23. • cross out {Item 19 J} - {L}
  24. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.13:
 ROIDs: I19ES2
 Stimuli Response
   1. NOT Maritime equipment is carried
   2. NOT (cross out {Item 19 S} - {M} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  12. • The total number of persons is known
  13. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  14. • cross out {Item 19 R} - {U}
  15. • cross out {Item 19 R} - {V}
  16. • Emergency location beacon is available
  17. • Polar equipment is carried
  18. • Desert equipment is carried
  19. • Jungle equipment is carried
  20. • cross out {Item 19 J} - {V}
  21. • cross out {Item 19 J} - {U}
  22. • cross out {Item 19 J} - {F }
  23. • cross out {Item 19 J} - {L}
  24. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.14:
 ROIDs: I19ES2
 Stimuli Response
   1. NOT Desert equipment is carried
   2. NOT (cross out {Item 19 S} - {D} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  12. • The total number of persons is known
  13. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  14. • cross out {Item 19 R} - {U}
  15. • cross out {Item 19 R} - {V}
  16. • Emergency location beacon is available
  17. • Polar equipment is carried
  18. • Maritime equipment is carried
  19. • Jungle equipment is carried
  20. • cross out {Item 19 J} - {V}
  21. • cross out {Item 19 J} - {U}
  22. • cross out {Item 19 J} - {F }
  23. • cross out {Item 19 J} - {L}
  24. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.15:
 ROIDs: I19ES2
 Stimuli Response
   1. NOT Polar equipment is carried
   2. NOT (cross out {Item 19 S} - {P} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  12. • The total number of persons is known
  13. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  14. • cross out {Item 19 R} - {U}
  15. • cross out {Item 19 R} - {V}
  16. • Emergency location beacon is available
  17. • Desert equipment is carried
  18. • Maritime equipment is carried
  19. • Jungle equipment is carried
  20. • cross out {Item 19 J} - {V}
  21. • cross out {Item 19 J} - {U}
  22. • cross out {Item 19 J} - {F }
  23. • cross out {Item 19 J} - {L}
  24. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.16:
 ROIDs: I19ES1
 Stimuli Response
   1. NOT Emergency location beacon is available
   2. NOT (cross out {Item 19 R} - {E} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  12. • The total number of persons is known
  13. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  14. • cross out {Item 19 R} - {U}
  15. • cross out {Item 19 R} - {V}
  16. • Polar equipment is carried
  17. • Desert equipment is carried
  18. • Maritime equipment is carried
  19. • Jungle equipment is carried
  20. • cross out {Item 19 J} - {V}
  21. • cross out {Item 19 J} - {U}
  22. • cross out {Item 19 J} - {F }
  23. • cross out {Item 19 J} - {L}
  24. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.17:
 ROIDs: I19ES3
 Stimuli Response
   1. NOT (cross out {Item 19 J} - {L} )
   2. NOT Life jackets are equipped with lights
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  12. • The total number of persons is known
  13. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  14. • cross out {Item 19 R} - {U}
  15. • cross out {Item 19 R} - {V}
  16. • Emergency location beacon is available
  17. • Polar equipment is carried
  18. • Desert equipment is carried
  19. • Maritime equipment is carried
  20. • Jungle equipment is carried
  21. • Life jackets are carried
  22. • cross out {Item 19 J} - {V}
  23. • cross out {Item 19 J} - {U}
  24. • cross out {Item 19 J} - {F }
  25. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.18:
 ROIDs: I19ES3
 Stimuli Response
   1. NOT (cross out {Item 19 J} - {F } )
   2. NOT Life jackets are equipped with fluorescein
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  12. • The total number of persons is known
  13. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  14. • cross out {Item 19 R} - {U}
  15. • cross out {Item 19 R} - {V}
  16. • Emergency location beacon is available
  17. • Polar equipment is carried
  18. • Desert equipment is carried
  19. • Maritime equipment is carried
  20. • Jungle equipment is carried
  21. • cross out {Item 19 J} - {V}
  22. • cross out {Item 19 J} - {U}
  23. • cross out {Item 19 J} - {L}
  24. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.19:
 ROIDs: I19ES3
 Stimuli Response
   1. cross out {Item 19 R} - {U}
   2. NOT (cross out {Item 19 J} - {U} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  12. • The total number of persons is known
  13. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  14. • cross out {Item 19 R} - {V}
  15. • Emergency location beacon is available
  16. • Polar equipment is carried
  17. • Desert equipment is carried
  18. • Maritime equipment is carried
  19. • Jungle equipment is carried
  20. • cross out {Item 19 J} - {V}
  21. • cross out {Item 19 J} - {F }
  22. • cross out {Item 19 J} - {L}
  23. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.20:
 ROIDs: I19ES3
 Stimuli Response
   1. cross out {Item 19 R} - {V}
   2. NOT (cross out {Item 19 J} - {V} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  12. • The total number of persons is known
  13. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  14. • cross out {Item 19 R} - {U}
  15. • Emergency location beacon is available
  16. • Polar equipment is carried
  17. • Desert equipment is carried
  18. • Maritime equipment is carried
  19. • Jungle equipment is carried
  20. • cross out {Item 19 J} - {U}
  21. • cross out {Item 19 J} - {F }
  22. • cross out {Item 19 J} - {L}
  23. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.21:
 ROIDs: I19ES1
 Stimuli Response
   1. NOT UHF on frequency 243.0 MHz is available
   2. NOT (cross out {Item 19 R} - {U} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  12. • The total number of persons is known
  13. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  14. • cross out {Item 19 R} - {V}
  15. • Emergency location beacon is available
  16. • Polar equipment is carried
  17. • Desert equipment is carried
  18. • Maritime equipment is carried
  19. • Jungle equipment is carried
  20. • cross out {Item 19 J} - {V}
  21. • NOT (cross out {Item 19 J} - {U} )
  22. • cross out {Item 19 J} - {F }
  23. • cross out {Item 19 J} - {L}
  24. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.22:
 ROIDs: I19P
 Stimuli Response
   1. Number of persons is required by the ATS
      authority
   2. NOT The total number of persons is known
   3. NOT (insert {Item 19 P} - {TBN} )
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • Equipment is correct
   8. • Departure Aerodrome and time are correct
   9. • Route is correct
  10. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  11. • Other Information is correct
  12. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  13. • cross out {Item 19 R} - {U}
  14. • cross out {Item 19 R} - {V}
  15. • Emergency location beacon is available
  16. • Polar equipment is carried
  17. • Desert equipment is carried
  18. • Maritime equipment is carried
  19. • Jungle equipment is carried
  20. • cross out {Item 19 J} - {V}
  21. • cross out {Item 19 J} - {U}
  22. • cross out {Item 19 J} - {F }
  23. • cross out {Item 19 J} - {L}
  24. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.23:
 ROIDs: I19E
 Stimuli Response
   1. NOT (insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes} )
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Route is correct
   8. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   9. • Other Information is correct
  10. • The total number of persons is known
  11. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  12. • cross out {Item 19 R} - {U}
  13. • cross out {Item 19 R} - {V}
  14. • Emergency location beacon is available
  15. • Polar equipment is carried
  16. • Desert equipment is carried
  17. • Maritime equipment is carried
  18. • Jungle equipment is carried
  19. • cross out {Item 19 J} - {V}
  20. • cross out {Item 19 J} - {U}
  21. • cross out {Item 19 J} - {F }
  22. • cross out {Item 19 J} - {L}
  23. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.24:
 ROIDs: I19ES1
 Stimuli Response
   1. NOT VHF on frequency 121.5 MHz is available
   2. NOT (cross out {Item 19 R} - {V} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  12. • The total number of persons is known
  13. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  14. • cross out {Item 19 R} - {U}
  15. • Emergency location beacon is available
  16. • Polar equipment is carried
  17. • Desert equipment is carried
  18. • Maritime equipment is carried
  19. • Jungle equipment is carried
  20. • NOT (cross out {Item 19 J} - {V} )
  21. • cross out {Item 19 J} - {U}
  22. • cross out {Item 19 J} - {F }
  23. • cross out {Item 19 J} - {L}
  24. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.25:
 ROIDs: I19ES3
 Stimuli Response
   1. NOT (cross out {Item 19 R} - {U} )
   2. Life jackets are carried
   3. cross out {Item 19 J} - {U}
   4. • Aircraft Identification is correct
   5. • FlightRules and Type of Flight is correct
   6. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   7. • Equipment is correct
   8. • Departure Aerodrome and time are correct
   9. • Route is correct
  10. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  11. • Other Information is correct
  12. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  13. • The total number of persons is known
  14. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  15. • UHF on frequency 243.0 MHz is available
  16. • cross out {Item 19 R} - {V}
  17. • Emergency location beacon is available
  18. • Polar equipment is carried
  19. • Desert equipment is carried
  20. • Maritime equipment is carried
  21. • Jungle equipment is carried
  22. • cross out {Item 19 J} - {V}
  23. • cross out {Item 19 J} - {F }
  24. • cross out {Item 19 J} - {L}
  25. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.26:
 ROIDs: I19ES3
 Stimuli Response
   1. NOT Life jackets are carried
   2. NOT (cross out {Item 19 J} - {L} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • insert {Item 19 E} - {the four digit fuel
      endurance in hours and minutes}
  12. • The total number of persons is known
  13. • insert {Item 19 P} - {the total number of
      persons [passengers and crew] on board}
  14. • UHF on frequency 243.0 MHz is available
  15. • VHF on frequency 121.5 MHz is available
  16. • Emergency location beacon is available
  17. • Polar equipment is carried
  18. • Desert equipment is carried
  19. • Maritime equipment is carried
  20. • Jungle equipment is carried
  21. • cross out {Item 19 J} - {V}
  22. • cross out {Item 19 J} - {U}
  23. • cross out {Item 19 J} - {F }
  24. • Life jackets are equipped with lights
  25. • Supplementary Information [Part 2] is correct

                                                          1. report
                                                             error

--Test Frame 1.1:
 Stimuli Response
   1. NOT Supplementary Information [Part 1] is
      correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Route is correct
   8. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   9. • Other Information is correct
  10. • Dinghies are carried
  11. • cross out {Item 19 D} - {C}
  12. • insert {Item 19 D} - {number of dinghies
      carried}
  13. • insert {Item 19 D} - {total capacity in
      persons of all dinghies carried}
  14. • insert {Item 19 D} - {colour of dinghies}
  15. • insert {Item 19 A} - {colour of aircraft and
      significant markings}
  16. • There are remarks
  17. • indicate {Item 19 N} - {any other survival
      equipment carried and any other remarks
      regarding survival equipment}
  18. • insert {Item 19 C} - {name of pilot in
      command}

                                                          1. report
                                                             error

--Test Frame 1.2:
 Stimuli Response
   1. NOT Other Information is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Route is correct
   8. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   9. • Supplementary Information [Part 1] is correct
  10. • Dinghies are carried
  11. • cross out {Item 19 D} - {C}
  12. • insert {Item 19 D} - {number of dinghies
      carried}
  13. • insert {Item 19 D} - {total capacity in
      persons of all dinghies carried}
  14. • insert {Item 19 D} - {colour of dinghies}
  15. • insert {Item 19 A} - {colour of aircraft and
      significant markings}
  16. • There are remarks
  17. • indicate {Item 19 N} - {any other survival
      equipment carried and any other remarks
      regarding survival equipment}
  18. • insert {Item 19 C} - {name of pilot in
      command}

                                                          1. report
                                                             error

--Test Frame 1.3:
 Stimuli Response
   1. NOT Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Route is correct
   8. • Other Information is correct
   9. • Supplementary Information [Part 1] is correct
  10. • Dinghies are carried
  11. • cross out {Item 19 D} - {C}
  12. • insert {Item 19 D} - {number of dinghies
      carried}
  13. • insert {Item 19 D} - {total capacity in
      persons of all dinghies carried}
  14. • insert {Item 19 D} - {colour of dinghies}
  15. • insert {Item 19 A} - {colour of aircraft and
      significant markings}
  16. • There are remarks
  17. • indicate {Item 19 N} - {any other survival
      equipment carried and any other remarks
      regarding survival equipment}
  18. • insert {Item 19 C} - {name of pilot in
      command}

                                                          1. report
                                                             error

--Test Frame 1.4:
 Stimuli Response
   1. NOT Route is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   8. • Other Information is correct
   9. • Supplementary Information [Part 1] is correct
  10. • Dinghies are carried
  11. • cross out {Item 19 D} - {C}
  12. • insert {Item 19 D} - {number of dinghies
      carried}
  13. • insert {Item 19 D} - {total capacity in
      persons of all dinghies carried}
  14. • insert {Item 19 D} - {colour of dinghies}
  15. • insert {Item 19 A} - {colour of aircraft and
      significant markings}
  16. • There are remarks
  17. • indicate {Item 19 N} - {any other survival
      equipment carried and any other remarks
      regarding survival equipment}
  18. • insert {Item 19 C} - {name of pilot in
      command}

                                                          1. report
                                                             error

--Test Frame 1.5:
 Stimuli Response
   1. NOT Departure Aerodrome and time are correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Route is correct
   7. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   8. • Other Information is correct
   9. • Supplementary Information [Part 1] is correct
  10. • Dinghies are carried
  11. • cross out {Item 19 D} - {C}
  12. • insert {Item 19 D} - {number of dinghies
      carried}
  13. • insert {Item 19 D} - {total capacity in
      persons of all dinghies carried}
  14. • insert {Item 19 D} - {colour of dinghies}
  15. • insert {Item 19 A} - {colour of aircraft and
      significant markings}
  16. • There are remarks
  17. • indicate {Item 19 N} - {any other survival
      equipment carried and any other remarks
      regarding survival equipment}
  18. • insert {Item 19 C} - {name of pilot in
      command}

                                                          1. report
                                                             error

--Test Frame 1.6:
 Stimuli Response
   1. NOT Equipment is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Departure Aerodrome and time are correct
   6. • Route is correct
   7. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   8. • Other Information is correct
   9. • Supplementary Information [Part 1] is correct
  10. • Dinghies are carried
  11. • cross out {Item 19 D} - {C}
  12. • insert {Item 19 D} - {number of dinghies
      carried}
  13. • insert {Item 19 D} - {total capacity in
      persons of all dinghies carried}
  14. • insert {Item 19 D} - {colour of dinghies}
  15. • insert {Item 19 A} - {colour of aircraft and
      significant markings}
  16. • There are remarks
  17. • indicate {Item 19 N} - {any other survival
      equipment carried and any other remarks
      regarding survival equipment}
  18. • insert {Item 19 C} - {name of pilot in
      command}

                                                          1. report
                                                             error

--Test Frame 1.7:
 Stimuli Response
   1. NOT Number and Type of Aircraft and Wake
      Turbulence Category is correct
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Equipment is correct
   5. • Departure Aerodrome and time are correct
   6. • Route is correct
   7. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   8. • Other Information is correct
   9. • Supplementary Information [Part 1] is correct
  10. • Dinghies are carried
  11. • cross out {Item 19 D} - {C}
  12. • insert {Item 19 D} - {number of dinghies
      carried}
  13. • insert {Item 19 D} - {total capacity in
      persons of all dinghies carried}
  14. • insert {Item 19 D} - {colour of dinghies}
  15. • insert {Item 19 A} - {colour of aircraft and
      significant markings}
  16. • There are remarks
  17. • indicate {Item 19 N} - {any other survival
      equipment carried and any other remarks
      regarding survival equipment}
  18. • insert {Item 19 C} - {name of pilot in
      command}

                                                          1. report
                                                             error

--Test Frame 1.8:
 Stimuli Response
   1. NOT FlightRules and Type of Flight is correct
   2. • Aircraft Identification is correct
   3. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   4. • Equipment is correct
   5. • Departure Aerodrome and time are correct
   6. • Route is correct
   7. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   8. • Other Information is correct
   9. • Supplementary Information [Part 1] is correct
  10. • Dinghies are carried
  11. • cross out {Item 19 D} - {C}
  12. • insert {Item 19 D} - {number of dinghies
      carried}
  13. • insert {Item 19 D} - {total capacity in
      persons of all dinghies carried}
  14. • insert {Item 19 D} - {colour of dinghies}
  15. • insert {Item 19 A} - {colour of aircraft and
      significant markings}
  16. • There are remarks
  17. • indicate {Item 19 N} - {any other survival
      equipment carried and any other remarks
      regarding survival equipment}
  18. • insert {Item 19 C} - {name of pilot in
      command}

                                                          1. report
                                                             error

--Test Frame 1.9:
 Stimuli Response
   1. NOT Aircraft Identification is correct
   2. • FlightRules and Type of Flight is correct
   3. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   4. • Equipment is correct
   5. • Departure Aerodrome and time are correct
   6. • Route is correct
   7. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   8. • Other Information is correct
   9. • Supplementary Information [Part 1] is correct
  10. • Dinghies are carried
  11. • cross out {Item 19 D} - {C}
  12. • insert {Item 19 D} - {number of dinghies
      carried}
  13. • insert {Item 19 D} - {total capacity in
      persons of all dinghies carried}
  14. • insert {Item 19 D} - {colour of dinghies}
  15. • insert {Item 19 A} - {colour of aircraft and
      significant markings}
  16. • There are remarks
  17. • indicate {Item 19 N} - {any other survival
      equipment carried and any other remarks
      regarding survival equipment}
  18. • insert {Item 19 C} - {name of pilot in
      command}

                                                          1. report
                                                             error

--Test Frame 1.10:
 ROIDs: I19ES6
 Stimuli Response
   1. There are remarks
   2. NOT (indicate {Item 19 N} - {any other survival
      equipment carried and any other remarks
      regarding survival equipment} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • Supplementary Information [Part 1] is correct
  12. • Dinghies are carried
  13. • cross out {Item 19 D} - {C}
  14. • insert {Item 19 D} - {number of dinghies
      carried}
  15. • insert {Item 19 D} - {total capacity in
      persons of all dinghies carried}
  16. • insert {Item 19 D} - {colour of dinghies}
  17. • insert {Item 19 A} - {colour of aircraft and
      significant markings}
  18. • insert {Item 19 C} - {name of pilot in
      command}

                                                          1. report
                                                             error

--Test Frame 1.11:
 ROIDs: I19ES6
 Stimuli Response
   1. NOT There are remarks
   2. NOT (cross out {Item 19 N} - {N} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • Supplementary Information [Part 1] is correct
  12. • Dinghies are carried
  13. • cross out {Item 19 D} - {C}
  14. • insert {Item 19 D} - {number of dinghies
      carried}
  15. • insert {Item 19 D} - {total capacity in
      persons of all dinghies carried}
  16. • insert {Item 19 D} - {colour of dinghies}
  17. • insert {Item 19 A} - {colour of aircraft and
      significant markings}
  18. • insert {Item 19 C} - {name of pilot in
      command}

                                                          1. report
                                                             error

--Test Frame 1.12:
 ROIDs: I19ES4
 Stimuli Response
   1. NOT (cross out {Item 19 D} - {C} )
   2. NOT Dinghies are covered
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • Supplementary Information [Part 1] is correct
  12. • Dinghies are carried
  13. • insert {Item 19 D} - {number of dinghies
      carried}
  14. • insert {Item 19 D} - {total capacity in
      persons of all dinghies carried}
  15. • insert {Item 19 D} - {colour of dinghies}
  16. • insert {Item 19 A} - {colour of aircraft and
      significant markings}
  17. • There are remarks
  18. • indicate {Item 19 N} - {any other survival
      equipment carried and any other remarks
      regarding survival equipment}
  19. • insert {Item 19 C} - {name of pilot in
      command}

                                                          1. report
                                                             error

--Test Frame 1.13:
 ROIDs: I19ES4
 Stimuli Response
   1. NOT Dinghies are carried
   2. NOT (cross out {Item 19 D} - {D} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • Supplementary Information [Part 1] is correct
  12. • cross out {Item 19 D} - {C}
  13. • insert {Item 19 A} - {colour of aircraft and
      significant markings}
  14. • There are remarks
  15. • indicate {Item 19 N} - {any other survival
      equipment carried and any other remarks
      regarding survival equipment}
  16. • insert {Item 19 C} - {name of pilot in
      command}

                                                          1. report
                                                             error

--Test Frame 1.14:
 ROIDs: I19ES4
 Stimuli Response
   1. Dinghies are carried
   2. NOT (insert {Item 19 D} - {colour of dinghies} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • Supplementary Information [Part 1] is correct
  12. • cross out {Item 19 D} - {C}
  13. • insert {Item 19 D} - {number of dinghies
      carried}
  14. • insert {Item 19 D} - {total capacity in
      persons of all dinghies carried}
  15. • insert {Item 19 A} - {colour of aircraft and
      significant markings}
  16. • There are remarks
  17. • indicate {Item 19 N} - {any other survival
      equipment carried and any other remarks
      regarding survival equipment}
  18. • insert {Item 19 C} - {name of pilot in
      command}

                                                          1. report
                                                             error

--Test Frame 1.15:
 ROIDs: I19ES7
 Stimuli Response
   1. NOT (insert {Item 19 C} - {name of pilot in
      command} )
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Route is correct
   8. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   9. • Other Information is correct
  10. • Supplementary Information [Part 1] is correct
  11. • Dinghies are carried
  12. • cross out {Item 19 D} - {C}
  13. • insert {Item 19 D} - {number of dinghies
      carried}
  14. • insert {Item 19 D} - {total capacity in
      persons of all dinghies carried}
  15. • insert {Item 19 D} - {colour of dinghies}
  16. • insert {Item 19 A} - {colour of aircraft and
      significant markings}
  17. • There are remarks
  18. • indicate {Item 19 N} - {any other survival
      equipment carried and any other remarks
      regarding survival equipment}

                                                          1. report
                                                             error

--Test Frame 1.16:
 ROIDs: I19ES5
 Stimuli Response
   1. NOT (insert {Item 19 A} - {colour of aircraft
      and significant markings} )
   2. • Aircraft Identification is correct
   3. • FlightRules and Type of Flight is correct
   4. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   5. • Equipment is correct
   6. • Departure Aerodrome and time are correct
   7. • Route is correct
   8. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
   9. • Other Information is correct
  10. • Supplementary Information [Part 1] is correct
  11. • Dinghies are carried
  12. • cross out {Item 19 D} - {C}
  13. • insert {Item 19 D} - {number of dinghies
      carried}
  14. • insert {Item 19 D} - {total capacity in
      persons of all dinghies carried}
  15. • insert {Item 19 D} - {colour of dinghies}
  16. • There are remarks
  17. • indicate {Item 19 N} - {any other survival
      equipment carried and any other remarks
      regarding survival equipment}
  18. • insert {Item 19 C} - {name of pilot in
      command}

                                                          1. report
                                                             error

--Test Frame 1.17:
 ROIDs: I19ES4
 Stimuli Response
   1. Dinghies are carried
   2. NOT (insert {Item 19 D} - {total capacity in
      persons of all dinghies carried} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • Supplementary Information [Part 1] is correct
  12. • cross out {Item 19 D} - {C}
  13. • insert {Item 19 D} - {number of dinghies
      carried}
  14. • insert {Item 19 D} - {colour of dinghies}
  15. • insert {Item 19 A} - {colour of aircraft and
      significant markings}
  16. • There are remarks
  17. • indicate {Item 19 N} - {any other survival
      equipment carried and any other remarks
      regarding survival equipment}
  18. • insert {Item 19 C} - {name of pilot in
      command}

                                                          1. report
                                                             error

--Test Frame 1.18:
 ROIDs: I19ES4
 Stimuli Response
   1. Dinghies are carried
   2. NOT (insert {Item 19 D} - {number of dinghies
      carried} )
   3. • Aircraft Identification is correct
   4. • FlightRules and Type of Flight is correct
   5. • Number and Type of Aircraft and Wake
      Turbulence Category is correct
   6. • Equipment is correct
   7. • Departure Aerodrome and time are correct
   8. • Route is correct
   9. • Destination Aerodrome and Total Estimated
      Elapsed Time is correct
  10. • Other Information is correct
  11. • Supplementary Information [Part 1] is correct
  12. • cross out {Item 19 D} - {C}
  13. • insert {Item 19 D} - {total capacity in
      persons of all dinghies carried}
  14. • insert {Item 19 D} - {colour of dinghies}
  15. • insert {Item 19 A} - {colour of aircraft and
      significant markings}
  16. • There are remarks
  17. • indicate {Item 19 N} - {any other survival
      equipment carried and any other remarks
      regarding survival equipment}
  18. • insert {Item 19 C} - {name of pilot in
      command}

                                                          1. report
                                                             error